3GPP TS 38.214 V16.0.0 (2019-12)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

NR;

Physical layer procedures for data

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

3GPP, New Radio, Layer 1

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 6

1 Scope 7

2 References 7

3 Definitions, symbols and abbreviations 8

3.1 Definitions 8

3.2 Symbols 8

3.3 Abbreviations 8

4 Power control 9

4.1 Power allocation for downlink 9

5 Physical downlink shared channel related procedures 10

5.1 UE procedure for receiving the physical downlink shared channel 10

5.1.1 Transmission schemes 12

5.1.1.1 Transmission scheme 1 12

5.1.2 Resource allocation 12

5.1.2.1 Resource allocation in time domain 12

5.1.2.1.1 Determination of the resource allocation table to be used for PDSCH 15

5.1.2.2 Resource allocation in frequency domain 19

5.1.2.2.1 Downlink resource allocation type 0 19

5.1.2.2.2 Downlink resource allocation type 1 20

5.1.2.3 Physical resource block (PRB) bundling 21

5.1.3 Modulation order, target code rate, redundancy version and transport block size determination 22

5.1.3.1 Modulation order and target code rate determination 24

5.1.3.2 Transport block size determination 28

5.1.4 PDSCH resource mapping 31

5.1.4.1 PDSCH resource mapping with RB symbol level granularity 31

5.1.4.2 PDSCH resource mapping with RE level granularity 32

5.1.5 Antenna ports quasi co-location 34

5.1.6 UE procedure for receiving reference signals 36

5.1.6.1 CSI-RS reception procedure 36

5.1.6.1.1 CSI-RS for tracking 37

5.1.6.1.2 CSI-RS for L1-RSRP and L1-SINR computation 38

5.1.6.1.3 CSI-RS for mobility 38

5.1.6.2 DM-RS reception procedure 39

5.1.6.3 PT-RS reception procedure 41

5.1.6.4 SRS reception procedure for CLI 43

5.1.6.5 PRS reception procedure 43

5.1.7 Code block group based PDSCH transmission 46

5.1.7.1 UE procedure for grouping of code blocks to code block groups 46

5.1.7.2 UE procedure for receiving code block group based transmissions 46

5.2 UE procedure for reporting channel state information (CSI) 46

5.2.1 Channel state information framework 46

5.2.1.1 Reporting settings 47

5.2.1.2 Resource settings 47

5.2.1.3 (void) 48

5.2.1.4 Reporting configurations 48

5.2.1.4.1 Resource Setting configuration 51

5.2.1.4.2 Report Quantity Configurations 51

5.2.1.4.3 L1-RSRP Reporting 53

5.2.1.4.4 L1-SINR Reporting 53

5.2.1.5 Triggering/activation of CSI Reports and CSI-RS 54

5.2.1.5.1 Aperiodic CSI Reporting/Aperiodic CSI-RS when the triggering PDCCH and the CSI-RS have the same numerology 54

5.2.1.5.1a Aperiodic CSI Reporting/Aperiodic CSI-RS when the triggering PDCCH and the CSI-RS have different numerologies 55

5.2.1.5.2 Semi-persistent CSI/Semi-persistent CSI-RS 57

5.2.1.6 CSI processing criteria 58

5.2.2 Channel state information 59

5.2.2.1 Channel quality indicator (CQI) 59

5.2.2.1.1 (void) 61

5.2.2.2 Precoding matrix indicator (PMI) 61

5.2.2.2.1 Type I Single-Panel Codebook 61

5.2.2.2.2 Type I Multi-Panel Codebook 68

5.2.2.2.3 Type II Codebook 72

5.2.2.2.4 Type II Port Selection Codebook 79

5.2.2.2.5 Enhanced Type II Codebook 81

5.2.2.2.6 Enhanced Type II Port Selection Codebook 88

5.2.2.3 Reference signal (CSI-RS) 89

5.2.2.3.1 NZP CSI-RS 89

5.2.2.4 Channel State Information – Interference Measurement (CSI-IM) 91

5.2.2.5 CSI reference resource definition 91

5.2.3 CSI reporting using PUSCH 93

5.2.4 CSI reporting using PUCCH 96

5.2.5 Priority rules for CSI reports 97

5.3 UE PDSCH processing procedure time 97

5.3.1 Application delay of the minimum scheduling offset restriction 99

5.4 UE CSI computation time 99

5.5 UE PDSCH reception preparation time with cross carrier scheduling with different subcarrier spacings for PDCCH and PDSCH 101

6 Physical uplink shared channel related procedure 101

6.1 UE procedure for transmitting the physical uplink shared channel 101

6.1.1 Transmission schemes 103

6.1.1.1 Codebook based UL transmission 103

6.1.1.2 Non-Codebook based UL transmission 104

6.1.2 Resource allocation 105

6.1.2.1 Resource allocation in time domain 105

6.1.2.1.1 Determination of the resource allocation table to be used for PUSCH 109

6.1.2.2 Resource allocation in frequency domain 111

6.1.2.2.1 Uplink resource allocation type 0 112

6.1.2.2.2 Uplink resource allocation type 1 112

6.1.2.2.3 Uplink resource allocation type 2 113

6.1.2.3 Resource allocation for uplink transmission with configured grant 114

6.1.3 UE procedure for applying transform precoding on PUSCH 116

6.1.4 Modulation order, redundancy version and transport block size determination 117

6.1.4.1 Modulation order and target code rate determination 118

6.1.4.2 Transport block size determination 122

6.1.5 Code block group based PUSCH transmission 123

6.1.5.1 UE procedure for grouping of code blocks to code block groups 123

6.1.5.2 UE procedure for transmitting code block group based transmissions 124

6.2 UE reference signal (RS) procedure 124

6.2.1 UE sounding procedure 124

6.2.1.1 UE SRS frequency hopping procedure 128

6.2.1.2 UE sounding procedure for DL CSI acquisition 128

6.2.1.3 UE sounding procedure between component carriers 129

6.2.1.4 UE sounding procedure for positioning purposes 131

6.2.2 UE DM-RS transmission procedure 131

6.2.3 UE PT-RS transmission procedure 133

6.2.3.1 UE PT-RS transmission procedure when transform precoding is not enabled 133

6.2.3.2 UE PT-RS transmission procedure when transform precoding is enabled 135

6.3 UE PUSCH frequency hopping procedure 136

6.3.1 Frequency hopping for PUSCH repetition Type A 136

6.3.2 Frequency hopping for PUSCH repetition Type B 137

6.4 UE PUSCH preparation procedure time 137

7 UE procedures for transmitting and receiving on a carrier with intra-cell guard bands 138

8 Physical sidelink shared channel related procedures 138

8.1 UE procedure for transmitting the physical sidelink shared channel 139

8.1.1 Transmission schemes 139

8.1.2 Resource allocation 139

8.1.2.1 Resource allocation in time domain 139

8.1.2.2 Resource allocation in frequency domain 140

8.1.3 Modulation order, target code rate, redundancy version and transport block size determination 140

8.1.3.1 Modulation order and target code rate determination 140

8.1.3.2 Transport block size determination 140

8.1.4 UE procedure for determining the subset of resources to be reported to higher layers in PSSCH resource selection in sidelink resource allocation mode 2 140

8.1.5 UE procedure for determining slots and resource blocks for PSSCH transmission associated with an SCI format 0-1 142

8.2 UE procedure for transmitting sidelink reference signals 142

8.2.1 CSI-RS transmission procedure 142

8.2.2 PSSCH DM-RS transmission procedure 142

8.2.3 PT-RS transmission procedure 143

8.3 UE procedure for receiving the physical sidelink shared channel 143

8.4 UE procedure for receiving reference signals 143

8.4.1 CSI-RS reception procedure 143

8.4.2 DM-RS reception procedure for RSRP computation 143

8.4.3 PT-RS reception procedure 143

8.5 UE procedure for reporting channel state information (CSI) 143

8.5.1 Channel state information framework 143

8.5.1.1 Reporting configurations 144

8.5.1.2 Triggering of CSI reports 144

8.5.2 Channel state information 144

8.5.2.1 CSI reporting quantities 144

8.5.2.1.1 Channel quality indicator (CQI) 144

8.5.2.2 Reference signal (CSI-RS) 144

8.5.2.3 CSI reference resource definition 144

8.5.3 CSI reporting 144

Annex A (informative): Change history 145

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies and establishes the characteristics of the physicals layer procedures of data channels for 5G-NR.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications"

[2] 3GPP TS 38.201: " NR; Physical Layer – General Description"

[3] 3GPP TS 38.202: "NR; Services provided by the physical layer"

[4] 3GPP TS 38.211: "NR; Physical channels and modulation"

[5] 3GPP TS 38.212: "NR; Multiplexing and channel coding"

[6] 3GPP TS 38.213: "NR; Physical layer procedures for control"

[7] 3GPP TS 38.215: "NR; Physical layer measurements"

[8] 3GPP TS 38.101: "NR; User Equipment (UE) radio transmission and reception"

[9] 3GPP TS 38.104: "NR; Base Station (BS) radio transmission and reception"

[10] 3GPP TS 38.321: "NR; Medium Access Control (MAC) protocol specification"

[11] 3GPP TS 38.133: "NR; Requirements for support of radio resource management"

[12] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol specification"

[13] 3GPP TS 38.306: "NR; User Equipment (UE) radio access capabilities"

[14] 3GPP TS 38.423: "NG-RAN; Xn signalling transport"

[15] 3GPP TS 36.211: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical channels and modulation"

[16] 3GPP TS 37.213: "Physical layer procedures for shared spectrum channel access"

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

BWP Bandwidth part

CBG Code block group

CLI Cross Link Interference

CP Cyclic prefix

CQI Channel quality indicator

CPU CSI processing unit

CRB Common resource block

CRC Cyclic redundancy check

CRI CSI-RS Resource Indicator

CSI Channel state information

CSI-RS Channel state information reference signal

CSI-RSRP CSI reference signal received power

CSI-RSRQ CSI reference signal received quality

CSI-SINR CSI signal-to-noise and interference ratio

CW Codeword

DCI Downlink control information

DL Downlink

DM-RS Dedicated demodulation reference signals

EPRE Energy per resource element

IAB-MT Integrated Access and Backhaul – Mobile Terminal

L1-RSRP Layer 1 reference signal received power

LI Layer Indicator

MCS Modulation and coding scheme

PDCCH Physical downlink control channel

PDSCH Physical downlink shared channel

PSS Primary Synchronisation signal

PUCCH Physical uplink control channel

QCL Quasi co-location

PMI Precoding Matrix Indicator

PRB Physical resource block

PRG Precoding resource block group

PRS Positioning reference signal

PT-RS Phase-tracking reference signal

RB Resource block

RBG Resource block group

RI Rank Indicator

RIV Resource indicator value

RS Reference signal

SLIV Start and length indicator value

SR Scheduling Request

SRS Sounding reference signal

SS Synchronisation signal

SSS Secondary Synchronisation signal

SS-RSRP SS reference signal received power

SS-RSRQ SS reference signal received quality

SS-SINR SS signal-to-noise and interference ratio

TB Transport Block

TCI Transmission Configuration Indicator

TDM Time division multiplexing

UE User equipment

UL Uplink

# 4 Power control

Throughout this specification, unless otherwise noted, statements using the term "UE" in clauses 4, 5, or 6 are equally applicable to the IAB-MT part of an IAB node.

## 4.1 Power allocation for downlink

The gNB determines the downlink transmit EPRE.

For the purpose of SS-RSRP, SS-RSRQ and SS-SINR measurements, the UE may assume downlink EPRE is constant across the bandwidth. For the purpose of SS-RSRP, SS-RSRQ and SS-SINR measurements, the UE may assume downlink EPRE is constant over SSS carried in different SS/PBCH blocks. For the purpose of SS-RSRP, SS-RSRQ and SS-SINR measurements, the UE may assume that the ratio of SSS EPRE to PBCH DM-RS EPRE is 0 dB.

For the purpose of CSI-RSRP, CSI-RSRQ and CSI-SINR measurements, the UE may assume downlink EPRE of a port of CSI-RS resource configuration is constant across the configured downlink bandwidth and constant across all configured OFDM symbols.

The downlink SS/PBCH SSS EPRE can be derived from the SS/PBCH downlink transmit power given by the parameter *ss-PBCH-BlockPower* provided by higher layers. The downlink SSS transmit power is defined as the linear average over the power contributions (in [W]) of all resource elements that carry the SSS within the operating system bandwidth.

The downlink CSI-RS EPRE can be derived from the SS/PBCH block downlink transmit power given by the parameter *ss-PBCH-BlockPower* and CSI-RS power offset given by the parameter *powerControlOffsetSS* provided by higher layers. The downlink reference-signal transmit power is defined as the linear average over the power contributions (in [W]) of the resource elements that carry the configured CSI-RS within the operating system bandwidth.

For downlink DM-RS associated with PDSCH, the UE may assume the ratio of PDSCH EPRE to DM-RS EPRE ( [dB]) is given by Table 4.1-1 according to the number of DM-RS CDM groups without data as described in Clause 5.1.6.2. The DM-RS scaling factor  specified in Clause 7.4.1.1.2 of [4, TS 38.211] is given by .

Table 4.1-1: The ratio of PDSCH EPRE to DM-RS EPRE

|  |  |  |
| --- | --- | --- |
| Number of DM-RS CDM groups without data | DM-RS configuration type 1 | DM-RS configuration type 2 |
| 1 | 0 dB | 0 dB |
| 2 | -3 dB | -3 dB |
| 3 | - | -4.77 dB |

When the UE is scheduled with a PT-RS port associated with the PDSCH,

- if the UE is configured with the higher layer parameter *epre-Ratio*, the ratio of PT-RS EPRE to PDSCH EPRE per layer per RE for PT-RS port () is given by Table 4.1-2 according to the *epre-Ratio*, the PT-RS scaling factor specified in clause 7.4.1.2.2 of [4, TS 38.211] is given by.

- otherwise, the UE shall assume *epre-Ratio* is set to state '0' in Table 4.1-2 if not configured.

Table 4.1-2: PT-RS EPRE to PDSCH EPRE per layer per RE ()

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *epre-Ratio* | The number of PDSCH layers | | | | | |
| 1 | 2 | 3 | 4 | 5 | 6 |
| 0 | 0 | 3 | 4.77 | 6 | 7 | 7.78 |
| 1 | 0 | 0 | 0 | 0 | 0 | 0 |
| 2 | reserved | | | | | |
| 3 | reserved | | | | | |

For link recovery, as described in clause 6 of [6, TS 38.213] the ratio of the PDCCH EPRE to NZP CSI-RS EPRE is assumed as 0 dB.

# 5 Physical downlink shared channel related procedures

## 5.1 UE procedure for receiving the physical downlink shared channel

For downlink, a maximum of 16 HARQ processes per cell is supported by the UE. The number of processes the UE may assume will at most be used for the downlink is configured to the UE for each cell separately by higher layer parameter *nrofHARQ-ProcessesForPDSCH*, and when no configuration is provided the UE may assume a default number of 8 processes.

A UE shall upon detection of a PDCCH with a configured DCI format 1\_0, 1\_1 or 1\_2 decode the corresponding PDSCHs as indicated by that DCI. For any HARQ process ID(s) in a given scheduled cell, the UE is not expected to receive a PDSCH that overlaps in time with another PDSCH. The UE is not expected to receive another PDSCH for a given HARQ process until after the end of the expected transmission of HARQ-ACK for that HARQ process, where the timing is given by Clause 9.2.3 of [6]. In a given scheduled cell, the UE is not expected to receive a first PDSCH in slot *i*, with the corresponding HARQ-ACK assigned to be transmitted in slot *j*, and a second PDSCH starting later than the first PDSCH with its corresponding HARQ-ACK assigned to be transmitted in a slot before slot *j*. For any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start receiving a first PDSCH starting in symbol *j* by a PDCCH ending in symbol *i*, the UE is not expected to be scheduled to receive a PDSCH starting earlier than the end of the first PDSCH with a PDCCH that ends later than symbol *i*. In a given scheduled cell, for any PDSCH corresponding to SI-RNTI, the UE is not expected to decode a re-transmission of an earlier PDSCH with a starting symbol less than *N* symbols after the last symbol of that PDSCH, where the value of *N* depends on the PDSCH subcarrier spacing configuration *μ,* with *N*=13 for *μ*=0, *N*=13 for *μ*=1, *N*=20 for *μ*=2, and *N*=24 for *μ*=3.

When receiving PDSCH scheduled with SI-RNTI or P-RNTI, the UE may assume that the DM-RS port of PDSCH is quasi co-located with the associated SS/PBCH block with respect to Doppler shift, Doppler spread, average delay, delay spread, spatial RX parameters when applicable.

When receiving PDSCH scheduled with RA-RNTI, or MsgB-RNTI, the UE may assume that the DM-RS port of PDSCH is quasi co-located with the SS/PBCH block or the CSI-RS resource the UE used for RACH association as applicable, and transmission with respect to Doppler shift, Doppler spread, average delay, delay spread, spatial RX parameters when applicable. When receiving a PDSCH scheduled with RA-RNTI in response to a random access procedure triggered by a PDCCH order which triggers contention-free random access procedure for the SpCell [10, TS 38.321], the UE may assume that the DM-RS port of the received PDCCH order and the DM-RS ports of the corresponding PDSCH scheduled with RA-RNTI are quasi co-located with the same SS/PBCH block or CSI-RS with respect to Doppler shift, Doppler spread, average delay, delay spread, spatial RX parameters when applicable.

When receiving PDSCH in response to a PUSCH transmission scheduled by a RAR UL grant or corresponding PUSCH retransmission, or when receiving PDSCH in response to a PUSCH for Type-2 random access procedure, or a PUSCH scheduled by a fallbackRAR UL grant or corresponding PUSCH retransmission, the UE may assume that the DM-RS port of PDSCH is quasi co-located with the SS/PBCH block the UE selected for RACH association and transmission with respect to Doppler shift, Doppler spread, average delay, delay spread, spatial RX parameters when applicable.

If the UE is not configured for PUSCH/PUCCH transmission for at least one serving cell configured with slot formats comprised of DL and UL symbols, and if the UE is not capable of simultaneous reception and transmission on serving cell *c1*and serving cell *c2*, the UE is not expected to receive PDSCH on serving cell *c1* if the PDSCH overlaps in time with SRS transmission (including any interruption due to uplink or downlink RF retuning time [10]) on serving cell *c2* not configured for PUSCH/PUCCH transmission.

The UE is not expected to decode a PDSCH scheduled in a serving cell with C-RNTI or MCS-C-RNTI and another PDSCH scheduled in the same serving cell with CS-RNTI if the PDSCHs partially or fully overlap in time except if the PDCCH scheduling the PDSCH with C-RNTI or MCS-C-RNTI ends at least 14 symbols before the start of the PDSCH with CS-RNTI without the corresponding DCI, in which case the UE shall decode the PDSCH scheduled with C-RNTI or MCS-C-RNTI.

The UE is not expected to decode a PDSCH scheduled with C-RNTI, MCS-C-RNTI, or CS-RNTI if another PDSCH in the same cell scheduled with RA-RNTI or MsgB-RNTI partially or fully overlap in time.

The UE in RRC\_IDLE and RRC\_INACTIVE modes shall be able to decode two PDSCHs each scheduled with SI-RNTI, P-RNTI, RA-RNTI or TC-RNTI, with the two PDSCHs partially or fully overlapping in time in non-overlapping PRBs.

On a frequency range 1 cell, the UE shall be able to decode a PDSCH scheduled with C-RNTI, MCS-C-RNTI, or CS-RNTI and, during a process of P-RNTI triggered SI acquisition, another PDSCH scheduled with SI-RNTI that partially or fully overlap in time in non-overlapping PRBs, unless the PDSCH scheduled with C-RNTI, MCS-C-RNTI, or CS-RNTI requires Capability 2 processing time according to clause 5.3 in which case the UE may skip decoding of the scheduled PDSCH with C-RNTI, MCS-C-RNTI, or CS-RNTI.

On a frequency range 2 cell, the UE is not expected to decode a PDSCH scheduled with C-RNTI, MCS-C-RNTI, or CS-RNTI if in the same cell, during a process of P-RNTI triggered SI acquisition, another PDSCH scheduled with SI-RNTI partially or fully overlap in time.

The UE is expected to decode a PDSCH scheduled with C-RNTI, MCS-C-RNTI, or CS-RNTI during a process of autonomous SI acquisition.

If the UE is configured by higher layers to decode a PDCCH with its CRC scrambled by a CS-RNTI, the UE shall receive PDSCH transmissions without corresponding PDCCH transmissions using the higher-layer-provided PDSCH configuration for those PDSCHs.

If a UE is configured by higher layer parameter *PDCCH-Config* that contains two different values of *CORESETPoolIndex* in *ControlResourceSet*, the UE may expect to receive multiple PDCCHs scheduling fully/partially/non-overlapped PDSCHs in time and frequency domain. The UE may expect the reception of full/partially-overlapped PDSCHs in time only when PDCCHs that schedule two PDSCHs are associated to different *ControlResourceSets* having different values of *CORESETPoolIndex*. For a *ControlResourceSet* without *CORESETPoolIndex*, the UE may assume that the *ControlResourceSet* is assigned with *CORESETPoolIndex* as 0. When the UE is scheduled with full/partially/non-overlapped PDSCHs in time and frequency domain, the full scheduling information for receiving a PDSCH is indicated and carried only by the corresponding PDCCH, the UE is expected to be scheduled with the same active BWP and the same SCS. When the UE is scheduled with full/partially-overlapped PDSCHs in time and frequency domain, the UE can be scheduled with at most two codewords simultaneously. When PDCCHs that schedule two PDSCHs are associated to different *ControlResourceSets* having different values of *CORESETPoolIndex,* the following operations are allowed:

- For any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start receiving a first PDSCH starting in symbol *j* by a PDCCH associated with a value of *CORESETpoolIndex* ending in symbol *i*, the UE can be scheduled to receive a PDSCH starting earlier than the end of the first PDSCH with a PDCCH associated with a different value of *CORESETpoolIndex* that ends later than symbol *i*.

- In a given scheduled cell, the UE can receive a first PDSCH in slot *i*, with the corresponding HARQ-ACK assigned to be transmitted in slot *j*, and a second PDSCH associated with a value of *CORESETpoolindex* different from that of the first PDSCH starting later than the first PDSCH with its corresponding HARQ-ACK assigned to be transmitted in a slot before slot *j*.

If PDCCHs that schedule corresponding PDSCHs are associated to the same or different *ControlResourceSets* having the same value of *CORESETPoolIndex*, the UE procedure for receiving the PDSCH upon detection of a PDCCH follows Clause 5.1.

When a UE is configured by higher layer parameter *RepSchemeEnabler* set to one of ‘*FDMSchemeA’*, ‘*FDMSchemeB’*, ‘*TDMSchemeA’*, if the UE is indicated with two TCI states in a codepoint of the DCI field *'Transmission Configuration Indication'* and DM-RS port(s) within one CDM group in the DCI field “*Antenna Port(s)”*.

- When two TCI states are indicated in a DCI and the UE is set to ‘*FDMSchemeA’,* the UE shall receive a single PDSCH transmission occasion of the TB with each TCI state associated to a non-overlapping frequency domain resource allocation as described in Clause 5.1.2.3.

- When two TCI states are indicated in a DCI and the UE is set to ‘*FDMSchemeB’*, the UE shall receive two PDSCH transmission occasions of the same TB with each TCI state associated to a PDSCH transmission occasion which has non-overlapping frequency domain resource allocation with respect to the other PDSCH transmission occasion as described in Clause 5.1.2.3.

- When two TCI states are indicated in a DCI and the UE is set to ‘*TDMSchemeA’*, the UE shall receive two PDSCH transmission occasions of the same TB with each TCI state associated to a PDSCH transmission occasion which has non-overlapping time domain resource allocation with respect to the other PDSCH transmission occasion and both PDSCH transmission occasions shall be received within a given slot as described in Clause 5.1.2.1.

When a UE is configured by the higher layer parameter *PDSCH-config* that indicates at least one entry in *pdsch-TimeDomainAllocationList* containing *RepNumR16* in *PDSCH-TimeDomainResourceAllocatio*n, the UE may expect to be indicated with one or two TCI states in a codepoint of the DCI field *'Transmission Configuration Indication'* together with the DCI field “*Time domain resource assignment*’ indicating an entry in *pdsch-TimeDomainAllocationList* which contain *RepNum16* in *PDSCH-TimeDomainResourceAllocatio*n and DM-RS port(s) within one CDM group in the DCI field “*Antenna Port(s)”*.

- When two TCI states are indicated in a DCI with ‘*Transmission Configuration Indication*’ field, the UE may expect to receive multiple slot level PDSCH transmission occasions of the same TB with two TCI states used across multiple PDSCH transmission occasions as defined in Clause 5.1.2.1.

- When one TCI state is indicated in a DCI with ‘*Transmission Configuration Indication*’ field, the UE may expect to receive multiple slot level PDSCH transmission occasions of the same TB with one TCI state used across multiple PDSCH transmission occasions as defined in Clause 5.1.2.1.

When a UE is not indicated with a DCI that DCI field “*Time domain resource assignment*’ indicating an entry in *pdsch-TimeDomainAllocationList* which contain *RepNumR16* in *PDSCH-TimeDomainResourceAllocatio*n, and it is indicated with two TCI states in a codepoint of the DCI field *'Transmission Configuration Indication'* and DM-RS port(s) within two CDM group in the DCI field “*Antenna Port(s)”*, the UE may expect to receive a single PDSCH where the association between the DM-RS ports and the TCI states are as defined in Clause 5.1.6.2.

When a UE is not indicated with a DCI that DCI field “*Time domain resource assignment*’ indicating an entry in *pdsch-TimeDomainAllocationList* which contain *RepNumR16* in *PDSCH-TimeDomainResourceAllocatio*n, and it is indicated with one TCI states in a codepoint of the DCI field *'Transmission Configuration Indication',* the UE procedure for receiving the PDSCH upon detection of a PDCCH follows Clause 5.1.

If more than one PDSCH on a serving cell each without a corresponding PDCCH transmission are partially or fully overlapping in time, a UE is not required to decode a PDSCH among these PDSCHs other than one with the lowest configured *sps-ConfigIndex*.

### 5.1.1 Transmission schemes

Only one transmission scheme is defined for the PDSCH, and is used for all PDSCH transmissions.

#### 5.1.1.1 Transmission scheme 1

For transmission scheme 1 of the PDSCH, the UE may assume that a gNB transmission on the PDSCH would be performed with up to 8 transmission layers on antenna ports 1000-1011 as defined in Clause 7.3.1.4 of [4, TS 38.211], subject to the DM-RS reception procedures in Clause 5.1.6.2.

### 5.1.2 Resource allocation

#### 5.1.2.1 Resource allocation in time domain

When the UE is scheduled to receive PDSCH by a DCI, the *Time domain resource assignment* field value *m* of the DCI provides a row index *m* + 1 to an allocation table. The determination of the used resource allocation table is defined in Clause 5.1.2.1.1. The indexed row defines the slot offset *K0*, the start and length indicator *SLIV*, or directly the start symbol *S* and the allocation length *L*, and the PDSCH mapping type to be assumed in the PDSCH reception.

Given the parameter values of the indexed row:

- The slot allocated for the PDSCH is , where *n* is the slot with the scheduling DCI, and *K0* is based on the numerology of PDSCH, and  and are the subcarrier spacing configurations for PDSCH and PDCCH, respectively, and

- and the  for the {scheduling, scheduled} carrier pair is defined in clause 4.5 of [4, TS 38.211].

- The reference point *S0* for starting symbol *S* is defined as:

- if configured with *ReferenceofSLIV-ForDCIFormat1\_2*, and when receiving PDSCH scheduled by DCI format 1\_2 with CRC scrambled by C-RNTI, MCS-C-RNTI, CS-RNTI with *K0=0*, and PDSCH mapping Type B, the starting symbol *S* is relative to the starting symbol *S0* of the PDCCH monitoring occasion where DCI format 1\_2 is detected;

- otherwise, the starting symbol *S* is relative to the start of the slot using *S0=0*, and the starting symbol *S* relative to the start of the slot, and the number of consecutive symbols *L* counting from the symbol *S* allocated for the PDSCH are determined from the start and length indicator *SLIV*:

if  then



else



where, and

- the PDSCH mapping type is set to Type A or Type B as defined in Clause 7.4.1.1.2 of [4, TS 38.211].

The UE shall consider the *S* and *L* combinations defined in table 5.1.2.1-1 satisfying  for normal cyclic prefix and  for extended cyclic prefix as valid PDSCH allocations:

Table 5.1.2.1-1: Valid *S* and *L* combinations

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| PDSCH mapping type | Normal cyclic prefix | | | Extended cyclic prefix | | |
| *S* | *L* | *S+L* | *S* | *L* | *S+L* |
| Type A | {0,1,2,3}  (Note 1) | {3,…,14} | {3,…,14} | {0,1,2,3}  (Note 1) | {3,…,12} | {3,…,12} |
| Type B | {0,…,12} | {2,…,13} | {2,…,14} | {0,…,10} | {2,4,6} | {2,…,12} |
| Note 1: S = 3 is applicable only if *dmrs-TypeA-Position* = 3 | | | | | | |

When receiving PDSCH scheduled by DCI format 1\_1 or 1\_2 in PDCCH with CRC scrambled by C-RNTI, MCS-C-RNTI, CS-RNTI, or PDSCH scheduled without corresponding PDCCH transmission using *sps-Config* and activated by DCI format 1\_1 or 1\_2, if the UE is configured with *pdsch-AggregationFactor*, the same symbol allocation is applied across the *pdsch-AggregationFactor* consecutive slots. The UE may expect that the TB is repeated within each symbol allocation among each of the *pdsch-AggregationFactor* consecutive slots and the PDSCH is limited to a single transmission layer. The redundancy version to be applied on the *n*th transmission occasion of the TB, where n = 0, 1, …*pdsch-AggregationFactor* -1, is determined according to table 5.1.2.1-2 and "*rvid* indicated by the DCI scheduling the PDSCH" in table 5.1.2.1-2 is assumed to be 0 for PDSCH scheduled without corresponding PDCCH transmission using *sps-Config* and activated by DCI format 1\_1 or 1\_2.

Table 5.1.2.1-2: Applied redundancy version when *pdsch-AggregationFactor* is present

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *rvid* indicated by the DCI scheduling the PDSCH | *rvid* to be applied to *n*th transmission occasion | | | |
| *n* mod 4 = 0 | *n* mod 4 = 1 | *n* mod 4 = 2 | *n* mod 4 = 3 |
| 0 | 0 | 2 | 3 | 1 |
| 2 | 2 | 3 | 1 | 0 |
| 3 | 3 | 1 | 0 | 2 |
| 1 | 1 | 0 | 2 | 3 |

A PDSCH reception in a slot of a multi-slot PDSCH reception is omitted according to the conditions in Clause 11.1 of [6, TS38.213].

The UE is not expected to receive a PDSCH with mapping type A in a slot, if the PDCCH scheduling the PDSCH was received in the same slot and was not contained within the first three symbols of the slot.

The UE is not expected to receive a PDSCH with mapping type B in a slot, if the first symbol of the PDCCH scheduling the PDSCH was received in a later symbol than the first symbol indicated in the PDSCH time domain resource allocation.

When the UE configured with [*minimumSchedulingOffset*] in an active DL BWP it applies a minimum scheduling offset restriction indicated by the **[**‘Minimum applicable scheduling offset indicator’]field in DCI format 0\_1 or 1\_1. When the UE configured with [*minimumSchedulingOffset*] in active DL BWP and it has not received [‘Minimum applicable scheduling offset indicator’] field in DCI format 0\_1 or 1\_1, UE shall apply a minimum scheduling offset restriction indicated based on [‘Minimum applicable scheduling offset indicator’] value ‘0’. When the *minimum scheduling offset restriction* is applied the UE is not expected to be scheduled with a DCI in slot *n* to receive a PDSCH scheduled with C-RNTI, CS-RNTI or MCS-C-RNTI with *K*0 smaller than the applicable minimum scheduling offset restriction *K*0min. The minimum scheduling offset restriction is not applied when PDSCH transmission is scheduled with C-RNTI, CS-RNTI or MCS-C-RNTI in common search space associated with CORESET0 and default PDSCH time domain resource allocation is used or when PDSCH transmission is scheduled with SI-RNTI or RA-RNTI. The application delay of the change of the minimum scheduling offset restriction is determined in Section 5.3.1.

The UE is not expected to be configured with *ReferenceofSLIV-ForDCIFormat1\_2* for serving cells configured for cross-carrier scheduling with a scheduling cell of a different downlink SCS configuration.

When a UE is configured by the higher layer parameter *RepSchemeEnabler* set to ‘*TDMSchemeA’* and indicated DM-RS port(s) within one CDM group in the DCI field “*Antenna Port(s)”*, the number of PDSCH transmission occasions is derived by the number of TCI states indicated by the DCI field *'Transmission Configuration Indication'* of the scheduling DCI*.*

- If two TCI states are indicated by the DCI field ‘*Transmission Configuration Indication*’, the UE is expected to receive two PDSCH transmission occasions, where the first TCI state is applied to the first PDSCH transmission occasion and resource allocation in time domain for the first PDSCH transmission occasion follows Clause 5.1.2.1. The second TCI state is applied to the second PDSCH transmission occasion, and the second PDSCH transmission occasion shall have the same number of symbols as the first PDSCH transmission occasion. If the UE is configured by the higher layers with a value in *StartingSymbolOffsetK*, it shall determine that the first symbol of the second PDSCH transmission occasion starts after symbols from the last symbol of the first PDSCH transmission occasion. If the value is not configured via the higher layer parameter *StartingSymbolOffsetK*, = 0 shall be assumed by the UE. The UE is not expected to receive more than two PDSCH transmission layers for each PDSCH transmission occasion. For two PDSCH transmission occasions, the redundancy version to be applied is derived according to Table 5.1.2.1-2, where applied respectively to the first and second TCI state.

- Otherwise, the UE is expected to receive a single PDSCH transmission occasion, and the resource allocation in the time domain follows Clause 5.1.2.1.

When a UE configured by the higher layer parameter *PDSCH-config* that indicates at least one entry in *pdsch-TimeDomainAllocationList* contain*RepNumR16* in *PDSCH-TimeDomainResourceAllocatio*n,

- If two TCI states are indicated by the DCI field ‘Transmission Configuration Indication’ together with the DCI field “Time domain resource assignment’ indicating an entry in pdsch-TimeDomainAllocationList which contain RepNumR16 in PDSCH-TimeDomainResourceAllocation and DM-RS port(s) within one CDM group in the DCI field “Antenna Port(s)”, the same SLIV is applied for all PDSCH transmission occasions, the first TCI state is applied to the first PDSCH transmission occasion and resource allocation in time domain for the first PDSCH transmission occasion follows Clause 5.1.2.1.

When the value indicated by RepNumR16 in PDSCH-TimeDomainResourceAllocation equals to two, the second TCI state is applied to the second PDSCH transmission occasion. When the value indicated by RepNumR16 in PDSCH-TimeDomainResourceAllocation is larger than two, the UE may be further configured to enable CycMapping or SeqMapping in RepTCIMapping.

- When CycMapping is enabled, the first and second TCI states are applied to the first and second PDSCH transmission occasions, respectively, and the same TCI mapping pattern continues to the remaining PDSCH transmission occasions.

- When SeqMapping is enabled, first TCI state is applied to the first and second PDSCH transmissions, and the second TCI state is applied to the third and fourth PDSCH transmissions, and the same TCI mapping pattern continues to the remaining PDSCH transmission occasions.

The UE may expect that each PDSCH transmission occasion is limited to two transmission layers. For all PDSCH transmission occasions associated with the first TCI state, the redundancy version to be applied is derived according to Table 5.1.2.1-2, where is counted only considering PDSCH transmission occasions associated with the first TCI state. The redundancy version for PDSCH transmission occasions associated with the second TCI state is derived according to Table 5.1.2.1-3, where additional shifting operation for each redundancy version is configured by higher layer parameter RVSeqOffset and is counted only considering PDSCH transmission occasions associated with the second TCI state.

Table 5.1.2.1-3: Applied redundancy version for the second TCI state when *RVSeqOffset* is present

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *rvid* indicated by the DCI scheduling the PDSCH | *rvid* to be applied to *n*th transmission occasion with second TCI state | | | |
| *n* mod 4 = 0 | *n* mod 4 = 1 | *n* mod 4 = 2 | *n* mod 4 = 3 |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

- If one TCI state is indicated by the DCI field ‘Transmission Configuration Indication’ together with the DCI field “Time domain resource assignment’ indicating an entry in pdsch-TimeDomainAllocationList which contain RepNumR16 in PDSCH-TimeDomainResourceAllocation and DM-RS port(s) within one CDM group in the DCI field “Antenna Port(s)”, the same SLIV is applied for all PDSCH transmission occasions, the first PDSCH transmission occasion follows Clause 5.1.2.1, the same TCI state is applied to all PDSCH transmission occasions. The UE may expect that each PDSCH transmission occasion is limited to two transmission layers. For all PDSCH transmission occasions, the redundancy version to be applied is derived according to Table 5.1.2.1-2, where is counted considering PDSCH transmission occasions.

- Otherwise, the UE is expected to receive a single PDSCH transmission occasion, and the resource allocation in the time domain follows Clause 5.1.2.1.

##### 5.1.2.1.1 Determination of the resource allocation table to be used for PDSCH

Table 5.1.2.1.1-1 and Table 5.1.2.1.1-1A define which PDSCH time domain resource allocation configuration to apply. Either a default PDSCH time domain allocation A, B or C according to tables 5.1.2.1.1-2, 5.1.2.1.1-3, 5.1.2.1.1-4 and 5.1.2.1.1-5 is applied, or the higher layer configured *pdsch-TimeDomainAllocationList* or *pdsch-TimeDomainAllocationList-ForDCIFormat1\_2* is applied. For operation with shared spectrum channel access, as described in [16, TS 37.213], UE reinterprets *S* and *L* in row 9 of Table 5.1.2.1.1-2 as *S=6* and *L=7*.

Table 5.1.2.1.1-1: Applicable PDSCH time domain resource allocation for DCI formats 1\_0 and 1\_1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RNTI | PDCCH search space | SS/PBCH block and CORESET multiplexing pattern | *pdsch-ConfigCommon* includes *pdsch-TimeDomainAllocationList* | *pdsch-Config* includes *pdsch-TimeDomainAllocationList* | PDSCH time domain resource allocation to apply |
| SI-RNTI | Type0 common | 1 | - | - | Default A for normal CP |
| 2 | - | - | Default B |
| 3 | - | - | Default C |
| SI-RNTI | Type0A common | 1 | No | - | Default A |
| 2 | No | - | Default B |
| 3 | No | - | Default C |
| 1,2,3 | Yes | - | *pdsch-TimeDomainAllocationList provided in pdsch-ConfigCommon* |
| RA-RNTI, MsgB-RNTI, TC-RNTI | Type1 common | 1, 2, 3 | No | - | Default A |
| 1, 2, 3 | Yes | - | *pdsch-TimeDomainAllocationList* provided in *pdsch-ConfigCommon* |
| P-RNTI | Type2 common | 1 | No | - | Default A |
| 2 | No | - | Default B |
| 3 | No | - | Default C |
| 1,2,3 | Yes | - | *pdsch-TimeDomainAllocationList provided in pdsch-ConfigCommon* |
| C-RNTI, MCS-C-RNTI, CS-RNTI | Any common search space associated with CORESET 0 | 1, 2, 3 | No | - | Default A |
| 1, 2, 3 | Yes | - | *pdsch-TimeDomainAllocationList* provided in *pdsch-ConfigCommon* |
| C-RNTI, MCS-C-RNTI, CS-RNTI | Any common search space not associated with CORESET 0  UE specific search space | 1,2,3 | No | No | Default A |
| 1,2,3 | Yes | No | *pdsch-TimeDomainAllocationList* provided in *pdsch-ConfigCommon* |
| 1,2,3 | No/Yes | Yes | *pdsch-TimeDomainAllocationList* provided in *pdsch-Config* |

Table 5.1.2.1.1-1A: Applicable PDSCH time domain resource allocation for DCI format 1\_2

|  |  |  |  |
| --- | --- | --- | --- |
| *pdsch-ConfigCommon* includes *pdsch-TimeDomainAllocationList* | *pdsch-Config includes pdsch-TimeDomainAllocationList* | *pdsch-Config* includes *pdsch-TimeDomainAllocationList* *-ForDCIformat1\_2* | PDSCH time domain resource allocation to apply |
| No | No | No | Default A |
| Yes | No | No | *pdsch-TimeDomainAllocationList* provided in *pdsch-ConfigCommon* |
| No/Yes | Yes | No | *pdsch-TimeDomainAllocationList* provided in *pdsch-Config* |
| No/Yes | No/Yes | Yes | *pdsch-TimeDomainAllocationList-ForDCIformat1\_2* provided in *pdsch-Config* |

Table 5.1.2.1.1-2: Default PDSCH time domain resource allocation A for normal CP

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Row index | *dmrs-TypeA-Position* | PDSCH mapping type | *K0* | *S* | *L* |
| 1 | 2 | Type A | 0 | 2 | 12 |
| 3 | Type A | 0 | 3 | 11 |
| 2 | 2 | Type A | 0 | 2 | 10 |
| 3 | Type A | 0 | 3 | 9 |
| 3 | 2 | Type A | 0 | 2 | 9 |
| 3 | Type A | 0 | 3 | 8 |
| 4 | 2 | Type A | 0 | 2 | 7 |
| 3 | Type A | 0 | 3 | 6 |
| 5 | 2 | Type A | 0 | 2 | 5 |
| 3 | Type A | 0 | 3 | 4 |
| 6 | 2 | Type B | 0 | 9 | 4 |
| 3 | Type B | 0 | 10 | 4 |
| 7 | 2 | Type B | 0 | 4 | 4 |
| 3 | Type B | 0 | 6 | 4 |
| 8 | 2,3 | Type B | 0 | 5 | 7 |
| 9 | 2,3 | Type B | 0 | 5 | 2 |
| 10 | 2,3 | Type B | 0 | 9 | 2 |
| 11 | 2,3 | Type B | 0 | 12 | 2 |
| 12 | 2,3 | Type A | 0 | 1 | 13 |
| 13 | 2,3 | Type A | 0 | 1 | 6 |
| 14 | 2,3 | Type A | 0 | 2 | 4 |
| 15 | 2,3 | Type B | 0 | 4 | 7 |
| 16 | 2,3 | Type B | 0 | 8 | 4 |

Table 5.1.2.1.1-3: Default PDSCH time domain resource allocation A for extended CP

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Row index | *dmrs-TypeA-Position* | PDSCH mapping type | *K0* | *S* | *L* |
| 1 | 2 | Type A | 0 | 2 | 6 |
| 3 | Type A | 0 | 3 | 5 |
| 2 | 2 | Type A | 0 | 2 | 10 |
| 3 | Type A | 0 | 3 | 9 |
| 3 | 2 | Type A | 0 | 2 | 9 |
| 3 | Type A | 0 | 3 | 8 |
| 4 | 2 | Type A | 0 | 2 | 7 |
| 3 | Type A | 0 | 3 | 6 |
| 5 | 2 | Type A | 0 | 2 | 5 |
| 3 | Type A | 0 | 3 | 4 |
| 6 | 2 | Type B | 0 | 6 | 4 |
| 3 | Type B | 0 | 8 | 2 |
| 7 | 2 | Type B | 0 | 4 | 4 |
| 3 | Type B | 0 | 6 | 4 |
| 8 | 2,3 | Type B | 0 | 5 | 6 |
| 9 | 2,3 | Type B | 0 | 5 | 2 |
| 10 | 2,3 | Type B | 0 | 9 | 2 |
| 11 | 2,3 | Type B | 0 | 10 | 2 |
| 12 | 2,3 | Type A | 0 | 1 | 11 |
| 13 | 2,3 | Type A | 0 | 1 | 6 |
| 14 | 2,3 | Type A | 0 | 2 | 4 |
| 15 | 2,3 | Type B | 0 | 4 | 6 |
| 16 | 2,3 | Type B | 0 | 8 | 4 |

Table 5.1.2.1.1-4: Default PDSCH time domain resource allocation B

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Row index** | ***dmrs-TypeA-Position*** | **PDSCH mapping type** | ***K0*** | ***S*** | ***L*** |
| 1 | 2,3 | Type B | 0 | 2 | 2 |
| 2 | 2,3 | Type B | 0 | 4 | 2 |
| 3 | 2,3 | Type B | 0 | 6 | 2 |
| 4 | 2,3 | Type B | 0 | 8 | 2 |
| 5 | 2,3 | Type B | 0 | 10 | 2 |
| 6 | 2,3 | Type B | 1 | 2 | 2 |
| 7 | 2,3 | Type B | 1 | 4 | 2 |
| 8 | 2,3 | Type B | 0 | 2 | 4 |
| 9 | 2,3 | Type B | 0 | 4 | 4 |
| 10 | 2,3 | Type B | 0 | 6 | 4 |
| 11 | 2,3 | Type B | 0 | 8 | 4 |
| 12 (Note 1) | 2,3 | Type B | 0 | 10 | 4 |
| 13 (Note 1) | 2,3 | Type B | 0 | 2 | 7 |
| 14 (Note 1) | 2 | Type A | 0 | 2 | 12 |
| 3 | Type A | 0 | 3 | 11 |
| 15 | 2,3 | Type B | 1 | 2 | 4 |
| 16 | Reserved | | | | |
| Note 1: If the PDSCH was scheduled with SI-RNTI in PDCCH Type0 common search space, the UE may assume that this PDSCH resource allocation is not applied | | | | | |

Table 5.1.2.1.1-5: Default PDSCH time domain resource allocation C

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Row index** | ***dmrs-TypeA-Position*** | **PDSCH mapping type** | ***K0*** | ***S*** | ***L*** |
| 1 (Note 1) | 2,3 | Type B | 0 | 2 | 2 |
| 2 | 2,3 | Type B | 0 | 4 | 2 |
| 3 | 2,3 | Type B | 0 | 6 | 2 |
| 4 | 2,3 | Type B | 0 | 8 | 2 |
| 5 | 2,3 | Type B | 0 | 10 | 2 |
| 6 | Reserved | | | | |
| 7 | Reserved | | | | |
| 8 | 2,3 | Type B | 0 | 2 | 4 |
| 9 | 2,3 | Type B | 0 | 4 | 4 |
| 10 | 2,3 | Type B | 0 | 6 | 4 |
| 11 | 2,3 | Type B | 0 | 8 | 4 |
| 12 | 2,3 | Type B | 0 | 10 | 4 |
| 13 (Note 1) | 2,3 | Type B | 0 | 2 | 7 |
| 14 (Note 1) | 2 | Type A | 0 | 2 | 12 |
| 3 | Type A | 0 | 3 | 11 |
| 15 (Note 1) | 2,3 | Type A | 0 | 0 | 6 |
| 16 (Note 1) | 2,3 | Type A | 0 | 2 | 6 |
| Note 1: The UE may assume that this PDSCH resource allocation is not used, if the PDSCH was scheduled with SI-RNTI in PDCCH Type0 common search space | | | | | |

#### 5.1.2.2 Resource allocation in frequency domain

Two downlink resource allocation schemes, type 0 and type 1, are supported. The UE shall assume that when the scheduling grant is received with DCI format 1\_0, then downlink resource allocation type 1 is used.

If the scheduling DCI is configured to indicate the downlink resource allocation type as part of the *Frequency domain resource assignment* field by setting a higher layer parameter *resourceAllocation* in *pdsch-Config* to 'dynamicswitch', for DCI format 1\_1 or setting a higher layer parameter *resourceAllocation-ForDCIFormat1\_2* in *pdsch-Config* to 'dynamicswitch' for DCI format 1\_2, the UE shall use downlink resource allocation type 0 or type 1 as defined by this DCI field. Otherwise the UE shall use the downlink frequency resource allocation type as defined by the higher layer parameter *resourceAllocation* for DCI format 1\_1 or by the higher layer parameter *resourceAllocation-ForDCIFormat1\_2* for DCI format 1\_2.

If a bandwidth part indicator field is not configured in the scheduling DCI or the UE does not support active BWP change via DCI, the RB indexing for downlink type 0 and type 1 resource allocation is determined within the UE's active bandwidth part. If a bandwidth part indicator field is configured in the scheduling DCI and the UE supports active BWP change via DCI, the RB indexing for downlink type 0 and type 1 resource allocation is determined within the UE's bandwidth part indicated by bandwidth part indicator field value in the DCI. The UE shall upon detection of PDCCH intended for the UE determine first the downlink bandwidth part and then the resource allocation within the bandwidth part.

For a PDSCH scheduled with a DCI format 1\_0 in any type of PDCCH common search space, regardless of which bandwidth part is the active bandwidth part, RB numbering starts from the lowest RB of the CORESET in which the DCI was received; otherwise RB numbering starts from the lowest RB in the determined downlink bandwidth part.

##### 5.1.2.2.1 Downlink resource allocation type 0

In downlink resource allocation of type 0, the resource block assignment information includes a bitmap indicating the Resource Block Groups (RBGs) that are allocated to the scheduled UE where a RBG is a set of consecutive virtual resource blocks defined by higher layer parameter *rbg-Size* configured by *PDSCH-Config* and the size of the bandwidth part as defined in Table 5.1.2.2.1-1.

Table 5.1.2.2.1-1: Nominal RBG size *P*

|  |  |  |
| --- | --- | --- |
| Bandwidth Part Size | Configuration 1 | Configuration 2 |
| 1 – 36 | 2 | 4 |
| 37 – 72 | 4 | 8 |
| 73 – 144 | 8 | 16 |
| 145 – 275 | 16 | 16 |

The total number of RBGs () for a downlink bandwidth part *i* of size PRBs is given by , where

- the size of the first RBG is ,

- the size of last RBG is if  and *P* otherwise,

- the size of all other RBGs is *P*.

The bitmap is of size bits with one bitmap bit per RBG such that each RBG is addressable. The RBGs shall be indexed in the order of increasing frequency and starting at the lowest frequency of the bandwidth part. The order of RBG bitmap is such that RBG 0 to RBG are mapped from MSB to LSB. The RBG is allocated to the UE if the corresponding bit value in the bitmap is 1, the RBG is not allocated to the UE otherwise.

##### 5.1.2.2.2 Downlink resource allocation type 1

In downlink resource allocation of type 1, the resource block assignment information indicates to a scheduled UE a set of contiguously allocated non-interleaved or interleaved virtual resource blocks within the active bandwidth part of size  PRBs except for the case when DCI format 1\_0 is decoded in any common search space in which case the size of CORESET 0 shall be used if CORESET 0 is configured for the cell and the size of initial DL bandwidth part shall be used if CORESET 0 is not configured for the cell.

A downlink type 1 resource allocation field consists of a resource indication value (*RIV*) corresponding to a starting virtual resource block () and a length in terms of contiguously allocated resource blocks. The resource indication value is defined by

if  then



else



where≥ 1 and shall not exceed .

When the DCI size for DCI format 1\_0 in USS is derived from the size of DCI format 1\_0 in CSS but applied to an active BWP with size of , a downlink type 1 resource block assignment field consists of a resource indication value (*RIV*) corresponding to a starting resource block and a length in terms of virtually contiguously allocated resource blocks , where  is given by

- the size of CORESET 0 if CORESET 0 is configured for the cell;

- the size of initial DL bandwidth part if CORESET 0 is not configured for the cell.

The resource indication value is defined by:

if  then



else



where, and where shall not exceed .

If , *K* is the maximum value from set {1, 2, 4, 8} which satisfies ; otherwise *K* = 1.

When the scheduling grant is received with DCI format 1\_2, a downlink type 1 resource allocation field consists of [TBD]. [If the resource allocation indicates the corresponding PDSCH is mapped to RB index , the UE shall assume the PDSCH is also mapped to PRB indexes to .]

#### 5.1.2.3 Physical resource block (PRB) bundling

The PRB bundling procedures for PDSCH scheduled by PDCCH with DCI format 1\_1 described in this clause equally apply to PDSCH scheduled by PDCCH with DCI format 1\_2, by applying the parameters of *prb-BundlingType-ForDCIFormat1\_2* instead of *prb-BundlingType* as well as *vrb-ToPRB-Interleaver-ForDCIFormat1\_2* instead of *vrb-ToPRB-Interleaver*.

A UE may assume that precoding granularity is  consecutive resource blocks in the frequency domain.  can be equal to one of the values among {2, 4, wideband}.

If  is determined as "wideband", the UE is not expected to be scheduled with non-contiguous PRBs and the UE may assume that the same precoding is applied to the allocated resource.

If  is determined as one of the values among {2, 4}, Precoding Resource Block Group (PRGs) partitions the bandwidth part *i* with  consecutive PRBs. Actual number of consecutive PRBs in each PRG could be one or more.

The first PRG size is given by and the last PRG size given by  if , and the last PRG size is if .

The UE may assume the same precoding is applied for any downlink contiguous allocation of PRBs in a PRG.

For PDSCH carrying SIB1 scheduled by PDCCH with CRC scrambled by SI-RNTI, a PRG is partitioned from the lowest numbered resource block of CORESET 0 if the corresponding PDCCH is associated with CORESET 0 and Type0-PDCCH common search space and is addressed to SI-RNTI; otherwise, a PRG is partitioned from common resource block 0.

If a UE is scheduled a PDSCH with DCI format 1\_0, the UE shall assume that is equal to 2 PRBs.

When receiving PDSCH scheduled by PDCCH with DCI format 1\_1 with CRC scrambled by C-RNTI, MCS-C-RNTI, or CS-RNTI, for bandwidth part is equal to 2 PRBs unless configured by the higher layer parameter *prb-BundlingType* given by *PDSCH-Config*.

When receiving PDSCH scheduled by PDCCH with DCI format 1\_1 with CRC scrambled by C-RNTI, MCS-C-RNTI, or CS-RNTI, if the higher layer parameter *prb-BundlingType* is set to 'dynamicBundling', the higher layer parameters *bundleSizeSet1* and *bundleSizeSet2* configure two sets of  values, the first set can take one or two  values among {2, 4, wideband}, and the second set can take one  value among {2, 4, wideband}.

If the *PRB bundling size indicator* signalled in DCI format 1\_1 as defined in Clause 7.3.1.2.2 of [5, TS 38.212]

- is set to '0', the UE shall use the  value from the second set of  values when receiving PDSCH scheduled by the same DCI.

- is set to '1' and one value is configured for the first set of  values, the UE shall use this  value when receiving PDSCH scheduled by the same DCI

- is set to '1' and two values are configured for the first set of  values as 'n2-wideband' (corresponding to two  values 2 and wideband) or 'n4-wideband' (corresponding to two  values 4 and wideband), the UE shall use the value when receiving PDSCH scheduled by the same DCI as follows:

- If the scheduled PRBs are contiguous and the size of the scheduled PRBs is larger than ,  is the same as the scheduled bandwidth, otherwise  is set to the remaining configured value of 2 or 4, respectively.

When receiving PDSCH scheduled by PDCCH with DCI format 1\_1 with CRC scrambled by C-RNTI, MCS-C-RNTI, or CS-RNTI, if the higher layer parameter *prb-BundlingType* is set to 'staticBundling', the  value is configured with the single value indicated by the higher layer parameter *bundleSize*.

When a UE is configured with nominal RBG size for bandwidth part *i* according to Clause 5.1.2.2.1, or when a UE is configured with interleaving unit of 2 for VRB to PRB mapping provided by the higher layer parameter *vrb-ToPRB-Interleaver* given by *PDSCH-Config* for bandwidth part *i*, the UE is not expected to be configured with = 4.

For a UE configured by the higher layer parameter *RepSchemeEnabler* set to ‘*FDMSchemeA’ or* ‘*FDMSchemeB’, and* when the UE is indicated with two TCI states in a codepoint of the DCI field *'Transmission Configuration Indication* and DM-RS port(s) within one CDM group in the DCI field “*Antenna Port(s)*”,

- If  is determined as "wideband", the first PRBs are assigned to the first TCI state and the remaining PRBs are assigned to the second TCI state, where is the total number of allocated PRBs for the UE.

- If  is determined as one of the values among {2, 4}, even PRGs within the allocated frequency domain resources are assigned to the first TCI state and odd PRGs within the allocated frequency domain resources are assigned to the second TCI state.

- The UE is not expected to receive more than two PDSCH transmission layers for each PDSCH transmission occasion.

For a UE configured by the higher layer parameter *RepSchemeEnabler* set to ‘*FDMSchemeB’,* andwhen the UE is indicated with two TCI states in a codepoint of the DCI field *'Transmission Configuration Indication* and DM-RS port(s) within one CDM group in the DCI field “*Antenna Port(s)”,* each PDSCH transmission occasion shall follow the Clause 7.3.1 of [4, TS 38.211] with themapping to resource elements determined by the assigned PRBs for corresponding TCI state of the PDSCH transmission occasion, and the UE shall only expect at most two code blocks per PDSCH transmission occasion when a single transmission layer is scheduled and a single code block per PDSCH transmission occasion when two transmission layers are scheduled. For two PDSCH transmission occasions, the redundancy version to be applied is derived according to Table 5.1.2.1-2, where are applied to the first and second TCI state, respectively.

### 5.1.3 Modulation order, target code rate, redundancy version and transport block size determination

To determine the modulation order, target code rate, and transport block size(s) in the physical downlink shared channel, the UE shall first

- read the 5-bit modulation and coding scheme field (*IMCS*) in the DCI to determine the modulation order (*Qm*) and target code rate (*R*) based on the procedure defined in Clause 5.1.3.1, and

- read *redundancy version* field (*rv*) in the DCI to determine the redundancy version.

and second

- the UE shall use the number of layers (ʋ), the total number of allocated PRBs before rate matching (*nPRB*) to determine to the transport block size based on the procedure defined in Clause 5.1.3.2.

The UE may skip decoding a transport block in an initial transmission if the effective channel code rate is higher than 0.95, where the effective channel code rate is defined as the number of downlink information bits (including CRC bits) divided by the number of physical channel bits on PDSCH.

The UE is not expected to handle any transport blocks (TBs) in a 14 consecutive-symbol duration for normal CP (or 12 for extended CP) ending at the last symbol of the latest PDSCH transmission within an active BWP on a serving cell whenever

where, for the serving cell,

- S is the set of TBs belonging to PDSCH(s) that are partially or fully contained in the consecutive-symbol duration

- for the *i*th TB

*- Ci'* is the number of scheduled code blocks for as defined in [5, 38.212].

*- Li* is the number of OFDM symbols assigned to the PDSCH

*- xi* is the number of OFDM symbols of the PDSCH contained in the consecutive-symbol duration

- based on the values defined in Clause 5.4.2.1 [5, TS 38.212]

- is the starting location of RV for the th transmission

- of the scheduled code blocks for the transmission

- is the circular buffer length

- is the current (re)transmission for the *i*th TB

- corresponds to the subcarrier spacing of the BWP (across all configured BWPs of a carrier) that has the largest configured number of PRBs

- in case there is more than one BWP corresponding to the largest configured number of PRBs, *µ'* follows the BWP with the largest subcarrier spacing.

- corresponds to the subcarrier spacing of the active BWP

- RLBRM = 2/3 as defined in Clause 5.4.2.1 [5, TS 38.212]

- TBSLBRM as defined in Clause 5.4.2.1 [5, TS 38.212]

- X as defined for downlink in Clause 5.4.2.1 [5, TS 38.212].

If the UE skips decoding, the physical layer indicates to higher layer that the transport block is not successfully decoded.

Within a cell group, a UE is not required to handle PDSCH(s) transmissions in slot *sj* in serving cell-*j*, and for *j* = 0,1,2.. *J-1*, slot *sj* overlapping with any given point in time, if the following condition is not satisfied at that point in time:

where,

- *J* is the number of configured serving cells belonging to a frequency range

- for the *j-th* serving cell,

*- M* is the number of TB(s) transmitted in slot *sj*.

*- Tslotμ(j)* =10-3/2*μ(j)*, where *μ(j)* is the numerology for PDSCH(s) in slot *sj* of the *j*-th serving cell.

- for the *m*-th TB,

*- A* is the number of bits in the transport block as defined in Clause 7.2.1 [5, TS 38.212]

*- C* is the total number of code blocks for the transport block defined in Clause 5.2.2 [5, TS 38.212].

*-*  is the number of scheduled code blocks for the transport block as defined in Clause 5.4.2.1 [5, TS 38.212]

- [Mbps] is computed as the maximum data rate summed over all the carriers in the frequency range for any signaled band combination and feature set consistent with the configured servings cells, where the data rate value is given by the formula in Clause 4.1.2 in [13, TS 38.306], including the scaling factor *f(i).*

For a *j-*th serving cell, if higher layer parameter *processingType2Enabled* of *PDSCH-ServingCellConfig* is configured for the serving cell and set to *enable,* or if at least one *IMCS >* *W* for a PDSCH, where *W* = 28 for MCS tables 5.1.3.1-1 and 5.1.3.1-3, and *W* = 27 for MCS table 5.1.3.1-2, the UE is not required to handle PDSCH transmissions, if the following condition is not satisfied:

where

- is the number of symbols assigned to the PDSCH

- M is the number of TB(s) in the PDSCH

- where *μ* is the numerology of the PDSCH

- for the *m*-th TB,

*- A* is the number of bits in the transport block as defined in Clause 7.2.1 [5, TS 38.212]

*- C* is the total number of code blocks for the transport block defined in Clause 5.2.2 [5, TS 38.212]

*-*  is the number of scheduled code blocks for the transport block as defined in Clause 5.4.2.1 [5, TS 38.212]

- [Mbps] is computed as the maximum data rate for a carrier in the frequency band of the serving cell for any signaled band combination and feature set consistent with the serving cell, where the data rate value is given by the formula in Clause 4.1.2 in [13, TS 38.306], including the scaling factor *f(i).*

#### 5.1.3.1 Modulation order and target code rate determination

For the PDSCH scheduled by a PDCCH with DCI format 1\_0, format 1\_1 or format 1\_2 with CRC scrambled by C-RNTI, MCS-C-RNTI, TC-RNTI, CS-RNTI, SI-RNTI, RA-RNTI, MsgB-RNTI, or P-RNTI, or for the PDSCH scheduled without corresponding PDCCH transmissions using the higher-layer-provided PDSCH configuration *SPS-Config*,

if the higher layer parameter *mcs-Table-ForDCIFormat1\_2* given by *PDSCH-Config* is set to 'qam256', and the PDSCH is scheduled by a PDCCH with DCI format 1\_2 with CRC scrambled by C-RNTI

- the UE shall use *IMCS* and Table 5.1.3.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical downlink shared channel.

elseif the UE is not configured with MCS-C-RNTI, the higher layer parameter *mcs-Table-ForDCIFormat1\_2* given by *PDSCH-Config* is set to 'qam64LowSE', and the PDSCH is scheduled by a PDCCH with DCI format 1\_2 scrambled by C-RNTI

- the UE shall use *IMCS* and Table 5.1.3.1-3 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical downlink shared channel.

elseif the higher layer parameter *mcs-Table* given by *PDSCH-Config* is set to 'qam256', and the PDSCH is scheduled by a PDCCH with DCI format 1\_1 with CRC scrambled by C-RNTI

- the UE shall use *IMCS* and Table 5.1.3.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical downlink shared channel.

elseif the UE is not configured with MCS-C-RNTI, the higher layer parameter *mcs-Table* given by *PDSCH-Config* is set to 'qam64LowSE', and the PDSCH is scheduled by a PDCCH with a DCI format other than DCI format 1\_2 in a UE-specific search space with CRC scrambled by C-RNTI

- the UE shall use *IMCS* and Table 5.1.3.1-3 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical downlink shared channel.

elseif the UE is configured with MCS-C-RNTI, and the PDSCH is scheduled by a PDCCH with CRC scrambled by MCS-C-RNTI

- the UE shall use *IMCS* and Table 5.1.3.1-3 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical downlink shared channel.

elseif the UE is not configured with the higher layer parameter *mcs-Table* given by *SPS-config*, the higher layer parameter *mcs-Table-ForDCIFormat1\_2* given by *PDSCH-Config* is set to 'qam256', and the PDSCH is scheduled by a PDCCH with DCI format 1\_2 with CRC scrambled by CS-RNTI

- the UE shall use *IMCS* and Table 5.1.3.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical downlink shared channel.

elseif the UE is not configured with the higher layer parameter *mcs-Table* given by *SPS-Config*, the higher layer parameter *mcs-Table* given by *PDSCH-Config* is set to 'qam256',

- if the PDSCH is scheduled by a PDCCH with DCI format 1\_1 with CRC scrambled by CS-RNTI or

- if the PDSCH is scheduled without corresponding PDCCH transmission using *SPS-Config*,

- the UE shall use *IMCS* and Table 5.1.3.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical downlink shared channel.

elseif the UE is configured with the higher layer parameter *mcs-Table* given by *SPS-Config* set to 'qam64LowSE'

- if the PDSCH is scheduled by a PDCCH with CRC scrambled by CS-RNTI or

- if the PDSCH is scheduled without corresponding PDCCH transmission using *SPS-Config*,

- the UE shall use *IMCS* and Table 5.1.3.1-3 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical downlink shared channel.

else

- the UE shall use *IMCS* and Table 5.1.3.1-1 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical downlink shared channel.

end

The UE is not expected to decode a PDSCH scheduled with P-RNTI, RA-RNTI, SI-RNTI and *Qm* > 2

For a UE configured with *FDMSchemeB*, and when the UE is indicated with two TCI states in a codepoint of the DCI field *'Transmission Configuration Indication* and DM-RS port(s) within one CDM group in the DCI field “*Antenna Port(s)*”, the determined modulation order of PDSCH transmission occasion associated with the first TCI state is applied to the PDSCH transmission occasion associated with the second TCI state.

Table 5.1.3.1-1: MCS index table 1 for PDSCH

|  |  |  |  |
| --- | --- | --- | --- |
| MCS Index *IMCS* | Modulation Order  *Qm* | Target code Rate *R* x [1024] | Spectral  efficiency |
| **0** | 2 | 120 | 0.2344 |
| **1** | 2 | 157 | 0.3066 |
| **2** | 2 | 193 | 0.3770 |
| **3** | 2 | 251 | 0.4902 |
| **4** | 2 | 308 | 0.6016 |
| **5** | 2 | 379 | 0.7402 |
| **6** | 2 | 449 | 0.8770 |
| **7** | 2 | 526 | 1.0273 |
| **8** | 2 | 602 | 1.1758 |
| **9** | 2 | 679 | 1.3262 |
| **10** | 4 | 340 | 1.3281 |
| **11** | 4 | 378 | 1.4766 |
| **12** | 4 | 434 | 1.6953 |
| **13** | 4 | 490 | 1.9141 |
| **14** | 4 | 553 | 2.1602 |
| **15** | 4 | 616 | 2.4063 |
| **16** | 4 | 658 | 2.5703 |
| **17** | 6 | 438 | 2.5664 |
| **18** | 6 | 466 | 2.7305 |
| **19** | 6 | 517 | 3.0293 |
| **20** | 6 | 567 | 3.3223 |
| **21** | 6 | 616 | 3.6094 |
| **22** | 6 | 666 | 3.9023 |
| **23** | 6 | 719 | 4.2129 |
| **24** | 6 | 772 | 4.5234 |
| **25** | 6 | 822 | 4.8164 |
| **26** | 6 | 873 | 5.1152 |
| **27** | 6 | 910 | 5.3320 |
| **28** | 6 | 948 | 5.5547 |
| **29** | 2 | reserved | |
| **30** | 4 | reserved | |
| **31** | 6 | reserved | |

Table 5.1.3.1-2: MCS index table 2 for PDSCH

|  |  |  |  |
| --- | --- | --- | --- |
| MCS Index *IMCS* | Modulation Order  *Qm* | Target code Rate *R* x [1024] | Spectral  efficiency |
| **0** | 2 | 120 | 0.2344 |
| **1** | 2 | 193 | 0.3770 |
| **2** | 2 | 308 | 0.6016 |
| **3** | 2 | 449 | 0.8770 |
| **4** | 2 | 602 | 1.1758 |
| **5** | 4 | 378 | 1.4766 |
| **6** | 4 | 434 | 1.6953 |
| **7** | 4 | 490 | 1.9141 |
| **8** | 4 | 553 | 2.1602 |
| **9** | 4 | 616 | 2.4063 |
| **10** | 4 | 658 | 2.5703 |
| **11** | 6 | 466 | 2.7305 |
| **12** | 6 | 517 | 3.0293 |
| **13** | 6 | 567 | 3.3223 |
| **14** | 6 | 616 | 3.6094 |
| **15** | 6 | 666 | 3.9023 |
| **16** | 6 | 719 | 4.2129 |
| **17** | 6 | 772 | 4.5234 |
| **18** | 6 | 822 | 4.8164 |
| **19** | 6 | 873 | 5.1152 |
| **20** | 8 | 682.5 | 5.3320 |
| **21** | 8 | 711 | 5.5547 |
| **22** | 8 | 754 | 5.8906 |
| **23** | 8 | 797 | 6.2266 |
| **24** | 8 | 841 | 6.5703 |
| **25** | 8 | 885 | 6.9141 |
| **26** | 8 | 916.5 | 7.1602 |
| **27** | 8 | 948 | 7.4063 |
| **28** | 2 | reserved | |
| **29** | 4 | reserved | |
| **30** | 6 | reserved | |
| **31** | 8 | reserved | |

Table 5.1.3.1-3: MCS index table 3 for PDSCH

|  |  |  |  |
| --- | --- | --- | --- |
| MCS Index *IMCS* | Modulation Order  *Qm* | Target code Rate *R* x [1024] | Spectral  efficiency |
| **0** | 2 | 30 | 0.0586 |
| **1** | 2 | 40 | 0.0781 |
| **2** | 2 | 50 | 0.0977 |
| **3** | 2 | 64 | 0.1250 |
| **4** | 2 | 78 | 0.1523 |
| **5** | 2 | 99 | 0.1934 |
| **6** | 2 | 120 | 0.2344 |
| **7** | 2 | 157 | 0.3066 |
| **8** | 2 | 193 | 0.3770 |
| **9** | 2 | 251 | 0.4902 |
| **10** | 2 | 308 | 0.6016 |
| **11** | 2 | 379 | 0.7402 |
| **12** | 2 | 449 | 0.8770 |
| **13** | 2 | 526 | 1.0273 |
| **14** | 2 | 602 | 1.1758 |
| **15** | 4 | 340 | 1.3281 |
| **16** | 4 | 378 | 1.4766 |
| **17** | 4 | 434 | 1.6953 |
| **18** | 4 | 490 | 1.9141 |
| **19** | 4 | 553 | 2.1602 |
| **20** | 4 | 616 | 2.4063 |
| **21** | 6 | 438 | 2.5664 |
| **22** | 6 | 466 | 2.7305 |
| **23** | 6 | 517 | 3.0293 |
| **24** | 6 | 567 | 3.3223 |
| **25** | 6 | 616 | 3.6094 |
| **26** | 6 | 666 | 3.9023 |
| **27** | 6 | 719 | 4.2129 |
| **28** | 6 | 772 | 4.5234 |
| **29** | 2 | reserved | |
| **30** | 4 | reserved | |
| **31** | 6 | reserved | |

#### 5.1.3.2 Transport block size determination

In case the higher layer parameter *maxNrofCodeWordsScheduledByDCI* indicates that two codeword transmission is enabled, then one of the two transport blocks is disabled by DCI format 1\_1 if *IMCS* = 26 and if *rvid* = 1 for the corresponding transport block. If both transport blocks are enabled, transport block 1 and 2 are mapped to codeword 0 and 1 respectively. If only one transport block is enabled, then the enabled transport block is always mapped to the first codeword.

For the PDSCH assigned by a PDCCH with DCI format 1\_0, format 1\_1 or format 1\_2 with CRC scrambled by C-RNTI, MCS-C-RNTI, TC-RNTI, CS-RNTI, or SI-RNTI, if Table 5.1.3.1-2 is used and *,* or a table other than Table 5.1.3.1-2 is usedand *,* the UE shall, except if the transport block is disabled in DCI format 1\_1, first determine the TBS as specified below:

1) The UE shall first determine the number of REs (*NRE*) within the slot.

- A UE first determines the number of REs allocated for PDSCH within a PRB () by , where is the number of subcarriers in a physical resource block,  is the number of symbols of the PDSCH allocation within the slot,  is the number of REs for DM-RS per PRB in the scheduled duration including the overhead of the DM-RS CDM groups without data, as indicated by DCI format 1\_1 or format 1\_2 or as described for format 1\_0 in Clause 5.1.6.2, and  is the overhead configured by higher layer parameter *xOverhead* in *PDSCH-ServingCellConfig*. If the *xOverhead* in *PDSCH-ServingCellconfig* is not configured (a value from 0, 6, 12, or 18), the  is set to 0. If the PDSCH is scheduled by PDCCH with a CRC scrambled by SI-RNTI, RA-RNTI, MsgB-RNTI or P-RNTI,  is assumed to be 0.

- A UE determines the total number of REs allocated for PDSCH () by , where *nPRB* is the total number of allocated PRBs for the UE.

2) Intermediate number of information bits (*Ninfo*) is obtained by .

If 

Use step 3 as the next step of the TBS determination

else

Use step 4 as the next step of the TBS determination

end if

3) When , TBS is determined as follows

- quantized intermediate number of information bits , where .

- use Table 5.1.3.2-1 find the closest TBS that is not less than .

Table 5.1.3.2-1: TBS for 

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Index | TBS | Index | TBS | Index | TBS | Index | TBS |
| 1 | 24 | 31 | 336 | 61 | 1288 | 91 | 3624 |
| 2 | 32 | 32 | 352 | 62 | 1320 | 92 | 3752 |
| 3 | 40 | 33 | 368 | 63 | 1352 | 93 | 3824 |
| 4 | 48 | 34 | 384 | 64 | 1416 |  |  |
| 5 | 56 | 35 | 408 | 65 | 1480 |  |  |
| 6 | 64 | 36 | 432 | 66 | 1544 |  |  |
| 7 | 72 | 37 | 456 | 67 | 1608 |  |  |
| 8 | 80 | 38 | 480 | 68 | 1672 |  |  |
| 9 | 88 | 39 | 504 | 69 | 1736 |  |  |
| 10 | 96 | 40 | 528 | 70 | 1800 |  |  |
| 11 | 104 | 41 | 552 | 71 | 1864 |  |  |
| 12 | 112 | 42 | 576 | 72 | 1928 |  |  |
| 13 | 120 | 43 | 608 | 73 | 2024 |  |  |
| 14 | 128 | 44 | 640 | 74 | 2088 |  |  |
| 15 | 136 | 45 | 672 | 75 | 2152 |  |  |
| 16 | 144 | 46 | 704 | 76 | 2216 |  |  |
| 17 | 152 | 47 | 736 | 77 | 2280 |  |  |
| 18 | 160 | 48 | 768 | 78 | 2408 |  |  |
| 19 | 168 | 49 | 808 | 79 | 2472 |  |  |
| 20 | 176 | 50 | 848 | 80 | 2536 |  |  |
| 21 | 184 | 51 | 888 | 81 | 2600 |  |  |
| 22 | 192 | 52 | 928 | 82 | 2664 |  |  |
| 23 | 208 | 53 | 984 | 83 | 2728 |  |  |
| 24 | 224 | 54 | 1032 | 84 | 2792 |  |  |
| 25 | 240 | 55 | 1064 | 85 | 2856 |  |  |
| 26 | 256 | 56 | 1128 | 86 | 2976 |  |  |
| 27 | 272 | 57 | 1160 | 87 | 3104 |  |  |
| 28 | 288 | 58 | 1192 | 88 | 3240 |  |  |
| 29 | 304 | 59 | 1224 | 89 | 3368 |  |  |
| 30 | 320 | 60 | 1256 | 90 | 3496 |  |  |

4) When , TBS is determined as follows.

- quantized intermediate number of information bits , where and ties in the round function are broken towards the next largest integer.

- if 

, where 

else

if 

, where 

else



end if

end if

else if Table 5.1.3.1-2 is used and *,*

- the TBS is assumed to be as determined from the DCI transported in the latest PDCCH for the same transport block using . If there is no PDCCH for the same transport block using , and if the initial PDSCH for the same transport block is semi-persistently scheduled, the TBS shall be determined from the most recent semi-persistent scheduling assignment PDCCH.

else

- the TBS is assumed to be as determined from the DCI transported in the latest PDCCH for the same transport block using . If there is no PDCCH for the same transport block using, and if the initial PDSCH for the same transport block is semi-persistently scheduled, the TBS shall be determined from the most recent semi-persistent scheduling assignment PDCCH.

The UE is not expected to receive a PDSCH assigned by a PDCCH with CRC scrambled by SI-RNTI with a TBS exceeding 2976 bits.

For a UE configured with *FDMSchemeB* and indicated with two TCI states in a codepoint of the DCI field *'Transmission Configuration Indication* and DM-RS port(s) within one CDM group in the DCI field “*Antenna Port(s)*”, the TBS determination follows the steps 1-4 with the following modification in step 1: a UE determines the total number of REs allocated for PDSCH () by , where *nPRB* is the total number of allocated PRBs corresponding to the first TCI state. and the determined TBS of PDSCH transmission occasion associated with the first TCI state is also applied to the PDSCH transmission occasion associated with the second TCI state.

For the PDSCH assigned by a PDCCH with DCI format 1\_0 with CRC scrambled by P-RNTI, or RA-RNTI, MsgB-RNTI, TBS determination follows the steps 1-4 with the following modification in step 2: a scaling  is applied in the calculation of *Ninfo*, where the scaling factor is determined based on the *TB scaling* field in the DCI as in Table 5.1.3.2-2.

Table 5.1.3.2-2: Scaling factor of *Ninfo* for P-RNTI and RA-RNTI

|  |  |
| --- | --- |
| TB scaling field | Scaling factor S |
| 00 | 1 |
| 01 | 0.5 |
| 10 | 0.25 |
| 11 |  |

The NDI and HARQ process ID, as signalled on PDCCH, and the TBS, as determined above, shall be reported to higher layers.

### 5.1.4 PDSCH resource mapping

When receiving the PDSCH scheduled with SI-RNTI and the system information indicator in DCI is set to 0, the UE shall assume that no SS/PBCH block is transmitted in REs used by the UE for a reception of the PDSCH.

When receiving the PDSCH scheduled with SI-RNTI and the system information indicator in DCI is set to 1, RA-RNTI, MsgB-RNTI, P-RNTI or TC-RNTI, the UE assumes SS/PBCH block transmission according to *ssb-PositionsInBurst*, and if the PDSCH resource allocation overlaps with PRBs containing SS/PBCH block transmission resources the UE shall assume that the PRBs containing SS/PBCH block transmission resources are not available for PDSCH in the OFDM symbols where SS/PBCH block is transmitted.

A UE expects a configuration provided by *ssb-PositionsInBurst* in *ServingCellConfigCommon* to be same as a configuration provided by *ssb-PositionsInBurst* in *SIB1*.

When receiving PDSCH scheduled by PDCCH with CRC scrambled by C-RNTI, MCS-C-RNTI, CS-RNTI, or PDSCHs with SPS, the REs corresponding to the configured or dynamically indicated resources in Clauses 5.1.4.1, 5.1.4.2 are not available for PDSCH. Furthermore, the UE assumes SS/PBCH block transmission according to *ssb-PositionsInBurst* if the PDSCH resource allocation overlaps with PRBs containing SS/PBCH block transmission resources, the UE shall assume that the PRBs containing SS/PBCH block transmission resources are not available for PDSCH in the OFDM symbols where SS/PBCH block is transmitted.

A UE is not expected to handle the case where PDSCH DM-RS REs are overlapping, even partially, with any RE(s) not available for PDSCH*.*

#### 5.1.4.1 PDSCH resource mapping with RB symbol level granularity

The procedures for PDSCH scheduled by PDCCH with DCI format 1\_1 described in this clause equally apply to PDSCH scheduled by PDCCH with DCI format 1\_2, by applying the parameters of *rateMatchPatternGroup1-ForDCIFormat1\_*2, *rateMatchPatternGroup2-ForDCIFormat1\_2* instead of *rateMatchPatternGroup1* and *rateMatchPatternGroup2*.

A UE may be configured with any of the following higher layer parameters indicating REs declared as not available for PDSCH:

- *rateMatchPatternToAddModList* given by *PDSCH-Config,* by *ServingCellConfig* or by *ServingCellConfigCommon* and configuring up to 4 *RateMatchPattern(s)* per BWP and up to 4 *RateMatchPattern(s)* per serving-cell. A *RateMatchPattern* may contain:

- within a BWP, when provided by *PDSCH-Config* or within a serving cell when provided by *ServingCellConfig* or *ServingCellConfigCommon*, a pair of reserved resources with numerology provided by higher layer parameter *subcarrierSpacing* given by *RateMatchPattern* when configured per serving cellor by numerology of associated BWP when configured per BWP.The pair of reserved resources are respectively indicated by an RB level bitmap (higher layer parameter *resourceBlocks* given by *RateMatchPattern* ) with 1RB granularity and a symbol level bitmap spanning one or two slots (higher layer parameters *symbolsInResourceBlock* given by *RateMatchPattern* ) for which the reserved RBs apply. A bit value equal to 1 in the RB and symbol level bitmaps indicates that the corresponding resource is not available for PDSCH. For each pair of RB and symbol level bitmaps, a UE may be configured with a time-domain pattern (higher layer parameter *periodicityAndPattern* given by *RateMatchPattern* ), where each bit of *periodicityAndPattern* corresponds to a unit equal to a duration of the symbol level bitmap, and a bit value equal to 1 indicates that the pair is present in the unit. The *periodicityAndPattern* can be {1, 2, 4, 5, 8, 10, 20 or 40} units long, but maximum of 40ms. The first symbol of *periodicityAndPattern* every 40ms/P periods is a first symbol in frame mod 4 = 0, where P is the duration of *periodicityAndPattern* in units of ms. When *periodicityAndPattern* is not configured for a pair, for a symbol level bitmap spanning two slots, the bits of the first and second slots correspond respectively to even and odd slots of a radio frame, and for a symbol level bitmap spanning one slot, the bits of the slot correspond to every slot of a radio frame. The pair can be included in one or two groups of resource sets (higher layer parameters *rateMatchPatternGroup1*and *rateMatchPatternGroup2*). The *rateMatchPatternToAddModList* given by *ServingCellConfig* or *ServingCellConfigCommon* configuration in numerology *µ* applies only to PDSCH of the same numerology *µ*.

- within a BWP, a frequency domain resource of a CORESET configured by *ControlResourceSet* with *controlResourceSetId* or *ControlResourceSetZero* and time domain resource determined by the higher layer parameters *monitoringSlotPeriodicityAndOffset,* *duration* and *monitoringSymbolsWithinSlot* of all search-space-sets configured by *SearchSpace* and time domain resource of search-space-set zero configured by *searchSpaceZero* associated with the CORESET as well as CORESET duration configured by *ControlResourceSet* with *controlResourceSetId* or *ControlResourceSetZero.* This resource not available for PDSCH can be included in one or two groups of resource sets (higher layer parameters *rateMatchPatternGroup1* and *rateMatchPatternGroup2*).

A configured group *rateMatchPatternGroup1* or *rateMatchPatternGroup2* contains alist of RB and symbol level resource set indices forming a union of resource-sets not available for PDSCH dynamically if a corresponding bit of the Rate matching indicator field of DCI format 1\_1 scheduling the PDSCH is equal to 1. The REs corresponding to the union of configured RB-symbol level resource-sets that are not included in either of the two groups are not available for PDSCH scheduled by DCI format 1\_1. When receiving PDSCH scheduled by DCI format 1\_0 or PDSCHs with SPS activated by DCI format 1\_0, the REs corresponding to configured resources in *rateMatchPatternGroup1* or *rateMatchPatternGroup2* are not available for PDSCH.

For a bitmap pair included in one or two groups of resource sets, the dynamic indication of availability for PDSCH applies to a set of slot(s) where the *rateMatchPatternToAddModList* is present among the slots of scheduled PDSCH.

If a UE monitors PDCCH candidates of aggregation levels 8 and 16 with the same starting CCE index in non-interleaved CORESET spanning one OFDM symbol and if a detected PDCCH scheduling the PDSCH has aggregation level 8, the resources corresponding to the aggregation level 16 PDCCH candidate are not available for the PDSCH.

If a PDSCH scheduled by a PDCCH would overlap with resources in the CORESET containing the PDCCH, the resources corresponding to a union of the detected PDCCH that scheduled the PDSCH and associated PDCCH DM-RS are not available for the PDSCH. When *precoderGranularity* configured in a CORESET where the PDCCH was detected is equal to *allContiguousRBs*, the associated PDCCH DM-RS are DM-RS in all REGs of the CORESET. Otherwise, the associated DM-RS are the DM-RS in REGs of the PDCCH.

#### 5.1.4.2 PDSCH resource mapping with RE level granularity

The procedures for PDSCH scheduled by PDCCH with DCI format 1\_1 described in this clause equally apply to PDSCH scheduled by PDCCH with DCI format 1\_2, by applying the parameters of *aperiodic-ZP-CSI-RS-ResourceSetsToAddModList-ForDCIFormat1\_2* instead of *aperiodic-ZP-CSI-RS-ResourceSetsToAddModList*.

A UE may be configured with any of the following higher layer parameters:

*-* REs indicated by the *RateMatchingPatternLTE-CRS* in *lte-CRS-ToMatchAround* in *ServingCellConfig* or *ServingCellConfigCommon* configuring common RS, in 15 kHz subcarrier spacing applicable only to 15 kHz subcarrier spacing PDSCH, of one LTE carrier in a serving cell are declared as not available for PDSCH.

*-* REs indicated by *RateMatchingPatternLTE-CRS* in *lte-CRS-PatternList-r16* in *ServingCellConfig* configuring common RS, in 15 kHz subcarrier spacing applicable only to 15 kHz subcarrier spacing PDSCH, of one LTE carrier in a serving cell are declared as not available for PDSCH.

- Each *RateMatchingPatternLTE-CRS* configuration contains *v-Shift* consisting of LTE-CRS-vshift(s), *nrofCRS-Ports* consisting of LTE-CRS antenna ports 1, 2 or 4 ports, *carrierFreqDL* representing the offset in units of 15 kHz subcarriers from (reference) point A to the LTE carrier centre subcarrier location, *carrierBandwidthDL* representing the LTE carrier bandwidth, and may also configure *mbsfn-SubframeConfigList* representing MBSFN subframe configuration. A UE determines the CRS position within the slot according to Clause 6.10.1.2 in [15, TS 36.211], where slot corresponds to LTE subframe.

- If the UE configured by higher layer parameter *PDCCH-Config* with two different values of *CORESETPoolIndex* in *ControlResourceSet* and also configured by the higher layer parameter *LTE-CRS-PatternList-r16* in *ServingCellConfig*, the following REs are declared as not available for PDSCH:

- REs indicated by *CRSPatternList-CORESETPoolIndex* for a UE supporting the capability of [*separate-lte-CRS-ToMatchAround*];

- REs indicated by *CRS-PatternList-r16* in *ServingCellConfig* for a UE not supporting the capability of [*separate-lte-CRS-ToMatchAround*].

- Within a BWP, the UE can be configured with one or more ZP CSI-RS resource set configuration(s) for aperiodic, semi-persistent and periodic time-domain behaviours (higher layer parameters *aperiodic-ZP-CSI-RS-ResourceSetsToAddModList,*  *sp-ZP-CSI-RS-ResourceSetsToAddModList* and *p-ZP-CSI-RS-ResourceSet* respectively comprised in *PDSCH-Config*), with each ZP-CSI-RS resource set consisting of at most 16 ZP CSI-RS resources (higher layer parameter *ZP-CSI-RS-Resource*) in numerology of the BWP. The REs indicated by *p-ZP-CSI-RS-ResourceSet* are declared as not available for PDSCH. The REs indicated by *sp-ZP-CSI-RS-ResourceSetsToAddModList* and aperiodic-ZP-CSI-RS-ResourceSetsToAddModList are declared as not available for PDSCH when their triggering and activation are applied, respectively. The following parameters are configured via higher layer signaling for each ZP CSI-RS resource configuration:

- *zp-CSI-RS-ResourceId* in *ZP-CSI-RS-Resource* determines ZP CSI-RS resource configuration identity.

- *nrofPorts* defines the number of CSI-RS ports, where the allowable values are given in Clause 7.4.1.5 of [4, TS 38.211].

- *cdm-Type* defines CDM values and pattern, where the allowable values are given in Clause 7.4.1.5 of [4, TS 38.211].

- *resourceMapping* given by *ZP-CSI-RS-Resource* defines the OFDM symbol and subcarrier occupancy of the ZP-CSI-RS resource within a slot that are given in Clause 7.4.1.5 of [4, TS 38.211].

- *periodicityAndOffset* in*ZP-CSI-RS-Resource* defines the ZP-CSI-RS periodicity and slot offset for periodic/semi-persistent ZP-CSI-RS.

The UE may be configured with a DCI field for triggering the aperiodic ZP-CSI-RS. A list of *ZP-CSI-RS-ResourceSet(s)*, provided by higher layer parameter *aperiodic-ZP-CSI-RS-ResourceSetsToAddModList* in*PDSCH-Config* , is configured for aperiodic triggering. The maximum number of aperiodic *ZP-CSI-RS-ResourceSet(s)* configured per BWP is 3. The bit-length of DCI field *ZP CSI-RS trigger* depends on the number of aperiodic *ZP-CSI-RS-ResourceSet(s)*configured (up to 2 bits). Each non-zero codepoint of *ZP CSI-RS trigger* in DCI format 1\_1 triggers one aperiodic *ZP-CSI-RS-*ResourceSet in the list *aperiodic-ZP-CSI-RS-ResourceSetsToAddModList* by indicating the aperiodic ZP CSI-RS resource set ID. The DCI codepoint '01' triggers the resource set with ZP-CSI-RS-ResourceSetIds = 1, the DCI codepoint '10' triggers the resource set with ZP-CSI-RS-ResourceSetIds = 2, and the DCI codepoint '11' triggers the resource set with ZP-CSI-RS-ResourceSetIds = 3. Codepoint '00' is reserved for not triggering aperiodic ZP CSI-RS. When receiving PDSCH scheduled by DCI format 1\_0 or PDSCHs with SPS activated by DCI format 1\_0, the REs corresponding to configured resources in *aperiodic-ZP-CSI-RS-ResourceSetsToAddModList* are available for PDSCH.

When the UE is configured with multi-slot and single-slot PDSCH scheduling, the triggered aperiodic ZP CSI-RS is applied to all the slot(s) of the PDSCH scheduled by the PDCCH containing the trigger.

For a UE configured with a list of *ZP-CSI-RS-ResourceSet(s)* provided by higher layer parameter *sp-ZP-CSI-RS-ResourceSetsToAddModList*:

- when the UE would transmit a PUCCH with HARQ-ACK information in slot *n* corresponding to the PDSCH carrying the activation command, as described in clause 6.1.3.19 of [10, TS 38.321], for ZP CSI-RS resource(s), the corresponding action in [10, TS 38.321] and the UE assumption on the PDSCH RE mapping corresponding to the activated ZP CSI-RS resource(s) shall be applied starting from the first slot that is after slot where ** is the SCS configuration for the PUCCH.

- when the UE would transmit a PUCCH with HARQ-ACK information in slot *n* corresponding to the PDSCH carrying the deactivation command, as described in clause 6.1.3.19 of [10, TS 38.321], for activated ZP CSI-RS resource(s), the corresponding action in [10, TS 38.321] and the UE assumption on cessation of the PDSCH RE mapping corresponding to the de-activated ZP CSI-RS resource(s) shall be applied starting from the first slot that is after slot where ** is the SCS configuration for the PUCCH.

### 5.1.5 Antenna ports quasi co-location

The UE can be configured with a list of up to *M* *TCI-State* configurations within the higher layer parameter *PDSCH-Config* to decode PDSCH according to a detected PDCCH with DCI intended for the UE and the given serving cell, where M depends on the UE capability *maxNumberConfiguredTCIstatesPerCC*. Each *TCI-State* contains parameters for configuring a quasi co-location relationship between one or two downlink reference signals and the DM-RS ports of the PDSCH, the DM-RS port of PDCCH or the CSI-RS port(s) of a CSI-RS resource. The quasi co-location relationship is configured by the higher layer parameter *qcl-Type1* for the first DL RS, and *qcl-Type2* for the second DL RS(if configured). For the case of two DL RSs, the QCL types shall not be the same, regardless of whether the references are to the same DL RS or different DL RSs. The quasi co-location types corresponding to each DL RS are given by the higher layer parameter *qcl-Type* in *QCL-Info* and may take one of the following values:

- 'QCL-TypeA': {Doppler shift, Doppler spread, average delay, delay spread}

- 'QCL-TypeB': {Doppler shift, Doppler spread}

- 'QCL-TypeC': {Doppler shift, average delay}

- 'QCL-TypeD': {Spatial Rx parameter}

The UE receives an activation command, as described in clause 6.1.3.14 of [10, TS 38.321] or in clause [6.1.3.x] of [10, TS 38.321], used to map up to 8 TCI states to the codepoints of the DCI field *'Transmission Configuration Indication'* in one CC/DL BWP or in a set of CCs/DL BWPs, respectively. When a set of TCI state IDs are activated for a set of CCs/DL BWPs, where the applicable list of CCs is determined by indicated CC in the activation command, the same set of TCI state IDs are applied for all DL BWPs in the indicated CCs.

When a UE supports two TCI states in a codepoint of the DCI field ‘*Transmission Configuration Indication’* the UE may receive an activation command, as described in clause [6.1.3.X] of [10, TS 38.321], the activation command is used to map up to 8 combinations of one or two TCI states to the codepoints of the DCI field *'Transmission Configuration Indication'*. The UE is not expected to receive more than 8 TCI states in the activation command.

When the UE would transmit a PUCCH with HARQ-ACK information in slot *n* corresponding to the PDSCH carrying the activation command, the indicated mapping between TCI states and codepoints of the DCI field *'Transmission Configuration Indication'* should be applied starting from the first slot that is after slot where ** is the SCS configuration for the PUCCH. If *tci-PresentInDCI* is set to "enabled" or *tci-PresentInDCI-ForFormat1\_2* is configured for the CORESET scheduling the PDSCH, and the time offset between the reception of the DL DCI and the corresponding PDSCH is equal to or greater than *timeDurationForQCL* if applicable, after a UE receives an initial higher layer configuration of TCI states and before reception of the activation command, the UE may assume that the DM-RS ports of PDSCH of a serving cell are quasi co-located with the SS/PBCH block determined in the initial access procedure with respect to 'QCL-TypeA', and when applicable, also with respect to'QCL-TypeD'.

If a UE is configured with the higher layer parameter *tci-PresentInDCI* that is set as 'enabled'for the CORESET scheduling the PDSCH, the UE assumes that the TCI field is present in the DCI format 1\_1 of the PDCCH transmitted on the CORESET. If a UE is configured with the higher layer parameter *tci-PresentInDCI-ForFormat1\_2* for the CORESET scheduling the PDSCH, the UE assumes that the TCI field with a DCI field size indicated by *tci-PresentInDCI-ForFormat1\_2* is present in the DCI format 1\_2 of the PDCCH transmitted on the CORESET. If the PDSCH is scheduled by a DCI format not having the TCI field present, and the time offset between the reception of the DL DCI and the corresponding PDSCH is equal to or greater than a threshold *timeDurationForQCL* if applicable, where the threshold is based on reported UE capability [13, TS 38.306], for determining PDSCH antenna port quasi co-location, the UE assumes that the TCI state or the QCL assumption for the PDSCH is identical to the TCI state or QCL assumption whichever is applied for the CORESET used for the PDCCH transmission.

If the PDSCH is scheduled by a DCI format having the TCI field present, the TCI field in DCI in the scheduling component carrier points to the activated TCI states in the scheduled component carrier or DL BWP, the UE shall use the *TCI-State* according to the value of the '*Transmission Configuration Indication*' field in the detected PDCCH with DCI for determining PDSCH antenna port quasi co-location. The UE may assume that the DM-RS ports of PDSCH of a serving cell are quasi co-located with the RS(s) in the TCI state with respect to the QCL type parameter(s) given by the indicated TCI state if the time offset between the reception of the DL DCI and the corresponding PDSCH is equal to or greater than a threshold *timeDurationForQCL*, where the threshold is based on reported UE capability [13, TS 38.306]. When the UE is configured with a single slot PDSCH, the indicated TCI state should be based on the activated TCI states in the slot with the scheduled PDSCH. When the UE is configured with a multi-slot PDSCH, the indicated TCI state should be based on the activated TCI states in the first slot with the scheduled PDSCH, and UE shall expect the activated TCI states are the same across the slots with the scheduled PDSCH. When the UE is configured with CORESET associated with a search space set for cross-carrier scheduling, and the PDCCH carrying the scheduling DCI and the PDSCH scheduled by that DCI are transmitted on the same carrier, the UE expects *tci-PresentInDCI* is set as 'enabled' or *tci-PresentInDCI-ForFormat1\_2* is configured for the CORESET, and if one or more of the TCI states configured for the serving cell scheduled by the search space set contains 'QCL-TypeD', the UE expects the time offset between the reception of the detected PDCCH in the search space set and the corresponding PDSCH is larger than or equal to the threshold *timeDurationForQCL.*

Independent of the configuration of *tci-PresentInDCI* and *tci-PresentInDCI-ForFormat1\_2* in RRC connected mode, if all the TCI codepoints are mapped to a single TCI state and the offset between the reception of the DL DCI and the corresponding PDSCH is less than the threshold *timeDurationForQCL*, the UE may assume that the DM-RS ports of PDSCH of a serving cell are quasi co-located with the RS(s) with respect to the QCL parameter(s) used for PDCCH quasi co-location indication of the CORESET associated with a monitored search space with the lowest *controlResourceSetId* in the latest slot in which one or more CORESETs within the active BWP of the serving cell are monitored by the UE. In this case, if the 'QCL-TypeD' of the PDSCH DM-RS is different from that of the PDCCH DM-RS with which they overlap in at least one symbol, the UE is expected to prioritize the reception of PDCCH associated with that CORESET. This also applies to the intra-band CA case (when PDSCH and the CORESET are in different component carriers). If none of configured TCI states for the serving cell of scheduled PDSCH contains 'QCL-TypeD', the UE shall obtain the other QCL assumptions from the indicated TCI states for its scheduled PDSCH irrespective of the time offset between the reception of the DL DCI and the corresponding PDSCH. If a UE configured by higher layer parameter *PDCCH-Config* that contains two different values of *CORESETPoolIndex* in *ControlResourceSet,* for both cases,when *tci-PresentInDCI* is set to 'enabled' and *tci-PresentInDCI* is not configured in RRC connected mode, if the offset between the reception of the DL DCI and the corresponding PDSCH is less than the threshold *timeDurationForQCL,* the UE may assume that the DM-RS ports of PDSCH associated with a value of *CORESETPoolIndex* of a serving cell are quasi co-located with the RS(s) with respect to the QCL parameter(s) used for PDCCH quasi co-location indication of the CORESET associated with a monitored search space with the lowest *CORESET-ID* among CORESETs, which are configured with the same value of *CORESETPoolIndex* as the PDCCH scheduling that PDSCH, in the latest slot in which one or more CORESETs associated with the same value of *CORESETPoolIndex* as the PDCCH scheduling that PDSCH within the active BWP of the serving cell are monitored by the UE. If the offset between the reception of the DL DCI and the corresponding PDSCH is less than the threshold *timeDurationForQCL* and atleast one configured TCI states for the serving cell of scheduled PDSCH contains the'QCL-TypeD', and at least one TCI codepoint indicates two TCI states, the UE may assume that the DM-RS ports of PDSCH of a serving cell are quasi co-located with the RS(s) with respect to the QCL parameter(s) associated with the TCI states corresponding to the lowest codepoint among the TCI codepoints containing two different TCI states.

If the PDCCH carrying the scheduling DCI is received on one component carrier, and the PDSCH scheduled by that DCI is on another component carrier:

- The *timeDurationForQCL* is determined based on the subcarrier spacing of the scheduled PDSCH. If µPDCCH < µPDSCH an additional timing delay *d* is added to the *timeDurationForQCL*, where *d* is defined in 5.2.1.5.1a-1;

- For both the cases when *tci-PresentInDCI* is set to 'enabled' and the offset between the reception of the DL DCI and the corresponding PDSCH is less than the threshold *timeDurationForQCL* and when *tci-PresentInDCI* is not configured, the UE obtains its QCL assumption for the scheduled PDSCH from the activated TCI state with the lowest ID applicable to PDSCH in the active BWP of the scheduled cell.

For a periodic CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info*, the UE shall expect that a TCI-State indicates one of the following quasi co-location type(s):

- 'QCL-TypeC' with an SS/PBCH block and, when applicable, 'QCL-TypeD' with the same SS/PBCH block, or

- 'QCL-TypeC' with an SS/PBCH block and, when applicable,'QCL-TypeD' with a CSI-RS resource in an *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *repetition*, or

For an aperiodic CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info,* the UE shall expect that a *TCI-State* indicates 'QCL-TypeA' with a periodic CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* and, when applicable,'QCL-TypeD' with the same periodic CSI-RS resource.

For a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured without higher layer parameter *trs-Info* and without the higher layer parameter *repetition*, the UE shall expect that a *TCI-State* indicates one of the following quasi co-location type(s):

- 'QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* and, when applicable, 'QCL-TypeD' with the same CSI-RS resource, or

- 'QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* and, when applicable, 'QCL-TypeD' with an SS/PBCH block , or

- 'QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* and, when applicable, 'QCL-TypeD' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *repetition*, or

- 'QCL-TypeB' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* when 'QCL-TypeD' is not applicable.

For a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *repetition,* the UE shall expect that a *TCI-State* indicates one of the following quasi co-location type(s):

- 'QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* and, when applicable, 'QCL-TypeD' with the same CSI-RS resource, or

- 'QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* and, when applicable, 'QCL-TypeD' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *repetition*, or

- 'QCL-TypeC' with an SS/PBCH block and, when applicable, 'QCL-TypeD' with the same SS/PBCH block.

For the DM-RS of PDCCH, the UE shall expect that a *TCI-State* indicates one of the following quasi co-location type(s):

- 'QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* and, when applicable, 'QCL-TypeD' with the same CSI-RS resource, or

- 'QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* and, when applicable, 'QCL-TypeD' with a CSI-RS resource in an *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *repetition*, or

- 'QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured without higher layer parameter trs-Info and without higher layer parameter *repetition* and,when applicable, 'QCL-TypeD' with the same CSI-RS resource.

For the DM-RS of PDSCH, the UE shall expect that a *TCI-State* indicates one of the following quasi co-location type(s):

- 'QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* and, when applicable, 'QCL-TypeD' with the same CSI-RS resource*,* or

- 'QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info* and, when applicable, 'QCL-TypeD' with a CSI-RS resource in an *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *repetition*,or

- QCL-TypeA' with a CSI-RS resource in a *NZP-CSI-RS-ResourceSet* configured without higher layer parameter *trs-Info* and without higher layer parameter *repetition* and, when applicable, 'QCL-TypeD' with the same CSI-RS resource.

### 5.1.6 UE procedure for receiving reference signals

#### 5.1.6.1 CSI-RS reception procedure

The CSI-RS defined in Clause 7.4.1.5 of [4, TS 38.211], may be used for time/frequency tracking, CSI computation, L1-RSRP computation and mobility.

For a CSI-RS resource associated with a *NZP-CSI-RS-ResourceSet* with the higher layer parameter *repetition* set to 'on', the UE shall not expect to be configured with CSI-RS over the symbols during which the UE is also configured to monitor the CORESET, while for other *NZP-CSI-RS-ResourceSet* configurations, if the UE is configured with a CSI-RS resource and a search space set associated with a CORESET in the same OFDM symbol(s), the UE may assume that the CSI-RS and a PDCCH DM-RS transmitted in all the search space sets associated with CORESET are quasi co-located with 'QCL-TypeD', if 'QCL-TypeD' is applicable. This also applies to the case when CSI-RS and the CORESET are in different intra-band component carriers, if 'QCL-TypeD' is applicable. Furthermore, the UE shall not expect to be configured with the CSI-RS in PRBs that overlap those of the CORESET in the OFDM symbols occupied by the search space set(s).

The UE is not expected to receive CSI-RS and *SIB1* message in the overlapping PRBs in the OFDM symbols where *SIB1* is transmitted.

If the UE is configured with DRX, the most recent CSI measurement occasion occurs in DRX active time for CSI to be reported.

##### 5.1.6.1.1 CSI-RS for tracking

A UE in RRC connected mode is expected to receive the higher layer UE specific configuration of a *NZP-CSI-RS-ResourceSet* configured with higher layer parameter *trs-Info*.

For a *NZP-CSI-RS-ResourceSet* configured with the higher layer parameter *trs-Info*, the UE shall assume the antenna port with the same port index of the configured NZP CSI-RS resources in the *NZP-CSI-RS-ResourceSet* is the same.

- For frequency range 1, the UE may be configured with one or more NZP CSI-RS set(s), where a *NZP-CSI-RS-ResourceSet* consists of four periodic NZP CSI-RS resources in two consecutive slots with two periodic NZP CSI-RS resources in each slot. If no two consecutive slots are indicated as downlink slots by *tdd-UL-DL-ConfigurationCommon* or *tdd-UL-DL-ConfigDedicated*, then the UE may be configured with one or more NZP CSI-RS set(s), where a *NZP-CSI-RS-ResourceSet* consists of two periodic NZP CSI-RS resources in one slot.

- For frequency range 2 the UE may be configured with one or more NZP CSI-RS set(s), where a *NZP-CSI-RS-ResourceSet* consists of two periodic CSI-RS resources in one slot or with a *NZP-CSI-RS-ResourceSet* of four periodic NZP CSI-RS resources in two consecutive slots with two periodic NZP CSI-RS resources in each slot.

A UE configured with *NZP-CSI-RS-ResourceSet(s)* configured with higher layer parameter *trs-Info* may have the CSI-RS resources configured as:

- Periodic, with the CSI-RS resources in the *NZP-CSI-RS-ResourceSet* configured with same periodicity, bandwidth and subcarrier location

- Periodic CSI-RS resource in one set and aperiodic CSI-RS resources in a second set, with the aperiodic CSI-RS and periodic CSI-RS resource having the same bandwidth (with same RB location) and the aperiodic CSI-RS being 'QCL-Type-A' and 'QCL-TypeD', where applicable, with the periodic CSI-RS resources. For frequency range 2, the UE does not expect that the scheduling offset between the last symbol of the PDCCH carrying the triggering DCI and the first symbol of the aperiodic CSI-RS resources is smaller than the UE reported *ThresholdSched-Offset*. The UE shall expect that the periodic CSI-RS resource set and aperiodic CSI-RS resource set are configured with the same number of CSI-RS resources and with the same number of CSI-RS resources in a slot. For the aperiodic CSI-RS resource set if triggered, and if the associated periodic CSI-RS resource set is configured with four periodic CSI-RS resources with two consecutive slots with two periodic CSI-RS resources in each slot, the higher layer parameter *aperiodicTriggeringOffset* indicates the triggering offset for the first slot for the first two CSI-RS resources in the set.

A UE does not expect to be configured with a *CSI-ReportConfig* that is linked to a *CSI-ResourceConfig* containing an *NZP-CSI-RS-ResourceSet* configured with *trs-Info* and with the *CSI-ReportConfig* configured with the higher layer parameter *timeRestrictionForChannelMeasurements* set to 'configured'.

A UE does not expect to be configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to other than 'none' for aperiodic NZP CSI-RS resource set configured with *trs-Info.*

A UE does not expect to be configured with a *CSI-ReportConfig* for periodic NZP CSI-RS resource set configured with *trs-Info*.

A UE does not expect to be configured with a *NZP-CSI-RS-ResourceSet* configured both with *trs-Info* and *repetition*.

Each CSI-RS resource, defined in Clause 7.4.1.5.3 of [4, TS 38.211], is configured by the higher layer parameter *NZP-CSI-RS-Resource* with the following restrictions:

- the time-domain locations of the two CSI-RS resources in a slot, or of the four CSI-RS resources in two consecutive slots (which are the same across two consecutive slots), as defined by higher layer parameter *CSI-RS-resourceMapping*, is given by one of

- , , or for frequency range 1 and frequency range 2,

- , , , , ,  or  for frequency range 2.

- a single port CSI-RS resource with density  given by Table 7.4.1.5.3-1 from [4, TS 38.211] and higher layer parameter *density* configured by *CSI-RS-ResourceMapping.*

- the bandwidth of the CSI-RS resource, as given by the higher layer parameter *freqBand* configured by *CSI-RS-ResourceMapping*, is the minimum of 52 and resource blocks, or is equal to resource blocks. For operation with shared spectrum channel access, *freqBand* configured by *CSI-RS-ResourceMapping*, is the minimum of 48 and resource blocks, or is equal to resource blocks.

- the UE is not expected to be configured with the periodicity of  slots if the bandwidth of CSI-RS resource is larger than 52 resource blocks.

- the periodicity and slot offset for periodic NZP CSI-RS resources, as given by the higher layer parameter *periodicityAndOffset* configured b*y NZP-CSI-RS-Resource*, is one of slots where 10, 20, 40, or 80 and where µ is defined in Clause 4.3 of [4, TS 38.211].

- same *powerControlOffset* and *powerControlOffsetSS* given by*NZP-CSI-RS-Resource* value across all resources.

##### 5.1.6.1.2 CSI-RS for L1-RSRP and L1-SINR computation

If a UE is configured with a *NZP-CSI-RS-ResourceSet* configured with the higher layer parameter *repetition* set to 'on', the UE may assume that the CSI-RS resources, described in Clause 5.2.2.3.1, within the *NZP-CSI-RS-ResourceSet* are transmitted with the same downlink spatial domain transmission filter, where the CSI-RS resources in the *NZP-CSI-RS-ResourceSet* are transmitted in different OFDM symbols. If *repetition* is set to 'off', the UE shall not assume that the CSI-RS resources within the *NZP-CSI-RS-ResourceSet* are transmitted with the same downlink spatial domain transmission filter.

If the UE is configured with a *CSI-ReportConfig* with *reportQuantity* set to "cri-RSRP", "cri-SINR" or "none" and if the *CSI-ResourceConfig* for channel measurement (higher layer parameter *resourcesForChannelMeasurement*) contains a *NZP-CSI-RS-ResourceSet* that is configured with the higher layer parameter *repetition* and without the higher layer parameter *trs-Info*, the UE can only be configured with the same number (1 or 2) of ports with the higher layer parameter *nrofPorts* for all CSI-RS resources within the set. If the UE is configured with the CSI-RS resource in the same OFDM symbol(s) as an SS/PBCH block, the UE may assume that the CSI-RS and the SS/PBCH block are quasi co-located with 'QCL-TypeD' if 'QCL-TypeD' is applicable. Furthermore, the UE shall not expect to be configured with the CSI-RS in PRBs that overlap with those of the SS/PBCH block, and the UE shall expect that the same subcarrier spacing is used for both the CSI-RS and the SS/PBCH block.

##### 5.1.6.1.3 CSI-RS for mobility

If a UE is configured with the higher layer parameter *CSI-RS-Resource-Mobility* and the higher layer parameter *associatedSSB* is not configured, the UE shall perform measurements based on *CSI-RS-Resource-Mobility* and the UE may base the timing of the CSI-RS resource on the timing of the serving cell.

If a UE is configured with the higher layer parameters *CSI-RS-Resource-Mobility* and *associatedSSB*, the UE may base the timing of the CSI-RS resource on the timing of the cell given by the *cellId* of the CSI-RS resource configuration. Additionally, for a given CSI-RS resource, if the associated SS/PBCH block is configured but not detected by the UE, the UE is not required to monitor the corresponding CSI-RS resource. The higher layer parameter *isQuasiColocated* indicates whether the associated SS/PBCH block given by the *associatedSSB* and the CSI-RS resource(s) are quasi co-located with respect to ['QCL-TypeD'].

If a UE is configured with the higher layer parameter *CSI-RS-Resource-Mobility* and with periodicity greater than 10 ms in paired spectrum, the UE may assume the absolute value of the time difference between radio frame *i* between any two cells, listed in the configuration with the higher layer parameter *CSI-RS-CellMobility* and with same *refFreqCSI-RS*, is less than 153600 *Ts*.

If the UE is configured with DRX, the UE is not required to perform measurement of CSI-RS resources other than during the active time for measurements based on *CSI-RS-Resource-Mobility*. When the UE is configured to monitor DCI format 2\_6, the UE is not required to perform measurements other than during the active time and during the timer duration indicated by *drx-onDurationTimer* based on *CSI-RS-Resource-Mobility*.

If the UE is configured with DRX and DRX cycle in use is larger than 80 ms, the UE may not expect CSI-RS resources are available other than during the active time for measurements based on *CSI-RS-Resource-Mobility*. If the UE is configured with DRX and configured to monitor DCI format 2\_6 and DRX cycle in use is larger than 80ms, the UE may not expect that the CSI-RS resources are available other than during the active time and during the time duration indicated by *drx-onDurationTimer* for measurements based on *CSI-RS-Resource-Mobility.* Otherwise, the UE may assume CSI-RS are available for measurements based on *CSI-RS-Resource-Mobility*.

A UE configured with the higher layer parameters *CSI-RS-Resource-Mobility* may expect to be configured

- with no more than 96 CSI-RS resources per higher layer parameter *MeasObjectNR* when all CSI-RS resources configured by the same higher layer parameter *MeasObjectNR* have been configured with *associatedSSB*, or,

- with no more than 64 CSI-RS resources per higher layer parameter *MeasObjectNR* when all CSI-RS resources have been configured without *associatedSSB* or when only some of the CSI-RS resources have been configured with associatedSSB by the same higher layer parameter *MeasObjectNR*

- For frequency range 1 the *associatedSSB* is optionally present for each CSI-RS resource

- For frequency range 2 the *associatedSSB* is either present for all configured CSI-RS resources or not present for any configured CSI-RS resource per higher layer parameter *MeasObjectNR*.

For any CSI-RS resource configuration, the UE shall assume that the value for parameter *cdm-Type* is 'noCDM', and there is only one antenna port.

#### 5.1.6.2 DM-RS reception procedure

The DM-RS reception procedures for PDSCH scheduled by PDCCH with DCI format 1\_1 described in this section equally apply to PDSCH scheduled by PDCCH with DCI format 1\_2, by applying the parameters of *dmrs-DownlinkForPDSCH-MappingTypeA-ForDCIFormat1\_2* and *dmrs-DownlinkForPDSCH-MappingTypeB-ForDCIFormat1\_2* instead of *dmrs-DownlinkForPDSCH-MappingTypeA* and *dmrs-DownlinkForPDSCH-MappingTypeB*.

When receiving PDSCH scheduled by DCI format 1\_0 or receiving PDSCH before dedicated higher layer configuration of any of the parameters *dmrs-AdditionalPosition*, *maxLength* and *dmrs-Type,* the UE shall assume that the PDSCH is not present in any symbol carrying DM-RS except for PDSCH with allocation duration of 2 symbols with PDSCH mapping type B (described in clause 7.4.1.1.2 of [4, TS 38.211]), and a single symbol front-loaded DM-RS of configuration type 1 on DM-RS port 1000 is transmitted, and that all the remaining orthogonal antenna ports are not associated with transmission of PDSCH to another UE and in addition

- For PDSCH with mapping type A, the UE shall assume *dmrs-AdditionalPosition*='pos2' and up to two additional single-symbol DM-RS present in a slot according to the PDSCH duration indicated in the DCI as defined in Clause 7.4.1.1 of [4, TS 38.211], and

- For PDSCH with allocation duration of 7 symbols for normal CP or 6 symbols for extended CP with mapping type B, the UE shall assume one additional single-symbol DM-RS present in the 5th or 6th symbol when the front-loaded DM-RS symbol is in the 1st or 2nd symbol respectively of the PDSCH allocation duration, otherwise the UE shall assume that the additional DM-RS symbol is not present, and

- For PDSCH with allocation duration of 4 symbols with mapping type B, the UE shall assume that no additional DM-RS are present, and

- For PDSCH with allocation duration of 2 symbols with mapping type B, the UE shall assume that no additional DM-RS are present, and the UE shall assume that the PDSCH is present in the symbol carrying DM-RS.

When receiving PDSCH scheduled by DCI format 1\_1 by PDCCH with CRC scrambled by C-RNTI, MCS-C-RNTI, or CS-RNTI,

- the UE may be configured with the higher layer parameter *dmrs-Type*, and the configured DM-RS configuration type is used for receiving PDSCH in as defined in Clause 7.4.1.1 of [4, TS 38.211].

- the UE may be configured with the maximum number of front-loaded DM-RS symbols for PDSCH by higher layer parameter *maxLength* given by *DMRS-DownlinkConfig..*

- if *maxLength* is set to 'len1', single-symbol DM-RS can be scheduled for the UE by DCI, and the UE can be configured with a number of additional DM-RS for PDSCH by higher layer parameter *dmrs-AdditionalPosition,* which can be set to 'pos0', 'pos1', 'pos2' or 'pos3'.

- if *maxLength* is set to 'len2', both single-symbol DM-RS and double symbol DM-RS can be scheduled for the UE by DCI, and the UE can be configured with a number of additional DM-RS for PDSCH by higher layer parameter *dmrs-AdditionalPosition,* which can be set to 'pos0' or 'pos1'.

- and the UE shall assume to receive additional DM-RS as specified in Table 7.4.1.1.2-3 and Table 7.4.1.1.2-4 as described in Clause 7.4.1.1.2 of [4, TS 38.211].

For the UE-specific reference signals generation as defined in Clause 7.4.1.1 of [4, TS 38.211], a UE can be configured by higher layers with one or two scrambling identity(s), *i* = 0,1 which are the same for both PDSCH mapping Type A and Type B.

A UE may be scheduled with a number of DM-RS ports by the antenna port index in DCI format 1\_1 as described in Clause 7.3.1.2 of [5, TS 38.212].

For DM-RS configuration type 1,

- if a UE is scheduled with one codeword and assigned with the antenna port mapping with indices of {2, 9, 10, 11 or 30} in Table 7.3.1.2.2-1 and Table 7.3.1.2.2-2 of Clause 7.3.1.2 of [5, TS 38.212], or

- if a UE is scheduled with two codewords,

the UE may assume that all the remaining orthogonal antenna ports are not associated with transmission of PDSCH to another UE.

For DM-RS configuration type 2,

- if a UE is scheduled with one codeword and assigned with the antenna port mapping with indices of {2, 10 or 23} in Table 7.3.1.2.2-3 and Table 7.3.1.2.2-4 of Clause 7.3.1.2 of [5, TS38.212], or

- if a UE is scheduled with two codewords,

the UE may assume that all the remaining orthogonal antenna ports are not associated with transmission of PDSCH to another UE.

If a UE receiving PDSCH is configured with the higher layer parameter *phaseTrackingRS* in *DMRS-DownlinkConfig*, the UE may assume that the following configurations are not occurring simultaneously for the received PDSCH:

- any DM-RS ports among 1004-1007 or 1006-1011 for DM-RS configurations type 1 and type 2, respectively are scheduled for the UE and the other UE(s) sharing the DM-RS REs on the same CDM group(s), and

- PT-RS is transmitted to the UE.

The UE is not expected to simultaneously be configured with the maximum number of front-loaded DM-RS symbols for PDSCH by higher layer parameter *maxLength* being set equal to 'len2' and more than one additional DM-RS symbol as given by the higher layer parameter *dmrs-AdditionalPosition*.

The UE is not expected to assume co-scheduled UE(s) with different DM-RS configuration with respect to the actual number of front-loaded DM-RS symbol(s), the actual number of additional DM-RS, the DM-RS symbol location, and DM-RS configuration type as described in Clause 7.4.1.1 of [4, TS 38.211].

The UE does not expect the precoding of the potential co-scheduled UE(s) in other DM-RS ports of the same CDM group to be different in the PRG-level grid configured to this UE with PRG =2 or 4.

The UE does not expect the resource allocation of the potential co-scheduled UE(s) in other DM-RS ports of the same CDM group to be misaligned in the PRG-level grid to this UE with PRG=2 or 4.

When receiving PDSCH scheduled by DCI format 1\_1, the UE shall assume that the CDM groups indicated in the configured index from Tables 7.3.1.2.2-1, 7.3.1.2.2-2, 7.3.1.2.2-3, 7.3.1.2.2-4 of [5, TS. 38.212] contain potential co-scheduled downlink DM-RS and are not used for data transmission, where "1", "2" and "3" for the number of DM-RS CDM group(s) in Tables 7.3.1.2.2-1, 7.3.1.2.2-2, 7.3.1.2.2-3, 7.3.1.2.2-4 of [5, TS. 38.212] correspond to CDM group 0, {0,1}, {0,1,2}, respectively.

When receiving PDSCH scheduled by DCI format 1\_0, the UE shall assume the number of DM-RS CDM groups without data is 1 which corresponds to CDM group 0 for the case of PDSCH with allocation duration of 2 symbols, and the UE shall assume that the number of DM-RS CDM groups without data is 2 which corresponds to CDM group {0,1} for all other cases.

The UE is not expected to receive PDSCH scheduling DCI which indicates CDM group(s) with potential DM-RS ports which overlap with any configured CSI-RS resource(s) for that UE.

If the UE receives the DM-RS for PDSCH and an SS/PBCH block in the same OFDM symbol(s), then the UE may assume that the DM-RS and SS/PBCH block are quasi co-located with 'QCL-TypeD', if 'QCL-TypeD' is applicable. Furthermore, the UE shall not expect to receive DM-RS in resource elements that overlap with those of the SS/PBCH block, and the UE can expect that the same or different subcarrier spacing is configured for the DM-RS and SS/PBCH block in a CC except for the case of 240 kHz where only different subcarrier spacing is supported.

If a UE is configured by the higher layer parameter *PDCCH-Config* that contains two different values of *CORESETPoolIndex* in *ControlResourceSet*, the UE may be scheduled with fully or partially overlapping PDSCHs in the time and frequency domain by multiple PDCCHs with the following restrictions,

- the UE is not expected to assume different DM-RS configuration with respect to the actual number of front-loaded DM-RS symbol(s), the actual number of additional DM-RS symbol(s), the actual DM-RS symbol location, and DM-RS configuration type.

- the UE is not expected to assume DM-RS ports in a CDM group indicated by two TCI states.

When a UE is not indicated with a DCI that DCI field “*Time domain resource assignment*’ indicating an entry in *pdsch-TimeDomainAllocationList* which contain *RepNumR16* in *PDSCH-TimeDomainResourceAllocatio*n and it is indicated with two TCI states in a codepoint of the DCI field *'Transmission Configuration Indication'* and DM-RS port(s) within two CDM group in the DCI field “*Antenna Port(s)”,*

- the first TCI state corresponds to the CDM group of the first antenna port indicated by the antenna port indication table, and the second TCI state corresponds to the other CDM group.

#### 5.1.6.3 PT-RS reception procedure

A UE shall report the preferred MCS and bandwidth thresholds based on the UE capability at a given carrier frequency, for each subcarrier spacing applicable to data channel at this carrier frequency, assuming the MCS table with the maximum Modulation Order as it reported to support.

If a UE is configured with the higher layer parameter *phaseTrackingRS* in *DMRS-DownlinkConfig*,

- the higher layer parameters *timeDensity* and *frequencyDensity* in *PTRS-DownlinkConfig* indicate the threshold values *ptrs-MCSi*, *i*=1,2,3 and *NRB,i* , *i*=0,1, as shown in Table 5.1.6.3-1 and Table 5.1.6.3-2, respectively.

- if either or both of the additional higher layer parameters *timeDensity* and *frequencyDensity* are configured, and the RNTI equals MCS-C-RNTI, C-RNTI or CS-RNTI, the UE shall assume the PT-RS antenna port' presence and pattern is a function of the corresponding scheduled MCS of the corresponding codeword and scheduled bandwidth in corresponding bandwidth part as shown in Table 5.1.6.3-1 and Table 5.1.6.3-2,

- if the higher layer parameter *timeDensity* given by *PTRS-DownlinkConfig* is not configured, the UE shall assume *LPT-RS* = 1.

- if the higher layer parameter *frequencyDensity* given by *PTRS-DownlinkConfig* is not configured, the UE shall assume *KPT-RS* = 2.

- otherwise, if neither of the additional higher layer parameters *timeDensity* and *frequencyDensity* are configured and the RNTI equals MCS-C-RNTI, C-RNTI or CS-RNTI, the UE shall assume the PT-RS is present with *LPT-RS* = 1, *KPT-RS* = 2, and the UE shall assume PT-RS is not present when

- the scheduled MCS from Table 5.1.3.1-1 is smaller than 10, or

- the scheduled MCS from Table 5.1.3.1-2 is smaller than 5, or

- the scheduled MCS from Table 5.1.3.1-3 is smaller than 15, or

- the number of scheduled RBs is smaller than 3, or

- otherwise, if the RNTI equals RA-RNTI, [MsgB-RNTI], SI-RNTI, or P-RNTI, the UE shall assume PT-RS is not present

Table 5.1.6.3-1: Time density of PT-RS as a function of scheduled MCS

|  |  |
| --- | --- |
| Scheduled MCS | Time density () |
| IMCS < ptrs-MCS1 | PT-RS is not present |
| ptrs-MCS1  IMCS < ptrs-MCS2 | 4 |
| ptrs-MCS2  IMCS < ptrs-MCS3 | 2 |
| ptrs-MCS3  IMCS < ptrs-MCS4 | 1 |

Table 5.1.6.3-2: Frequency density of PT-RS as a function of scheduled bandwidth

|  |  |
| --- | --- |
| Scheduled bandwidth | Frequency density () |
| *NRB* < *NRB0* | PT-RS is not present |
| *NRB0*  *NRB* < *NRB1* | 2 |
| *NRB1*  *NRB* | 4 |

If a UE is not configured with the higher layer parameter *phaseTrackingRS* in *DMRS-DownlinkConfig*, the UE assumes PT-RS is not present.

The higher layer parameter *PTRS-DownlinkConfig* provides the parameters *ptrs-MCSi*, *i*=1,2,3 and with values in range 0-29 when MCS Table 5.1.3.1-1 or MCS Table 5.1.3.1-3 is used and 0-28 when MCS Table 5.1.3.1-2 is used, respectively. *ptrs-MCS4* is not explicitly configured by higher layers but assumed 29 when MCS Table 5.1.3.1-1 or MCS Table 5.1.3.1-3 is used and 28 when MCS Table 5.1.3.1-2 is used, respectively. The higher layer parameter *frequencyDensity* in *PTRS-DownlinkConfig* provides the parameters *NRBi**i*=0,1 with values in range 1-276.

If the higher layer parameter *PTRS-DownlinkConfig* indicates that the time density thresholds *ptrs-MCSi* = *ptrs-MCSi+1*, then the time density *LPT-RS* of the associated row where both these thresholds appear in Table 5.1.6.3-1 is disabled. If the higher layer parameter *PTRS-DownlinkConfig* indicates that the frequency density thresholds *NRBi* = *NRBi**+1*, then the frequency density *KPTRS* of the associated row where both these thresholds appear in Table 5.1.6.3-2 is disabled.

If either or both of the parameters PT-RS time density (*LPT-RS*) and PT-RS frequency density (*KPT-RS*), shown in Table 5.1.6.3-1 and Table 5.1.6.3-2, indicates that 'PT-RS not present', the UE shall assume that PT-RS is not present.

When the UE is receiving a PDSCH with allocation duration of 2 symbols as defined in Clause 7.4.1.1.2 of [4, TS 38.211] and if *LPT-RS* is set to 2 or 4, the UE shall assume PT-RS is not transmitted.

When the UE is receiving a PDSCH with allocation duration of 4 symbols and if *LPT-RS* is set to 4, the UE shall assume PT-RS is not transmitted.

When a UE is receiving PDSCH for retransmission, if the UE is scheduled with an MCS index greater than V, where V=28 for MCS Table 5.1.3.1-1 and Table 5.1.3.1-3, and V=27 for MCS Table 5.1.3.1-2 respectively, the MCS for the PT-RS time-density determination is obtained from the DCI received for the same transport block in the initial transmission, which is smaller than or equal to V.

The DL DM-RS port(s) associated with a PT-RS port are assumed to be quasi co-located with respect to {'QCL-TypeA' and 'QCL-TypeD'}.If a UE is scheduled with one codeword, the PT-RS antenna port is associated with the lowest indexed DM-RS antenna port among the DM-RS antenna ports assigned for the PDSCH.

If a UE is scheduled with two codewords, the PT-RS antenna port is associated with the lowest indexed DM-RS antenna port among the DM-RS antenna ports assigned for the codeword with the higher MCS. If the MCS indices of the two codewords are the same, the PT-RS antenna port is associated with the lowest indexed DM-RS antenna port assigned for codeword 0.

When a UE is not indicated with a DCI that DCI field “*Time domain resource assignment*’ indicating an entry in *pdsch-TimeDomainAllocationList* which contain *RepNumR16* in *PDSCH-TimeDomainResourceAllocatio*n, and if the UE is configured with the higher layer parameter *maxNrofPorts* equal to *n2*, and if the UE is indicated with two TCI states by the codepoints of the DCI field *'Transmission Configuration Indication'* and DM-RS port(s) within two CDM group in the DCI field “*Antenna Port(s)”*, the UE shall receive two PT-RS ports which are associated to the lowest indexed DM-RS port among the DM-RS ports corresponding to the first/second indicated TCI state, respectively.

When a UE configured by the higher layer parameter *RepSchemeEnabler* set to ‘*FDMSchemeA’* or ‘*FDMSchemeB’,* and the UE is indicated with two TCI states in a codepoint of the DCI field *'Transmission Configuration Indication* and DM-RS port(s) within one CDM group in the DCI field “*Antenna Port(s)*”, the UE shall receive a single PT-RS port which is associated with the lowest indexed DM-RS antenna port among the DM-RS antenna ports assigned for the PDSCH, a PT-RS frequency density is determined by the number of PRBs associated to each TCI state, and a PT-RS resource element mapping is associated to the allocated PRBs for each TCI state.

#### 5.1.6.4 SRS reception procedure for CLI

The SRS resources defined in Clause 6.4.1.4 of [4, TS 38.211] may be configured for SRS-RSRP measurement for CLI, as defined in Clause 5.1.19 of [7, TS 38.215]. The UE is not expected to measure SRS-RSRP with a subcarrier spacing other than the one configured for the active BWP confining the SRS resource. The UE is not expected to measure more than 32 SRS resources, and the UE is not expected to receive more than 8 SRS resources in a slot.

#### 5.1.6.5 PRS reception procedure

The UE can be configured with one or more DL PRS resource set configuration(s) as indicated by the higher layer parameters *DL-PRS-ResourceSet* and *DL-PRS-Resource*. Each DL PRS resource set consists of K≥1 DL PRS resource(s) where each has an associated spatial transmission filter~~.~~ The UE can be configured with one or more DL PRS Positioning Frequency Layer configuration(s) as indicated by the higher layer parameter *DL-PRS-PositioningFrequencyLayer.* A DL PRS Positioning Frequency Layer is defined as a collection of DL PRS Resource Sets which have common parameters configured by *DL-PRS-PositioningFrequencyLayer*.

The UE assumes that the following parameters for each DL PRS resource(s) are configured via higher layer parameters *DL-PRS-PositioningFrequencyLayer, DL-PRS-ResourceSet* and *DL-PRS-Resource*.

A positioning frequency layer consists of one or more PRS resource sets and it is defined by:

*- DL-PRS-SubcarrierSpacing* defines the subcarrier spacing for the DL PRS resource. All DL PRS Resources and DL PRS Resource sets in the same DL-PRS-PositioningFrequencyLayer have the same value of *DL-PRS-SubcarrierSpacing*. The supported values of DL-PRS-SubcarrierSpacing are given in Table 4.2-1 of [4, TS38.211].

*- DL-PRS-CyclicPrefix* defines the cyclic prefix for the DL PRS resource. All DL PRS Resources and DL PRS Resource sets in the same DL-PRS-PositioningFrequencyLayer have the same value of *DL-PRS-CyclicPrefix.* The supported values of *DL-PRS-CyclicPrefix* are given in Table 4.2-1 of [4, TS38.211].

*- DL-PRS-PointA* defines the absolute frequency of the reference resource block. Its lowest subcarrier is also known as Point A. All DL PRS resources belonging to the same DL PRS Resource Set have common Point A and all DL PRS Resources sets belonging to the same DL-PRS-PositioningFrequencyLayer have a common Point A.

The UE expects that it will be configured with [IDs] each of which is defined such that it is associated with multiple DL PRS Resource Sets from the same cell. The UE expects that one of these [IDs] along with a *DL-PRS-ResourceSetId* and a *DL-PRS-ResourceId* can be used to uniquely identify a DL PRS Resource.

A PRS resource set consists of one or more PRS resources and it is defined by:

*- DL-PRS-ResourceSetId* defines the identity of the DL PRS resource set configuration.

*- DL-PRS-Periodicity* defines the DL PRS resource periodicity and takes values slots, where for *DL-PRS-SubcarrierSpacing*=15, 30, 60 and 120kHz respectively. 20480 is not supported for All the DL PRS resources within one resource set are configured with the same periodicity.

*- DL-PRS-ResourceRepetitionFactor* defines how many times each DL-PRS resource is repeated for a single instance of the DL-PRS resource set and takes values ,. All the DL PRS resources within one resource set have the same *ResourceRepetitionFactor*

*- DL-PRS-ResourceTimeGap* defines the offset in number of slots between two repeated instances of a DL PRS resource with the same *DL-PRS-ResourceID* within a single instance of the DL PRS resource set and takes values . The UE only expects to be configured with *DL-PRS-ResourceTimeGap* if *DL-PRS-ResourceRepetitionFactor* is configured with value greater than 1. The time duration spanned by one instance of a *DL-PRS-ResourceSet* is not expected to exceed the configured value of *DL-PRS-Periodicity*. All the DL PRS resources within one resource set have the same *DL-PRS-ResourceTimeGap.*

*- DL-PRS-MutingPattern* defines a bitmap of the time locations where the DL PRS resource is expected to not be transmitted for a DL PRS resource set. The bitmap size can be {2, 4, 8, 16, 32} bits long. The bitmap has two options for applicability. In the first option each bit in the bitmap corresponds to a configurable number of consecutive instances of a *DL-PRS-ResourceSet* where all the *DL-PRS-Resources* within the set are muted for the instance that is indicated to be muted. In the second option each bit in the bitmap corresponds to a single repetition index for each of the *DL-PRS-Resources* within each instance of a *DL-PRS-ResourceSet* and the length of the bitmap is equal to *DL-PRS-ResourceRepetitionFactor*. Both options may be configured at the same time in which case the logical AND operation is applied to the bit maps as described in clause 7.4.1.7.4 of [4, TS 38.211].

*- DL-PRS-SFN0-Offset* defines the time offset of the SFN0 slot 0 for the transmitting cell with respect to SFN0 slot 0 of [FFS in RAN2].

*- DL-PRS-ResourceSetSlotOffset* defines the slot offset with respect to SFN0 slot 0 and takes values .

*- DL-PRS-CombSizeN* defines the comb size of a DL PRS resource where the allowable values are given in Clause 7.4.1.7.1 of [TS38.211]. All DL PRS resource sets belonging to the same positioning frequency layer have the same value of *DL-PRS-combSizeN*.

*- DL-PRS-ResourceBandwidth* defines the number of resource blocks configured for PRS transmission. The parameter has a granularity of 4 PRBs with a minimum of 24 PRBs and a maximum of 272 PRBs. All DL PRS resources sets within a positioning frequency layer have the same value of *DL-PRS-ResourceBandwidth*.

A PRS resource is defined by:

*- DL-PRS-ResourceList* determines the DL PRS resources that are contained within one DL PRS resource set.

*- DL-PRS-ResourceId* determines the DL PRS resource configuration identity. All DL PRS resource IDs are locally defined within a DL PRS resource set.

*- DL-PRS-SequenceId* is used to initialize cinit value used in pseudo random generator [4, TS38.211, 7.4.1.7.2] for generation of DL PRS sequence for a given DL PRS resource.

*- DL-PRS-ReOffset* defines the starting RE offset of the first symbol within a DL PRS resource in frequency. The relative RE offsets of the remaining symbols within a DL PRS resource are defined based on the initial offset and the rule described in Clause 7.4.1.7.3 of [4, TS38.211].

*- DL-PRS-ResourceSlotOffset* determines the starting slot of the DL PRS resource with respect to corresponding *DL-PRS-ResourceSetSlotOffset*

*- DL-PRS-ResourceSymbolOffset* determines the starting symbol of the DL PRS resource within the starting slot.

*- DL-PRS-NumSymbols* defines the number of symbols of the DL PRS resource within a slot where the allowable values are given in Clause 7.4.1.7.1 of [4, TS38.211].

*- DL-PRS-QCL-Info* defines any quasi-colocation information of the DL PRS resource with other reference signals. The DL PRS may be configured to be ‘QCL-Type-D’ with a DL PRS or SS/PBCH Block from a serving cell or a non-serving cell. The DL PRS may be configured to be ‘QCL-Type-C’ with a SS/PBCH Block from a serving or non-serving cell. If the DL PRS is configured as both ‘QCL-Type-C’ and ‘QCL-Type-D’ with a SS/PBCH Block then the SSB index indicated should be the same.

*- DL-PRS-StartPRB* defines the starting PRB index of the DL PRS resource with respect to reference Point A. The starting PRB index has a granularity of one PRB with a minimum value of 0 and a maximum value of 2176 PRBs. All DL PRS Resource Sets belonging to the same Positioning Frequency Layer have the same value of Start PRB.

The UE assumes constant EPRE is used for all REs of a given DL PRS resource.

The UE may be indicated by the network that a DL PRS resources can be used as the reference for the RSTD measurement in a higher layer parameter *DL-PRS-RstdReferenceInfo*. The reference time indicated by the network to the UE can also be used by the UE to determine how to apply higher layer parameters DL-PRS-expectedRSTD and DL-PRS-expectedRSTD-uncertainty. The UE expects the reference time to be indicated whenever it is expected to receive the DL PRS. This reference time provided by *DL-PRS-RstdReferenceInfo* may include an [ID], a PRS resource set ID, and optionally a single PRS resource ID or a list of PRS resource IDs. The UE may use different DL PRS resources or a different DL PRS resource set to determine the reference time for the RSTD measurement as long as the condition that the DL PRS resources used belong to a single DL PRS resource set is met. If the UE chooses to use a different reference time than indicated by the network, then it is expected to report the DL PRS resource ID(s) or the DL PRS resource set ID used to determine the reference.

The UE may be configured to report quality metrics corresponding to the RSTD and UE Rx-Tx time difference measurements which include the following fields:

*- TimingMeasQuality-Value* which provides the best estimate of the uncertainty of the measurement

*- TimingMeasQuality-Resolution* which specifies the resolution levels used in the Value field

The UE expects to be configured with higher layer parameter *DL-PRS-expectedRSTD*, which defines the time difference with respect to the received DL subframe timing the UE is expected to receive DL PRS, and *DL-PRS-expectedRSTD-uncertainty*, which defines a search window around the expectedRSTD.

For DL UE positioning measurement reporting in higher layer parameters *DL-PRS-RstdMeasurementInfo or DL-PRS-UE-Rx-Tx-MeasurementInfo* the UE can be configured to report the DL PRS resource ID(s) or the DL PRS resource set ID(s) associated with the DL PRS resource(s) or the DL PRS resource set(s) which are used in determining the UE measurements DL RSTD, UE Tx-Rx time difference or the DL PRS-RSRP.

The UE can be configured in higher layer parameter *UE Rx-Tx Time-MeasRequestInfo* to report multiple UE Rx-Tx time difference measurements corresponding to a single configured SRS resource or resource set for positioning. Each measurement corresponds to a single received DL PRS resource or resource set which can be in difference positioning frequency layers.

For the DL RSTD, DL PRS-RSRP, and UE Rx-Tx time difference measurements the UE can report an associated higher layer parameter *Timestamp*. The *Timestamp* can include the SFN and the slot number for a subcarrier spacing. These values correspond to the reference which is provided by *DL-PRS-RSTDReferenceInfo*.

The UE is expected to measure the DL PRS resource outside the active DL BWP or with a numerology different from the numerology of the active DL BWP if the measurement is made during a configured measurement gap. When not configured with a measurement gap, the UE is only required to measure DL PRS within the active DL BWP and with the same numerology as the active DL BWP. If the UE is not provided with a measurement gap, the UE is not expected to process DL PRS resources on serving or non-serving cells on any symbols indicated as UL by the serving cell. When the UE is expected to measure the DL PRS resource outside the active DL BWP it may request a measurement gap in higher layer parameter [XYZ].

The UE assumes that for the serving cell the DL PRS is not mapped to any symbol that contains SS/PBCH. If the time frequency location of the SS/PBCH block transmissions from non-serving cells are provided to the UE then the UE also assumes that the DL PRS is not mapped to any symbol that contains the SS/PBCH block of the non-serving cell.

The UE may be configured to report, subject to UE capability, up to 4 DL RSTD measurements per pair of cells with each measurement between a different pair of DL PRS resources or DL PRS resource sets within the DL PRS configured for those cells. The up to 4 measurements being performed on the same pair of cells and all DL RSTD measurements in the same report use a single reference timing.

The UE may be configured to measure and report up to 8 DL PRS RSRP measurements on different DL PRS resources from the same cell. When the UE reports DL PRS RSRP measurements from one DL PRS resource set, the UE may indicate which DL PRS RSRP measurements have been performed using the same spatial domain filter for reception.

If the UE is configured with *DL-PRS-QCL-Info* and the QCL relation is between two DL PRS resources, then the UE assumes those DL PRS resources are from the same cell. If *DL-PRS-QCL-Info* is configured to the UE with ‘QCL-Type-D’ with a source DL-PRS-Resource then the *DL-PRS-ResourceSetId* and the *DL-PRS-ResrouceId* of the source DL-PRS-Resource are expected to be indicated to the UE.

The UE does not expect to process the DL PRS in the same symbol where other DL signals and channels are transmitted to the UE when there is no measurement gap configured to the UE.

### 5.1.7 Code block group based PDSCH transmission

#### 5.1.7.1 UE procedure for grouping of code blocks to code block groups

If a UE is configured to receive code block group (CBG) based transmissions by receiving the higher layer parameter *codeBlockGroupTransmission* for PDSCH, the UE shall determine the number of CBGs for atransport block reception as

,

where *N* is the maximum number of CBGs per transport block as configured by *maxCodeBlockGroupsPerTransportBlock* for PDSCH, and *C* is the number of code blocks in the transport block according to the procedure defined in Clause 7.2.3 of [5, TS 38.212].

Define , , and .

If , CBG *m*, , consists of code blocks with indices . CBG *m*, , consists of code blocks with indices .

#### 5.1.7.2 UE procedure for receiving code block group based transmissions

If a UE is configured to receive code block group based transmissions by receiving the higher layer parameter *codeBlockGroupTransmission* for PDSCH,

- The CBG transmission information (CBGTI) field of DCI format 1\_1 is of length bits, where is the value of the higher layer parameter *maxNrofCodeWordsScheduledByDCI*. If the CBGTI field bits are mapped such that the first set of bits starting from the MSB corresponds to the first TB while the second set of bits corresponds to a second TB, if scheduled. The first *M* bits of each set of bits in the CBGTI field have an in-order one-to-one mapping with the *M* CBGs of the TB, with the MSB mapped to CBG#0.

- For initial transmission of a TB as indicated by the *New Data Indicator* field of the scheduling DCI, the UE may assume that all the code block groups of the TB are present.

- For a retransmission of a TB as indicated by the *New Data Indicator* field of the scheduling DCI, the UE may assume that

- The *CBGTI* field of the scheduling DCI indicates which CBGs of the TB are present in the transmission. A bit value of 0' in the *CBGTI* field indicates that the corresponding CBG is not transmitted and 1' indicates that it is transmitted.

- If the CBG flushing out information *(CBGFI)* field of the scheduling DCI is present, *CBGFI* set to 0' indicates that the earlier received instances of the same CBGs being transmitted may be corrupted, and *CBGFI* set to 1' indicates that the CBGs being retransmitted are combinable with the earlier received instances of the same CBGs.

- A CBG contains the same CBs as in the initial transmission of the TB.

## 5.2 UE procedure for reporting channel state information (CSI)

### 5.2.1 Channel state information framework

The procedures on aperiodic CSI reporting described in this section assume that the CSI reporting is triggered by DCI format 0\_1, but they equally apply to CSI reporting triggered by DCI format 0\_2, by applying the parameters *CSI-AperiodicTriggerStateList-ForDCIFormat0\_2,* [*CSI-SemiPersistentOnPUSCH-TriggerStateList-ForDCIFormat0\_2]* and *reportTriggerSize-ForDCIFormat0\_2* instead of *CSI-AperiodicTriggerStateList,* [*CSI-SemiPersistentOnPUSCH-TriggerStateList]* and *reportTriggerSize*, respectively.

The time and frequency resources that can be used by the UE to report CSI are controlled by the gNB. CSI may consist of Channel Quality Indicator (CQI), precoding matrix indicator (PMI), CSI-RS resource indicator (CRI), SS/PBCH Block Resource indicator (SSBRI), layer indicator (LI), rank indicator (RI), L1-RSRP or L1-SINR.

For CQI, PMI, CRI, SSBRI, LI, RI, L1-RSRP, L1-SINR a UE is configured by higher layers with N≥1 *CSI-ReportConfig* Reporting Settings, M≥1 *CSI-ResourceConfig* Resource Settings, and one or two list(s) of trigger states (given by the higher layer parameters *CSI-AperiodicTriggerStateList* and *CSI-SemiPersistentOnPUSCH-TriggerStateList*). Each trigger state in *CSI-AperiodicTriggerStateList* contains a list of associated *CSI-ReportConfigs* indicating the Resource Set IDs for channel and optionally for interference. Each trigger state in *CSI-SemiPersistentOnPUSCH-TriggerStateList* contains one associated *CSI-ReportConfig*.

#### 5.2.1.1 Reporting settings

Each Reporting Setting *CSI-ReportConfig* is associated with a single downlink BWP (indicated by higher layer parameter *BWP-Id*) given in the associated *CSI-ResourceConfig* for channel measurement and contains the parameter(s) for one CSI reporting band:codebook configuration including codebook subset restriction, time-domain behavior, frequency granularity for CQI and PMI, measurement restriction configurations, and the CSI-related quantities to be reported by the UE such as the layer indicator (LI), L1-RSRP, L1-SINR, CRI, and SSBRI (SSB Resource Indicator).

The time domain behavior of the *CSI-ReportConfig* is indicated by the higher layer parameter *reportConfigType* and can be set to 'aperiodic', 'semiPersistentOnPUCCH', 'semiPersistentOnPUSCH', or 'periodic'. For periodic and semiPersistentOnPUCCH/semiPersistentOnPUSCH CSI reporting, the configured periodicity and slot offset applies in the numerology of the UL BWP in which the CSI report is configured to be transmitted on. The higher layer parameter *reportQuantity* indicates the CSI-related, L1-RSRP-related or L1-SINR-related quantities to report. The *reportFreqConfiguration* indicates the reporting granularity in the frequency domain, including the CSI reporting band and if PMI/CQI reporting is wideband or sub-band. The *timeRestrictionForChannelMeasurements* parameter in *CSI-ReportConfig* can be configured to enable time domain restriction for channel measurements and *timeRestrictionForInterferenceMeasurements* can be configured to enable time domain restriction for interference measurements. The *CSI-ReportConfig* can also contain *CodebookConfig*, which contains configuration parameters for Type-I, Type II or Enhanced Type II CSI including codebook subset restriction, and configurations of group based reporting.

For operation with shared spectrum channel access, the UE should not average CSI-RS measurements for channel estimation from occasions of an NZP CSI-RS (defined in [4, TS 38.211]) located in different DL transmissions burst (defined in [X, TS 37.213]).

#### 5.2.1.2 Resource settings

Each CSI Resource Setting *CSI-ResourceConfig* contains a configuration of a list of S≥1 CSI Resource Sets (given by higher layer parameter *csi-RS-ResourceSetList*), where the list is comprised of references to either or both of NZP CSI-RS resource set(s) and SS/PBCH block set(s) or the list is comprised of references to CSI-IM resource set(s). Each CSI Resource Setting is located in the DL BWP identified by the higher layer parameter *BWP-id*, and all CSI Resource Settings linked to a CSI Report Setting have the same DL BWP.

The time domain behavior of the CSI-RS resources within a CSI Resource Setting are indicated by the higher layer parameter *resourceType* and can be set to aperiodic, periodic, or semi-persistent. For periodic and semi-persistent CSI Resource Settings, the number of CSI-RS Resource Sets configured is limited to S=1. For periodic and semi-persistent CSI Resource Settings, the configured periodicity and slot offset is given in the numerology of its associated DL BWP, as given by *BWP-id.* When a UE is configured with multiple *CSI-ResourceConfigs* consisting the same NZP CSI-RS resource ID, the same time domain behavior shall be configured for the *CSI-ResourceConfigs*. When a UE is configured with multiple *CSI-ResourceConfigs* consisting the same CSI-IM resource ID, the same time-domain behavior shall be configured for the *CSI-ResourceConfigs*. All CSI Resource Settings linked to a CSI Report Setting shall have the same time domain behavior.

The following are configured via higher layer signaling for one or more CSI Resource Settings for channel and interference measurement:

- CSI-IM resource for interference measurement as described in Clause 5.2.2.4.

- NZP CSI-RS resource for interference measurement as described in Clause 5.2.2.3.1.

- NZP CSI-RS resource for channel measurement as described in Clause 5.2.2.3.1.

The UE may assume that the NZP CSI-RS resource(s) for channel measurement and the CSI-IM resource(s) for interference measurement configured for one CSI reporting are resource-wise QCLed with respect to 'QCL-TypeD'. When NZP CSI-RS resource(s) is used for interference measurement, the UE may assume that the NZP CSI-RS resource for channel measurement and the CSI- IM resource or NZP CSI-RS resource(s) for interference measurement configured for one CSI reporting are QCLed with respect to 'QCL-TypeD'.

For L1-SINR measurement:

- When one Resource Setting is configured, the Resource Setting (given by higher layer parameter *resourcesForChannelMeasurement*) is for channel and interference measurement for L1-SINR computation. UE may assume that same 1 port NZP CSI-RS resource(s) with density 3 REs/RB is used for both channel and interference measurements.

- When two Resource Settings are configured, the first one Resource Setting (given by higher layer parameter *resourcesForChannelMeasurement*) is for channel measurement on SSB or 1 port NZP CSI-RS with density 3 REs/RB and the second one (given by either higher layer parameter *csi-IM-ResourcesForInterference* or higher layer parameter *nzp-CSI-RS-ResourcesForInterference*) is for interference measurement performed on CSI-IM or on 1 port NZP CSI-RS with density 3 REs/RB, where each SSB or NZP CSI-RS resource for channel measurement is associated with one CSI-IM resource or one NZP CSI-RS resource for interference measurement by the ordering of the SSB or NZP CSI-RS resource for channel measurement and CSI-IM resource or NZP CSI-RS resource for interference measurement in the corresponding resource sets. The number of SSB(s) or CSI-RS resources for channel measurement equals to the number of CSI-IM resources or the number of NZP CSI-RS resource for interference measurement.

- UE may apply 'QCL-TypeD' assumption of the SSB or 'QCL-TypeD' configured to the NZP CSI-RS resource for channel measurement to measure the associated CSI- IM resource or associated NZP CSI-RS resource for interference measurement configured for one CSI reporting

- UE may expect that the NZP CSI-RS resource set for channel measurement and the NZP-CSI-RS resource set for interference measurement, if any, are configured with the higher layer parameter *repetition*.

- [When three Resource Settings are configured, the first one Resource Setting (given by higher layer *parameterresourcesForChannelMeasurement*) is for channel measurement on SSB or NZP CSI-RS. The second one (given by either higher layer parameter *csi-IM-ResourcesForInterference*) is for interference measurement performed on CSI-IM, where each NZP CSI-RS resource set for channel measurement is associated with one CSI-IM resource for interference measurement. The Third one (given by higher layer parameter *nzp-CSI-RS-ResourcesForInterference*) is for interference measurement performed on 1 port NZP CSI-RS with density 3 REs/RB.]

#### 5.2.1.3 (void)

#### 5.2.1.4 Reporting configurations

The UE shall calculate CSI parameters (if reported) assuming the following dependencies between CSI parameters (if reported)

- LI shall be calculated conditioned on the reported CQI, PMI, RI and CRI

- CQI shall be calculated conditioned on the reported PMI, RI and CRI

- PMI shall be calculated conditioned on the reported RI and CRI

- RI shall be calculated conditioned on the reported CRI.

The Reporting configuration for CSI can be aperiodic (using PUSCH), periodic (using PUCCH) or semi-persistent (using PUCCH, and DCI activated PUSCH). The CSI-RS Resources can be periodic, semi-persistent, or aperiodic. Table 5.2.1.4-1 shows the supported combinations of CSI Reporting configurations and CSI-RS Resource configurations and how the CSI Reporting is triggered for each CSI-RS Resource configuration. Periodic CSI-RS is configured by higher layers. Semi-persistent CSI-RS is activated and deactivated as described in Clause 5.2.1.5.2. Aperiodic CSI-RS is configured and triggered/activated as described in Clause 5.2.1.5.1.

Table 5.2.1.4-1: Triggering/Activation of CSI Reporting for the possible CSI-RS Configurations.

|  |  |  |  |
| --- | --- | --- | --- |
| CSI-RS Configuration | Periodic CSI Reporting | Semi-Persistent CSI Reporting | Aperiodic CSI Reporting |
| Periodic CSI-RS | No dynamic triggering/activation | For reporting on PUCCH, the UE receives an activation command, as described in clause 6.1.3.16 of [10, TS 38.321]; for reporting on PUSCH, the UE receives triggering on DCI | Triggered by DCI; additionally, subselection indication as described in clause 6.1.3.13 of [10, TS 38.321] possible as defined in Clause 5.2.1.5.1. |
| Semi-Persistent CSI-RS | Not Supported | For reporting on PUCCH, the UE receives an activation command, as described in clause 6.1.3.16 of [10, TS 38.321]; for reporting on PUSCH, the UE receives triggering on DCI | Triggered by DCI; additionally, subselection indication as described in clause 6.1.3.13 of [10, TS 38.321] possible as defined in Clause 5.2.1.5.1. |
| Aperiodic CSI-RS | Not Supported | Not Supported | Triggered by DCI; additionally, subselection indication as described in clause 6.1.3.13 of [10, TS 38.321] possible as defined in Clause 5.2.1.5.1. |

When the UE is configured with higher layer parameter *NZP-CSI-RS-ResourceSet* and when the higher layer parameter *repetition* is set to 'off', the UE shall determine a CRI from the supported set of CRI values as defined in Clause 6.3.1.1.2 of [5, TS 38.212] and report the number in each CRI report. When the higher layer parameter *repetition* is set to 'on', CRI is not reported. CRI reporting is not supported when the higher layer parameter *codebookType* is set to either 'typeII', 'typeII-PortSelection', ‘typeII-r16’ or to ‘typeII-PortSelection-r16’.

For a periodic or semi-persistent CSI report on PUCCH, the periodicity (measured in slots) and the slot offset are configured by the higher layer parameter *reportSlotConfig*. Unless specified otherwise, the UE shall transmit the CSI report in frames with SFN and slot number within the frame satisfying

where is the SCS configuration of the UL BWP the CSI report is transmitted on.

For a semi-persistent CSI report on PUSCH, the periodicity (measured in slots) is configured by the higher layer parameter *reportSlotConfig.* Unless specified otherwise, the UE shall transmit the CSI report in frames with SFN and slot number within the frame satisfying

where and are the SFN and slot number within the frame respectively of the initial semi-persistent PUSCH transmission according to the activating DCI.

For a semi-persistent or aperiodic CSI report on PUSCH, the allowed slot offsets are configured by the following higher layer parameters:

- if triggered/activated by DCI format 0\_2, the allowed slot offsets are configured by the higher layer parameter *reportSlotOffsetList-r16-ForDCIFormat0\_2*, and

- if triggered/activated by DCI format 0\_1 and *reportSlotOffsetList-r16-ForDCIFormat0\_1* is configured, the allowed slot offsets are configured by the higher layer parameter *reportSlotOffsetList-r16-ForDCIFormat0\_1,* and

- otherwise, the allowed slot offsets are configured] by the higher layer parameter *reportSlotOffsetList*.

The offset is selected in the activating/triggering DCI.

For CSI reporting, a UE can be configured via higher layer signaling with one out of two possible subband sizes, where a subband is defined as  contiguous PRBs and depends on the total number of PRBs in the bandwidth part according to Table 5.2.1.4-2.

Table 5.2.1.4-2: Configurable subband sizes

|  |  |
| --- | --- |
| **Bandwidth part (PRBs)** | **Subband size (PRBs)** |
| < 24 | N/A |
| 24 – 72 | 4, 8 |
| 73 – 144 | 8, 16 |
| 145 – 275 | 16, 32 |

The *reportFreqConfiguration* contained in a *CSI-ReportConfig* indicates the frequency granularity of the CSI Report. A CSI Reporting Setting configuration defines a CSI reporting band as a subset of subbands of the bandwidth part, where the *reportFreqConfiguration* indicates:

- the *csi-ReportingBand* as a contiguous or non-contiguous subset of subbands in the bandwidth part for which CSI shall be reported.

- A UE is not expected to be configured with *csi-ReportingBand* which contains a subband where a CSI-RS resource linked to the CSI Report setting has the frequency density of each CSI-RS port per PRB in the subband less than the configured density of the CSI-RS resource.

- If a CSI-IM resource is linked to the CSI Report Setting, a UE is not expected to be configured with *csi-ReportingBand* which contains a subband where not all PRBs in the subband have the CSI-IM REs present.

- wideband CQI or subband CQI reporting, as configured by the higher layer parameter *cqi-FormatIndicator*. When wideband CQI reporting is configured, a wideband CQI is reported for each codeword for the entire CSI reporting band. When subband CQI reporting is configured, one CQI for each codeword is reported for each subband in the CSI reporting band.

- wideband PMI or subband PMI reporting as configured by the higher layer parameter *pmi-FormatIndicator*. When wideband PMI reporting is configured, a wideband PMI is reported for the entire CSI reporting band. When subband PMI reporting is configured, except with 2 antenna ports, a single wideband indication (*i1* in Clause 5.2.2.2) is reported for the entire CSI reporting band and one subband indication (*i2* in clause 5.2.2.2) is reported for each subband in the CSI reporting band. When subband PMIs are configured with 2 antenna ports, a PMI is reported for each subband in the CSI reporting band.

A CSI Reporting Setting is said to have a wideband frequency-granularity if

- *reportQuantity* is set to 'cri-RI-PMI-CQI', or 'cri-RI-LI-PMI-CQI', *cqi-FormatIndicator* is set to 'widebandCQI' and *pmi-FormatIndicator* is set to 'widebandPMI', or

- *reportQuantity* is set to 'cri-RI-i1' or

- *reportQuantity* is set to 'cri-RI-CQI' or 'cri-RI-i1-CQI' and *cqi-FormatIndicator* is set to 'widebandCQI', or

- *reportQuantity* is set to 'cri-RSRP' or 'ssb-Index-RSRP'

otherwise, the CSI Reporting Setting is said to have a subband frequency-granularity.

The first subband size is given by  and the last subband size given by  if  and if 

If a UE is configured with semi-persistent CSI reporting, the UE shall report CSIwhen both CSI-IM and NZP CSI-RS resources are configured as periodic or semi-persistent. If a UE is configured with aperiodic CSI reporting, the UE shall report CSIwhen both CSI-IM and NZP CSI-RS resources are configured as periodic, semi-persistent or aperiodic.

A UE configured with DCI format 0\_1 or 0\_2 does not expect to be triggered with multiple CSI reports with the same *CSI-ReportConfigId*.

##### 5.2.1.4.1 Resource Setting configuration

For aperiodic CSI, each trigger state configured using the higher layer parameter *CSI-AperiodicTriggerState* is associated with one or multiple *CSI-ReportConfig* where each *CSI-ReportConfig* is linked to periodic, or semi-persistent, or aperiodic resource setting(s):

- When one Resource Setting is configured, the Resource Setting (given by higher layer parameter *resourcesForChannelMeasurement*) is for channel measurement for L1-RSRP or L1-SINR computation.

- When two Resource Settings are configured, the first one Resource Setting (given by higher layer parameter *resourcesForChannelMeasurement*) is for channel measurement and the second one (given by either higher layer parameter *csi-IM-ResourcesForInterference* or higher layer parameter *nzp-CSI-RS-ResourcesForInterference*) is for interference measurement performed on CSI-IM or on NZP CSI-RS.

- When three Resource Settings are configured, the first Resource Setting (higher layer parameter *resourcesForChannelMeasurement*) is for channel measurement, the second one (given by higher layer parameter *csi-IM-ResourcesForInterference*) is for CSI-IM based interference measurement and the third one (given by higher layer parameter *nzp-CSI-RS-ResourcesForInterference*) is for NZP CSI-RS based interference measurement.

For semi-persistent or periodic CSI, each *CSI-ReportConfig* is linked to periodic or semi-persistent Resource Setting(s):

- When one Resource Setting (given by higher layer parameter *resourcesForChannelMeasurement*) is configured, the Resource Setting is for channel measurement for L1-RSRP computation.

- When two Resource Settings are configured, the first Resource Setting (given by higher layer parameter *resourcesForChannelMeasurement*) is for channel measurement and the second Resource Setting (given by higher layer parameter *csi-IM-ResourcesForInterference*) is used for interference measurement performed on CSI-IM.

A UE is not expected to be configured with more than one CSI-RS resource in resource set for channel measurement for a *CSI-ReportConfig* with the higher layer parameter *codebookType* set to either 'typeII', 'typeII-PortSelection', ‘typeII-r16’ or to ‘typeII-PortSelection-r16’. A UE is not expected to be configured with more than 64 NZP CSI-RS resources in resource setting for channel measurement for a CSI-ReportConfig with the higher layer parameter *reportQuantity* set to 'none', 'cri-RI-CQI', 'cri-RSRP' or 'ssb-Index-RSRP'. If interference measurement is performed on CSI-IM, each CSI-RS resource for channel measurement is resource-wise associated with a CSI-IM resource by the ordering of the CSI-RS resource and CSI-IM resource in the corresponding resource sets. The number of CSI-RS resources for channel measurement equals to the number of CSI-IM resources.

If interference measurement is performed on NZP CSI-RS, a UE does not expect to be configured with more than one NZP CSI-RS resource in the associated resource set within the resource setting for channel measurement. The UE configured with the higher layer parameter *nzp-CSI-RS-ResourcesForInterference* may expect no more than 18 NZP CSI-RS ports configured in a NZP CSI-RS resource set.

For CSI measurement(s), a UE assumes:

- each NZP CSI-RS port configured for interference measurement corresponds to an interference transmission layer.

- all interference transmission layers on NZP CSI-RS ports for interference measurement take into account the associated EPRE ratios configured in 5.2.2.3.1;

- other interference signal on REs of NZP CSI-RS resource for channel measurement, NZP CSI-RS resource for interference measurement, or CSI-IM resource for interference measurement.

##### 5.2.1.4.2 Report Quantity Configurations

A UE may be configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to either 'none', 'cri-RI-PMI-CQI ', 'cri-RI-i1', 'cri-RI-i1-CQI', 'cri-RI-CQI', 'cri-RSRP', 'cri-SINR', 'ssb-Index-RSRP', 'ssb-Index-SINR' or 'cri-RI-LI-PMI-CQI'.

If the UE is configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to 'none', then the UE shall not report any quantity for the *CSI-ReportConfig*.

If the UE is configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to 'cri-RI-PMI-CQI', or 'cri-RI-LI-PMI-CQI', the UE shall report a preferred precoder matrix for the entire reporting band, or a preferred precoder matrix per subband, according to Clause 5.2.2.2.

If the UE is configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to 'cri-RI-i1',

- the UE expects, for that *CSI-ReportConfig,* to be configured with higher layer parameter *codebookType* set to 'typeI-SinglePanel' and *pmi-FormatIndicator* set to 'widebandPMI'and,

- the UE shall report a PMI consisting of a single wideband indication ( in Clause 5.2.2.2.1) for the entire CSI reporting band.

If the UE is configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to 'cri-RI-i1-CQI',

- the UE expects, for that *CSI-ReportConfig,* to be configured with higher layer parameter *codebookType* set to 'typeI-SinglePanel' and *pmi-FormatIndicator* set to 'widebandPMI'and,

- the UE shall report a PMI consisting of a single wideband indication ( in Clause 5.2.2.2.1) for the entire CSI reporting band. The CQI is calculated conditioned on the reported assuming PDSCH transmission with  precoders (corresponding to the same but different  in Clause 5.2.2.2.1), where the UE assumes that one precoder is randomly selected from the set of  precoders for each PRG on PDSCH, where the PRG size for CQI calculation is configured by the higher layer parameter *pdsch-BundleSizeForCSI*.

If the UE is configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to 'cri-RI-CQI',

- if the UE is configured with higher layer parameter *non-PMI-PortIndication* contained in a *CSI-ReportConfig,* *r* ports are indicated in the order of layer ordering for rank *r* and each CSI-RS resource in the CSI resource setting is linked to the *CSI-ReportConfig* based on the order of the associated *NZP-CSI-RS-ResourceId* in the linked CSI resource setting for channel measurement given by higher layer parameter *resourcesForChannelMeasurement*. The configured higher layer parameter *non-PMI-PortIndication* contains a sequence  of port indices, where  are the CSI-RS port indices associated with rank ν and  where is the number of ports in the CSI-RS resource. The UE shall only report RI corresponding to the configured fields of *PortIndexFor8Ranks*.

- if the UE is not configured with higher layer parameter *non-PMI-PortIndication,* the UE assumes, for each CSI-RS resource in the CSI resource setting linked to the *CSI-ReportConfig*, that the CSI-RS port indices  are associated with ranks  where  is the number of ports in the CSI-RS resource.

- When calculating the CQI for a rank, the UE shall use the ports indicated for that rank for the selected CSI-RS resource. The precoder for the indicated ports shall be assumed to be the identity matrix scaled by .

If the UE is configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to 'cri-RSRP' or 'ssb-Index-RSRP',

- if the UE is configured with the higher layer parameter *groupBasedBeamReporting* set to 'disabled', the UE is not required to update measurements for more than 64 CSI-RS and/or SSB resources, and the UE shall report in a single report *nrofReportedRS* (higher layer configured) different CRI or SSBRI for each report setting.

- if the UE is configured with the higher layer parameter *groupBasedBeamReporting* set to 'enabled', the UE is not required to update measurements for more than 64 CSI-RS and/or SSB resources, and the UE shall report in a single reporting instance two different CRI or SSBRI for each report setting, where CSI-RS and/or SSB resources can be received simultaneously by the UE either with a single spatial domain receive filter, or with multiple simultaneous spatial domain receive filters.

If the UE is configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to 'cri-SINR' or 'ssb-Index-SINR',

- if the UE is configured with the higher layer parameter *groupBasedBeamReporting* set to 'disabled', the UE shall report [in a single report] *nrofReportedRSForSINR* (higher layer configured) different CRI or SSBRI for each report setting.

- if the UE is configured with the higher layer parameter *groupBasedBeamReporting* set to 'enabled', the UE shall report in a single reporting instance two different CRI or SSBRI for each report setting, [where CSI-RS and/or SSB resources can be received simultaneously by the UE either with a single spatial domain receive filter, or with multiple simultaneous spatial domain receive filters.]

If the UE is configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to 'cri-RSRP', 'cri-RI-PMI-CQI ', 'cri-RI-i1', 'cri-RI-i1-CQI', 'cri-RI-CQI' or 'cri-RI-LI-PMI-CQI', and resources are configured in the corresponding resource set for channel measurement, then the UE shall derive the CSI parameters other than CRI conditioned on the reported CRI, where CRI *k* (*k* ≥ 0) corresponds to the configured (*k*+1)-th entry of associated *nzp-CSI-RSResource* in the corresponding *nzp-CSI-RS-ResourceSet* for channel measurement, and (*k*+1)-th entry of associated *csi-IM-Resource* in the corresponding *csi-IM-ResourceSet* (if configured) If CSI-RS resources are configured, each resource shall contain at most 16 CSI-RS ports. If CSI-RS resources are configured, each resource shall contain at most 8 CSI-RS ports.

If the UE is configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to 'ssb-Index-RSRP', the UE shall report SSBRI, where SSBRI *k* (*k* ≥ 0) corresponds to the configured (*k*+1)-th entry of the associated *csi-SSB-ResourceList* in the corresponding *CSI-SSB-ResourceSet.*

If the UE is configured with a *CSI-ReportConfig* with the higher layer parameter *reportQuantity* set to 'cri-RI-PMI-CQI', ' cri-RI-i1', 'cri-RI-i1-CQI', 'cri-RI-CQI' or 'cri-RI-LI-PMI-CQI', then the UE is not expected to be configured with more than 8 CSI-RS resources in a CSI-RS resource set contained within a resource setting that is linked to the *CSI-ReportConfig*.

If the UE is configured with a *CSI-ReportConfig* with higher layer parameter *reportQuantity* set to 'cri-RSRP' or 'none' and the *CSI-ReportConfig* is linked to a resource setting configured with the higher layer parameter *resourceType* set to 'aperiodic', then the UE is not expected to be configured with more than 16 CSI-RS resources in a CSI-RS resource set contained within the resource setting.

The LI indicates which column of the precoder matrix of the reported PMI corresponds to the strongest layer of the codeword corresponding to the largest reported wideband CQI. If two wideband CQIs are reported and have equal value, the LI corresponds to strongest layer of the first codeword.

##### 5.2.1.4.3 L1-RSRP Reporting

For L1-RSRP computation

- the UE may be configured with CSI-RS resources, SS/PBCH Block resources or both CSI-RS and SS/PBCH block resources, when resource-wise quasi co-located with 'QCL-Type C' and 'QCL-TypeD' when applicable.

- the UE may be configured with CSI-RS resource setting up to 16 CSI-RS resource sets having up to 64 resources within each set. The total number of different CSI-RS resources over all resource sets is no more than 128.

For L1-RSRP reporting, if the higher layer parameter *nrofReportedRS* in *CSI-ReportConfig* is configured to be one, the reported L1-RSRP value is defined by a 7-bit value in the range [-140, -44] dBm with 1dB step size, if the higher layer parameter *nrofReportedRS* is configured to be larger than one, or if the higher layer parameter *groupBasedBeamReporting* is configured as 'enabled', the UE shall use differential L1-RSRP based reporting, where the largest measured value of L1-RSRP is quantized to a 7-bit value in the range [-140, -44] dBm with 1dB step size, and the differential L1-RSRP is quantized to a 4-bit value. The differential L1-RSRP value is computed with 2 dB step size with a reference to the largest measured L1-RSRP value which is part of the same L1-RSRP reporting instance. The mapping between the reported L1-RSRP value and the measured quantity is described in [11, TS 38.133].

##### 5.2.1.4.4 L1-SINR Reporting

For L1-SINR computation, for channel measurement the UE may be configured with NZP CSI-RS resources and/or SS/PBCH Block resources, for interference measurement the UE may be configured with NZP CSI-RS or CSI-IM resources.

- for channel measurement, the UE may be configured with CSI-RS resource setting up to 64 CSI-RS resources or up to 64 SS/PBCH Block resources.

For L1-SINR reporting, if the higher layer parameter *nrofReportedRSForSINR* in *CSI-ReportConfig* is configured to be one, the reported L1-SINR value is defined by a 7-bit value in the range [-23, 40] dB with 0.5 dB step size, and if the higher layer parameter *nrofReportedRSForSINR* is configured to be larger than one, the UE shall use differential L1-SINR based reporting, where the largest measured value of L1-SINR is quantized to a 7-bit value in the range [-23, 40] dB with 0.5 dB step size, and the differential L1-SINR is quantized to a 4-bit value. The differential L1-SINR is computed with 1 dB step size with a reference to the largest measured L1-SINR value which is part of the same L1-SINR reporting instance.

#### 5.2.1.5 Triggering/activation of CSI Reports and CSI-RS

##### 5.2.1.5.1 Aperiodic CSI Reporting/Aperiodic CSI-RS when the triggering PDCCH and the CSI-RS have the same numerology

For CSI-RS resource sets associated with Resource Settings configured with the higher layer parameter *resourceType* set to 'aperiodic', 'periodic', or 'semi-persistent', trigger states for Reporting Setting(s) (configured with the higher layer parameter *reportConfigType* set to 'aperiodic') and/or Resource Setting for channel and/or interference measurement on one or more component carriers are configured using the higher layer parameter *CSI-AperiodicTriggerStateList*. For aperiodic CSI report triggering, a single set of CSI triggering states are higher layer configured, wherein the CSI triggering states can be associated with any candidate DL BWP. A UE is not expected to receive more than one DCI with non-zero CSI request per slot. A UE is not expected to be configured with different *TCI-StateId*'s for the same aperiodic CSI-RS resource ID configured in multiple aperiodic CSI-RS resource sets with the same triggering offset in the same aperiodic trigger state. A UE is not expected to receive more than one aperiodic CSI report request for transmission in a given slot. When a UE is triggered with a CSI report for a DL BWP that is non-active when expecting to receive the most recent occasion, no later than the CSI reference resource, of the associated NZP CSI-RS, the UE is not expected to report the CSI for the non-active DL BWP and the CSI report associated with that BWP is omitted. When a UE is triggered with aperiodic NZP CSI-RS in a DL BWP that is non-active when expecting to receive the NZP CSI-RS, the UE is not expected to measure the aperiodic CSI-RS. In the carrier of the serving cell expecting to receive that associated NZP CSI-RS, if the active DL BWP when receiving the NZP CSI-RS is different from the active DL BWP when receiving the triggering DCI,

- the last symbol of the PDCCH span of the DCI carrying the BWP switching shall be no later than the last symbol of the PDCCH span of the DCI carrying the CSI trigger, irrespective of whether they are in the same carrier of a serving cell or not and irrespective of whether they are in the same SCS or not;

- the UE is not expected to have any other BWP switching in that carrier after the last symbol of the PDCCH span covering the DCI carrying the CSI trigger and before the first symbol of the triggered NZP CSI-RS or CSI-IM.

A trigger state is initiated using the *CSI request* field in DCI.

- When all the bits of *CSI request* field in DCI are set to zero, no CSI is requested.

- When the number of configured CSI triggering states in *CSI-AperiodicTriggerStateList* is greater than , where  is the number of bits in the DCI *CSI request* field, the UE receives a subselection indication, as described in clause 6.1.3.13 of [10, TS 38.321], used to map up to  trigger states to the codepoints of the *CSI request* field in DCI.  is configured by the higher layer parameter *reportTriggerSize* where . When the UE would transmit a PUCCH with HARQ-ACK information in slot *n* corresponding to the PDSCH carrying the subselection indication, the corresponding action in [10, TS 38.321] and UE assumption on the mapping of the selected CSI trigger state(s) to the codepoint(s) of DCI CSI request field shall be applied starting from the first slot that is after slot where ** is the SCS configuration for the PUCCH.

- When the number of CSI triggering states in *CSI-AperiodicTriggerStateList* is less than or equal to , the *CSI request* field in DCI directly indicates the triggering state.

- For each aperiodic CSI-RS resource in a CSI-RS resource set associated with each CSI triggering state, the UE is indicated the quasi co-location configuration of quasi co-location RS source(s) and quasi co-location type(s), as described in Clause 5.1.5, through higher layer signaling of *qcl-info* which contains a list of references to *TCI-State's* for the aperiodic CSI-RS resources associated with the CSI triggering state. If a *State* referred toin the list is configured with a reference to an RS associated with '*QCL-TypeD*', that RS may be an SS/PBCH block located in the same or different CC/DL BWP or a CSI-RS resource configured as periodic or semi-persistent located in the same or different CC/DL BWP.

- If the scheduling offset between the last symbol of the PDCCH carrying the triggering DCI and the first symbol of the aperiodic CSI-RS resources in a *NZP-CSI-RS-ResourceSet* configured without higher layer parameter *trs-Info* is smaller than the UE reported threshold *beamSwitchTiming,* as defined in [13, TS 38.306], when the reported value is one of the values of {14, 28, 48}, or is smaller than 48 when the reported value of *beamSwitchTiming* is one of the values of {224, 336}.

- if there is any other DL signal with an indicated TCI state in the same symbols as the CSI-RS, the UE applies the QCL assumption of the other DL signal also when receiving the aperiodic CSI-RS. The other DL signal refers to PDSCH scheduled with offset larger than or equal to the threshold *timeDurationForQCL,* as defined in [13, TS 38.306], aperiodic CSI-RS scheduled with offset larger than or equal to the UE reported threshold *beamSwitchTiming* when the reported value is one of the values {14,28,48}, aperiodic CSI-RS scheduled with offset larger than or equal to 48 when the reported value of *beamSwitchTiming* is one of the values {224, 336}, periodic CSI-RS, semi-persistent CSI-RS;

- else, when receiving the aperiodic CSI-RS, the UE applies the QCL assumption used for the CORESET associated with a monitored search space with the lowest *controlResourceSetId* in the latest slot in which one or more CORESETs within the active BWP of the serving cell are monitored.

- If the scheduling offset between the last symbol of the PDCCH carrying the triggering DCI and the first symbol of the aperiodic CSI-RS resources is equal to or greater than the UE reported threshold *beamSwitchTiming* when the reported value is one of the values of {14,28,48}, or is equal to or greater than 48 when the reported value of *beamSwitchTiming* is one of the values of {224, 336}, the UE is expected to apply the QCL assumptions in the indicated TCI states for the aperiodic CSI-RS resources in the CSI triggering state indicated by the CSI trigger field in DCI.

- A non-zero codepoint of the CSI request field in the DCI is mapped to a CSI triggering state according to the order of the associated positions of the up to trigger states in *CSI-AperiodicTriggerStateList* with codepoint '1' mapped to the triggering state in the first position.

For a UE configured with the higher layer parameter *CSI-AperiodicTriggerStateList*, if a Resource Setting linked to a *CSI-ReportConfig* has multiple aperiodic resource sets, only one of the aperiodic CSI-RS resource sets from the Resource Setting is associated with the trigger state, and the UE is higher layer configured per trigger state per Resource Setting to select the one CSI-IM/NZP CSI-RS resource set from the Resource Setting.

When aperiodic CSI-RS is used with aperiodic reporting, the CSI-RS offset is configured per resource set by the higher layer parameter *aperiodicTriggeringOffset*. The CSI-RS triggering offset has the values of {0, 1, 2, 3, 4, 16, 24} slots. If the UE is not configured with [*minimumSchedulingOffset*] for any DL or UL BWP and if all the associated trigger states do not have the higher layer parameter *qcl-Type* set to 'QCL-TypeD' in the corresponding TCI states , the CSI-RS triggering offset is fixed to zero. The aperiodic triggering offset of the CSI-IM follows offset of the associated NZP CSI-RS for channel measurement.

The UE does not expect that aperiodic CSI-RS is transmitted before the OFDM symbol(s) carrying its triggering DCI. When the minimum scheduling offset restriction is applied, UE is not expected to be triggered by CSI triggering state indicated by the CSI request field in DCI in which CSI-RS triggering offset is smaller than the currently applicable minimum scheduling offset restriction *K*0min.

If interference measurement is performed on aperiodic NZP CSI-RS, a UE is not expected to be configured with a different aperiodic triggering offset of the NZP CSI-RS for interference measurement from the associated NZP CSI-RS for channel measurement.

If the UE is configured with a single carrier for uplink, the UE is not expected to transmit more than one aperiodic CSI report triggered by different DCIs on overlapping OFDM symbols.

##### 5.2.1.5.1a Aperiodic CSI Reporting/Aperiodic CSI-RS when the triggering PDCCH and the CSI-RS have different numerologies

When the triggering PDCCH and the triggered aperiodic CSI-RS are of different numerologies, the behavior defined in 5.2.1.5.1 for the case where the numerologies are the same applies with the following exceptions:

When the triggering PDCCH and the triggered aperiodic CSI-RS are of different numerologies, the behavior defined in 5.2.1.5.1 for the case where the numerologies are the same applies with the following exceptions:

Beam switch timing:

- If the µPDCCH < µCSIRS

- If the scheduling offset between the last symbol of the PDCCH carrying the triggering DCI and the first symbol of the aperiodic CSI-RS resources in a *NZP-CSI-RS-ResourceSet* configured without higher layer parameter *trs-Info* and without the higher layer parameter *repetition* is smaller than the UE reported threshold *beamSwitchTiming* + *d* in PDCCH symbols*,* as defined in [13, TS 38.306], when the reported value is one of the values of {14, 28, 48}and where the beam switching timing delay *d* is defined in Table 5.2.1.5.1a-1,

- if there is any other DL signal with an indicated TCI state in the same symbols as the CSI-RS, the UE applies the QCL assumption of the other DL signal also when receiving the aperiodic CSI-RS. The other DL signal refers to PDSCH scheduled with offset larger than or equal to the threshold *timeDurationForQCL,* as defined in [13, TS 38.306], aperiodic CSI-RS scheduled with offset larger than or equal to the UE reported threshold *beamSwitchTiming* + *d* in PDCCH symbols when the reported value is one of the values {14,28,48}, periodic CSI-RS, semi-persistent CSI-RS;

- else,

- if at least one CORESET is configured for the BWP in which the aperiodic CSI-RS is to be received, when receiving the aperiodic CSI-RS, the UE applies the QCL assumption used for the CORESET associated with a monitored search space with the lowest *CORESET-ID* in the latest slot in which one or more CORESETs within the active BWP of the serving cell are monitored.

- else, when receiving the aperiodic CSI-RS, the UE applies the QCL assumption of the lowest-ID activated TCI state applicable to the PDSCH within the active BWP of the cell in which the CSI-RS is to be received.

- If the scheduling offset between the last symbol of the PDCCH carrying the triggering DCI and the first symbol of the aperiodic CSI-RS resources is equal to or greater than the UE reported threshold *beamSwitchTiming* + *d* in PDCCH symbols, when the reported value is one of the values of {14,28,48}, the UE is expected to apply the QCL assumptions in the indicated TCI states for the aperiodic CSI-RS resources in the CSI triggering state indicated by the CSI trigger field in DCI.

Table 5.2.1.5.1a-1: Additional beam switching timing delay *d*

|  |  |
| --- | --- |
| ***µPDCCH*** | ***d* [PDCCH symbols]** |
| 0 | 8 |
| 1 | 8 |
| 2 | 14 |

Aperiodic CSI-RS timing:

- When the aperiodic CSI-RS is used with aperiodic CSI reporting, the CSI-RS triggering offset *X* is configured per resource set by the higher layer parameter *aperiodicTriggeringOffset*. The CSI-RS triggering offset has the values of {0, 1,…31} slots when the µPDCCH < µCSIRS and {0, 1, 2, 3, 4, 16, 24} when the µPDCCH > µCSIRS.. The aperiodic CSI-RS is transmitted in a slot  where

*- n* is the slot containing the triggering DCI, *X* is the CSI-RS triggering offset in the numerology of CSI-RS according to the higher layer parameter *aperiodicTriggeringOffset*,

- and are the subcarrier spacing configurations for CSI-RS and PDCCH, respectively,

- *CAoffset* is a higher-layer configured *CA-slot-offset* for cross-carrier scheduling with non-SFN aligned carriers.

- If the µPDCCH < µCSIRS, the UE is expected to be able to measure the aperiodic CSI RS, if the CSI-RS starts no earlier than the first symbol of the CSI-RS carrier’s slot that starts at least *Ncsirs* PDCCH symbols after the end of the PDCCH triggering the aperiodic CSI-RS.

- If the µPDCCH > µCSIRS, the UE is expected to be able to measure the aperiodic CSI RS, if the CSI-RS starts no earlier than at least *Ncsirs* PDCCH symbols after the end of the PDCCH triggering the aperiodic CSI-RS.

Table 5.2.1.5.1a: *Ncsirs* as a function of the subcarrier spacing of the triggering PDCCH

|  |  |
| --- | --- |
| ***µPDCCH*** | ***Ncsirs* [symbols]** |
| 0 | 4 |
| 1 | 5 |
| 2 | 10 |
| 3 | [14] |

##### 5.2.1.5.2 Semi-persistent CSI/Semi-persistent CSI-RS

For semi-persistent reporting on PUSCH, a set of trigger states are higher layer configured by *CSI-SemiPersistentOnPUSCH-TriggerStateList* [for DCI format 0\_1 and *CSI-SemiPersistentOnPUSCH-TriggerStateList-ForDCIFormat0\_2* for DCI format 0\_2]*,* where the CSI request field in DCI scrambled with SP-CSI-RNTI activates one of the trigger states. A UE is not expected to receive a DCI scrambled with SP-CSI-RNTI activating one semi-persistent CSI report with the same CSI-ReportConfigId as in a semi-persistent CSI report which is activated by a previously received DCI scrambled with SP-CSI-RNTI.

For semi-persistent reporting on PUCCH, the PUCCH resource used for transmitting the CSI report are configured by *reportConfigType*. Semi-persistent reporting on PUCCH is activated by an activation command as described in clause 6.1.3.16 of [10, TS 38.321], which selects one of the semi-persistent Reporting Settings for use by the UE on the PUCCH. When the UE would transmit a PUCCH with HARQ-ACK information in slot *n* corresponding to the PDSCH carrying the activation command, the indicated semi-persistent Reporting Setting should be applied starting from the first slot that is after slot where ** is the SCS configuration for the PUCCH.

For a UE configured with CSI resource setting(s) where the higher layer parameter *resourceType* set to 'semiPersistent'.

- when a UE receives an activation command, as described in clause 6.1.3.12 of [10, TS 38.321], for CSI-RS resource set(s) for channel measurement and CSI-IM/NZP CSI-RS resource set(s) for interference measurement associated with configured CSI resource setting(s), and when the UE would transmit a PUCCH with HARQ-ACK information in slot *n* corresponding to the PDSCH carrying the selection command, the corresponding actions in [10, TS 38.321] and the UE assumptions (including QCL assumptions provided by a list of reference to *TCI-State's,* one per activated resource) on CSI-RS/CSI-IM transmission corresponding to the configured CSI-RS/CSI-IM resource configuration(s) shall be applied starting from the first slot that is after slot where ** is the SCS configuration for the PUCCH. If a *TCI-State* referred to in the list is configured with a reference to an RS associated with 'QCL-TypeD', that RS can be an SS/PBCH block, periodic or semi-persistent CSI-RS located in same or different CC/DL BWP.

- when a UE receives a deactivation command, as described in clause 6.1.3.12 of [10, TS 38.321], for activated CSI-RS/CSI-IM resource set(s) associated with configured CSI resource setting(s), and when the UE would transmit a PUCCH with HARQ-ACK information in slot *n* corresponding to the PDSCH carrying the deactivation command, the corresponding actions in [10, TS 38.321] and UE assumption on cessation of CSI-RS/CSI-IM transmission corresponding to the deactivated CSI-RS/CSI-IM resource set(s) shall apply starting from the first slot that is after slot where ** is the SCS configuration for the PUCCH.

A codepoint of the CSI request field in the DCI is mapped to a SP-CSI triggering state according to the order of the positions of the configured trigger states in *CSI-SemiPersistentOnPUSCH-TriggerStateList*, with codepoint '0' mapped to the triggering state in the first position. A UE validates, for semi-persistent CSI activation or release, a DL semi-persistent assignment PDCCH on a DCI only if the following conditions are met:

- the CRC parity bits of the DCI format are scrambled with a SP-CSI-RNTI provided by higher layer parameter *sp-CSI-RNTI*

- Special fields for the DCI format are set according to Table 5.2.1.5.2-1 or Table 5.2.1.5.2-2.

If validation is achieved, the UE considers the information in the DCI format as a valid activation or valid release of semi-persistent CSI transmission on PUSCH, and the UE activates or deactivates a CSI Reporting Setting indicated by CSI request field in the DCI. If validation is not achieved, the UE considers the DCI format as having been detected with a non-matching CRC.

Table 5.2.1.5.2-1: Special fields for semi-persistent CSI activation PDCCH validation

|  |  |
| --- | --- |
|  | DCI format 0\_1/0\_2 |
| HARQ process number | set to all '0's |
| Redundancy version | set to all '0's |

Table 5.2.1.5.2-2: Special fields for semi-persistent CSI deactivation PDCCH validation

|  |  |
| --- | --- |
|  | DCI format 0\_1/0\_2 |
| HARQ process number | set to all '0's |
| Modulation and coding scheme | set to all '1's |
| Resource block assignment | If higher layer configures RA type 0 only, set to all '0's;  If higher layer configures RA type 1 only, set to all '1's;  If higher layer configures dynamic switch between RA type 0 and 1, then if MSB is'0', set to all '0's; else, set to all '1's |
| Redundancy version | set to all '0's |

If the UE has an active semi-persistent CSI-RS/CSI-IM resource configuration, or an active semi-persistent ZP CSI-RS resource set configuration, and has not received a deactivation command, the activated semi-persistent CSI-RS/CSI-IM resource set or the activated semi-persistent ZP CSI-RS resource set configurations are considered to be active when the corresponding DL BWP is active, otherwise they are considered suspended.

If the UE is configured with carrier deactivation, the following configurations in the carrier in activated state would also be deactivated and need re-activation configuration(s): semi-persistent CSI-RS/CSI- IM resource, semi-persistent CSI reporting on PUCCH, semi-persistent SRS, semi-persistent ZP CSI-RS resource set.

#### 5.2.1.6 CSI processing criteria

The UE indicates the number of supported simultaneous CSI calculations . If a UE supports simultaneous CSI calculations it is said to have CSI processing units for processing CSI reports across all configured cells. If *L* CPUs are occupied for calculation of CSI reports in a given OFDM symbol, the UE has unoccupied CPUs. If *N* CSI reports start occupying their respective CPUs on the same OFDM symbol on which CPUs are unoccupied, where each CSI report corresponds to , the UE is not required to update the requested CSI reports with lowest priority (according to Clause 5.2.5), where is the largest value such that holds.

A UE is not expected to be configured with an aperiodic CSI trigger state containing more than Reporting Settings.Processing of a CSI report occupies a number of CPUs for a number of symbols as follows:

- for a CSI report with CSI-ReportConfig with higher layer parameter *reportQuantity* set to 'none' and *CSI-RS-ResourceSet* with higher layer parameter *trs-Info* configured

- for a CSI report with *CSI-ReportConfig* with higher layer parameter *reportQuantity* set to 'cri-RSRP', 'ssb-Index-RSRP', 'cri-SINR', 'ssb-Index-SINR' or 'none' (and *CSI-RS-ResourceSet* with higher layer parameter *trs-Info* not configured)

- for a CSI report with *CSI-ReportConfig* with higher layer parameter *reportQuantity* set to 'cri-RI-PMI-CQI', 'cri-RI-i1', 'cri-RI-i1-CQI', 'cri-RI-CQI', or 'cri-RI-LI-PMI-CQI',

- if a CSI report is aperiodically triggered without transmitting a PUSCH with either transport block or HARQ-ACK or both when *L* = 0 CPUs are occupied, where the CSI corresponds to a single CSI with wideband frequency-granularity and to at most 4 CSI-RS ports in a single resource without CRI report and where *codebookType* is set to 'typeI-SinglePanel' or where *reportQuantity* is set to 'cri-RI-CQI', ,

- otherwise, , where is the number of CSI-RS resources in the CSI-RS resource set for channel measurement.

For a CSI report with *CSI-ReportConfig* with higher layer parameter *reportQuantity* not set to 'none', the CPU(s) are occupied for a number of OFDM symbols as follows:

- A periodic or semi-persistent CSI report (excluding an initial semi-persistent CSI report on PUSCH after the PDCCH triggering the report) occupies CPU(s) from the first symbol of the earliest one of each CSI-RS/CSI-IM/SSB resource for channel or interference measurement, respective latest CSI-RS/CSI-IM/SSB occasion no later than the corresponding CSI reference resource, until the last symbol of the PUSCH/PUCCH carrying the report.

- An aperiodic CSI report occupies CPU(s) from the first symbol after the PDCCH triggering the CSI report until the last symbol of the PUSCH carrying the report.

- An initial semi-persistent CSI report on PUSCH after the PDCCH trigger occupies CPU(s) from the first symbol after the PDCCH until the last symbol of the PUSCH carrying the report.

For a CSI report with *CSI-ReportConfig* with higher layer parameter *reportQuantity* set to 'none' and *CSI-RS-ResourceSet* with higher layer parameter *trs-Info* is not configured, the CPU(s) are occupied for a number of OFDM symbols as follows:

- A semi-persistent CSI report (excluding an initial semi-persistent CSI report on PUSCH after the PDCCH triggering the report) occupies CPU(s) from the first symbol of the earliest one of each transmission occasion of periodic or semi-persistent CSI-RS/SSB resource for channel measurement for L1-RSRP computation, until symbols after the last symbol of the latest one of the CSI-RS/SSB resource for channel measurement for L1-RSRP computation in each transmission occasion.

- An aperiodic CSI report occupies CPU(s) from the first symbol after the PDCCH triggering the CSI report until the last symbol between symbols after the first symbol after the PDCCH triggering the CSI report and symbols after the last symbol of the latest one of each CSI-RS/SSB resource for channel measurement for L1-RSRP computation.

where are defined in the table 5.4-2.

In any slot, the UE is not expected to have more active CSI-RS ports or active CSI-RS resources than reported as capability. NZP CSI-RS resource is active in a duration of time defined as follows. For aperiodic CSI-RS, starting from the end of the PDCCH containing the request and ending at the end of the PUSCH containing the report associated with this aperiodic CSI-RS. For semi-persistent CSI-RS, starting from the end of when the activation command is applied, and ending at the end of when the deactivation command is applied. For periodic CSI-RS, starting when the periodic CSI-RS is configured by higher layer signalling, and ending when the periodic CSI-RS configuration is released. If a CSI-RS resource is referred by *N* CSI reporting settings, the CSI-RS resource and the CSI-RS ports within the CSI-RS resource are counted *N* times.

### 5.2.2 Channel state information

#### 5.2.2.1 Channel quality indicator (CQI)

The CQI indices and their interpretations are given in Table 5.2.2.1-2 or Table 5.2.2.1-4 for reporting CQI based on QPSK, 16QAM and 64QAM. The CQI indices and their interpretations are given in Table 5.2.2.1-3 for reporting CQI based on QPSK, 16QAM, 64QAM and 256QAM.

Based on an unrestricted observation interval in time unless specified otherwise in this Clause, and an unrestricted observation interval in frequency, the UE shall derive for each CQI value reported in uplink slot *n* the highest CQI index which satisfies the following condition:

- A single PDSCH transport block with a combination of modulation scheme, target code rate and transport block size corresponding to the CQI index, and occupying a group of downlink physical resource blocks termed the CSI reference resource, could be received with a transport block error probability not exceeding:

- 0.1, if the higher layer parameter *cqi-Table* in *CSI-ReportConfig* configures 'table1' (corresponding to Table 5.2.2.1-2), or 'table2' (corresponding to Table 5.2.2.1-3), or

- 0.00001, if the higher layer parameter *cqi-Table* in *CSI-ReportConfig* configures 'table3' (corresponding to Table 5.2.2.1-4).

If a UE is not configured with higher layer parameter *timeRestrictionForChannelMeasurements*, the UE shall derive the channel measurements for computing CSI value reported in uplink slot n based on only the NZP CSI-RS, no later than the CSI reference resource, (defined in TS 38.211[4]) associated with the CSI resource setting.

If a UE is configured with higher layer parameter *timeRestrictionForChannelMeasurements* in*CSI-ReportConfig*, the UE shall derive the channel measurements for computing CSI reported in uplink slot n based on only the most recent, no later than the CSI reference resource, occasion of NZP CSI-RS (defined in [4, TS 38.211]) associated with the CSI resource setting.

If a UE is not configured with higher layer parameter *timeRestrictionForInterferenceMeasurements*, the UE shall derive the interference measurements for computing CSI value reported in uplink slot n based on only the CSI-IM and/or NZP CSI-RS for interference measurement no later than the CSI reference resource associated with the CSI resource setting.

If a UE is configured with higher layer parameter *timeRestrictionForInterferenceMeasurements* in *CSI-ReportConfig*, the UE shall derive the interference measurements for computing the CSI value reported in uplink slot n based on the most recent, no later than the CSI reference resource, occasion of CSI-IM and/or NZP CSI-RS for interference measurement (defined in [4, TS 38.211]) associated with the CSI resource setting.

For each sub-band index *s,* a 2-bit sub-band differential CQI is defined as:

- Sub-band Offset level (*s*) = sub-band CQI index (*s*) - wideband CQI index.

The mapping from the 2-bit sub-band differential CQI values to the offset level is shown in Table 5.2.2.1-1

Table 5.2.2.1-1: Mapping sub-band differential CQI value to offset level

|  |  |
| --- | --- |
| Sub-band differential CQI value | Offset level |
| 0 | 0 |
| 1 | 1 |
| 2 | ≥ 2 |
| 3 | ≤-1 |

A combination of modulation scheme and transport block size corresponds to a CQI index if:

- the combination could be signaled for transmission on the PDSCH in the CSI reference resource according to the Transport Block Size determination described in Clause 5.1.3.2, and

- the modulation scheme is indicated by the CQI index, and

- the combination of transport block size and modulation scheme when applied to the reference resource results in the effective channel code rate which is the closest possible to the code rate indicated by the CQI index. If more than one combination of transport block size and modulation scheme results in an effective channel code rate equally close to the code rate indicated by the CQI index, only the combination with the smallest of such transport block sizes is relevant.

Table 5.2.2.1-2: 4-bit CQI Table

|  |  |  |  |
| --- | --- | --- | --- |
| CQI index | modulation | code rate x 1024 | efficiency |
| 0 | out of range | | |
| 1 | QPSK | 78 | 0.1523 |
| 2 | QPSK | 120 | 0.2344 |
| 3 | QPSK | 193 | 0.3770 |
| 4 | QPSK | 308 | 0.6016 |
| 5 | QPSK | 449 | 0.8770 |
| 6 | QPSK | 602 | 1.1758 |
| 7 | 16QAM | 378 | 1.4766 |
| 8 | 16QAM | 490 | 1.9141 |
| 9 | 16QAM | 616 | 2.4063 |
| 10 | 64QAM | 466 | 2.7305 |
| 11 | 64QAM | 567 | 3.3223 |
| 12 | 64QAM | 666 | 3.9023 |
| 13 | 64QAM | 772 | 4.5234 |
| 14 | 64QAM | 873 | 5.1152 |
| 15 | 64QAM | 948 | 5.5547 |

Table 5.2.2.1-3: 4-bit CQI Table 2

|  |  |  |  |
| --- | --- | --- | --- |
| CQI index | modulation | code rate x 1024 | efficiency |
| 0 | out of range | | |
| 1 | QPSK | 78 | 0.1523 |
| 2 | QPSK | 193 | 0.3770 |
| 3 | QPSK | 449 | 0.8770 |
| 4 | 16QAM | 378 | 1.4766 |
| 5 | 16QAM | 490 | 1.9141 |
| 6 | 16QAM | 616 | 2.4063 |
| 7 | 64QAM | 466 | 2.7305 |
| 8 | 64QAM | 567 | 3.3223 |
| 9 | 64QAM | 666 | 3.9023 |
| 10 | 64QAM | 772 | 4.5234 |
| 11 | 64QAM | 873 | 5.1152 |
| 12 | 256QAM | 711 | 5.5547 |
| 13 | 256QAM | 797 | 6.2266 |
| 14 | 256QAM | 885 | 6.9141 |
| 15 | 256QAM | 948 | 7.4063 |

Table 5.2.2.1-4: 4-bit CQI Table 3

|  |  |  |  |
| --- | --- | --- | --- |
| CQI index | modulation | code rate x 1024 | efficiency |
| 0 | out of range | | |
| 1 | QPSK | 30 | 0.0586 |
| 2 | QPSK | 50 | 0.0977 |
| 3 | QPSK | 78 | 0.1523 |
| 4 | QPSK | 120 | 0.2344 |
| 5 | QPSK | 193 | 0.3770 |
| 6 | QPSK | 308 | 0.6016 |
| 7 | QPSK | 449 | 0.8770 |
| 8 | QPSK | 602 | 1.1758 |
| 9 | 16QAM | 378 | 1.4766 |
| 10 | 16QAM | 490 | 1.9141 |
| 11 | 16QAM | 616 | 2.4063 |
| 12 | 64QAM | 466 | 2.7305 |
| 13 | 64QAM | 567 | 3.3223 |
| 14 | 64QAM | 666 | 3.9023 |
| 15 | 64QAM | 772 | 4.5234 |

##### 5.2.2.1.1 (void)

#### 5.2.2.2 Precoding matrix indicator (PMI)

##### 5.2.2.2.1 Type I Single-Panel Codebook

For 2 antenna ports {3000, 3001} and the UE configured with higher layer parameter *codebookType* set to 'typeI-SinglePanel' each PMI value corresponds to a codebook index given in Table 5.2.2.2.1-1. The UE is configured with the higher layer parameter *twoTX-CodebookSubsetRestriction*. The bitmap parameter *twoTX-CodebookSubsetRestriction* forms the bit sequence  where  is the LSB and  is the MSB and where a bit value of zero indicates that PMI reporting is not allowed to correspond to the precoder associated with the bit. Bits 0 to 3 are associated respectively with the codebook indices 0 to 3 for  layer, and bits 4 and 5 are associated respectively with the codebook indices 0 and 1 for  layers.

Table 5.2.2.2.1-1: Codebooks for 1-layer and 2-layer CSI reporting using antenna ports 3000 to 3001

|  |  |  |
| --- | --- | --- |
| Codebook index | Number of layers | |
| 1 | 2 |
| 0 |  |  |
| 1 |  |  |
| 2 |  | - |
| 3 |  | - |

For 4 antenna ports {3000, 3001, 3002, 3003}, 8 antenna ports {3000, 3001, …, 3007}, 12 antenna ports {3000, 3001, …, 3011}, 16 antenna ports {3000, 3001, …, 3015}, 24 antenna ports {3000, 3001, …, 3023}, and 32 antenna ports {3000, 3001, …, 3031}, and the UE configured with higher layer parameter *codebookType* set to 'typeI-SinglePanel', except when the number of layers (where  is the associated RI value), each PMI value corresponds to three codebook indices ,,. When the number of layers , each PMI value corresponds to four codebook indices ,,,. The composite codebook index  is defined by



The codebooks for 1-8 layers are given respectively in Tables 5.2.2.2.1-5, 5.2.2.2.1-6, 5.2.2.2.1-7, 5.2.2.2.1-8, 5.2.2.2.1-9, 5.2.2.2.1-10, 5.2.2.2.1-11, and 5.2.2.2.1-12. The mapping from  to  and  for 2-layer reporting is given in Table 5.2.2.2.1-3. The mapping from  to  and  for 3-layer and 4-layer reporting when **** is given in Table 5.2.2.2.1-4. The quantities , , , , and  are given by



- The values of and  are configured with the higher layer parameter *n1-n2*, respectively. The supported configurations of  for a given number of CSI-RS ports and the corresponding values of  are given in Table 5.2.2.2.1-2. The number of CSI-RS ports, **, is.

- UE shall only use  and shall not report  if the value of *N2* is 1.

The bitmap parameter *n1-n2* forms the bit sequence  where  is the LSB and  is the MSB and where a bit value of zero indicates that PMI reporting is not allowed to correspond to any precoder associated with the bit. The number of bits is given by . Except when the number of layers and the number of antenna ports is 16, 24, or 32, bit  is associated with all precoders based on the quantity , , . When the number of layers and the number of antenna ports is 16, 24, or 32,

- bits , , and  are each associated with all precoders based on the quantity , , ;

- if one or more of the associated bits is zero, then PMI reporting is not allowed to correspond to any precoder based on .

For UE configured with higher layer parameter *codebookType* set to 'typeI-SinglePanel', the bitmap parameter *typeI-SinglePanel-ri‑Restriction* forms the bit sequence  where  is the LSB and  is the MSB. When  is zero, , PMI and RI reporting are not allowed to correspond to any precoder associated with  layers.

For UE configured with higher layer parameter *reportQuantity* set to 'cri-RI-i1-CQI', the bitmap parameter *typeI-SinglePanel-codebookSubsetRestriction-i2* forms the bit sequence , where is the LSB and is the MSB. The bit is associated with precoders corresponding to codebook index . When is zero, the randomly selected precoder for CQI calculation is not allowed to correspond to any precoder associated with the bit .



Table 5.2.2.2.1-2: Supported configurations of and 

|  |  |  |
| --- | --- | --- |
| Number of  CSI-RS antenna ports, |  |  |
|
| 4 | (2,1) | (4,1) |
| 8 | (2,2) | (4,4) |
| (4,1) | (4,1) |
| 12 | (3,2) | (4,4) |
| (6,1) | (4,1) |
| 16 | (4,2) | (4,4) |
| (8,1) | (4,1) |
| 24 | (4,3) | (4,4) |
| (6,2) | (4,4) |
| (12,1) | (4,1) |
| 32 | (4,4) | (4,4) |
| (8,2) | (4,4) |
| (16,1) | (4,1) |

Table 5.2.2.2.1-3: Mapping of  to  and  for 2-layer CSI reporting

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | |  | |  | |  | |
|  |  |  |  |  |  |  |  |
| 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| 1 |  | 0 |  | 0 |  | 0 |  | 0 |
| 2 | 0 |  | 0 |  |  |  |  | 0 |
| 3 |  | 0 |  |  |  |  |  | 0 |

Table 5.2.2.2.1-4: Mapping of  to  and  for 3-layer and 4-layer CSI reporting when 

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | |  | |  | |  | |  | |
|  |  |  |  |  |  |  |  |  |  |
| 0 |  | 0 |  | 0 |  | 0 |  | 0 |  | 0 |
| 1 |  |  |  | 0 |  | 0 | 0 |  | 0 |  |
| 2 |  |  |  | 0 |  | 0 |  |  |  |  |
| 3 |  |  |  |  |  | 0 |  |  |  | 0 |

Table 5.2.2.2.1-5: Codebook for 1-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |
| --- | --- | --- | --- |
| *codebookMode* = 1 | | | |
|  |  |  |  |
|  |  |  |  |
| where . | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *codebookMode* = 2, | | | | | |
|  |  |  | | | |
| 0 | 1 | 2 | 3 |
|  |  |  |  |  |  |
|  |  |  | | | |
| 4 | 5 | 6 | 7 |
|  |  |  |  |  |  |
|  |  |  | | | |
| 8 | 9 | 10 | 11 |
|  |  |  |  |  |  |
|  |  |  | | | |
| 12 | 13 | 14 | 15 |
|  |  |  |  |  |  |
| where . | | | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *codebookMode =* 2, | | | | | |
|  |  |  | | | |
| 0 | 1 | 2 | 3 |
|  |  |  |  |  |  |
|  |  |  | | | |
| 4 | 5 | 6 | 7 |
|  |  |  |  |  |  |
|  |  |  | | | |
| 8 | 9 | 10 | 11 |
|  |  |  |  |  |  |
|  |  |  | | | |
| 12 | 13 | 14 | 15 |
|  |  |  |  |  |  |
| where . | | | | | |

Table 5.2.2.2.1-6: Codebook for 2-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |
| --- | --- | --- | --- |
| *codebookMode* = 1 | | | |
|  |  |  |  |
|  |  |  |  |
| where .  and the mapping from  to  and  is given in Table 5.2.2.2.1-3. | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| *codebookMode =* 2, | | | |
|  |  |  | |
| 0 | 1 |
|  |  |  |  |
|  |  |  | |
| 2 | 3 |
|  |  |  |  |
|  |  |  | |
| 4 | 5 |
|  |  |  |  |
|  |  |  | |
| 6 | 7 |
|  |  |  |  |
| where .  and the mapping from  to  and  is given in Table 5.2.2.2.1-3. | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *codebookMode =* 2, | | | | | |
|  |  |  | | | |
| 0 | 1 | 2 | 3 |
|  |  |  |  |  |  |
|  |  |  | | | |
| 4 | 5 | 6 | 7 |
|  |  |  |  |  |  |
| where .  and the mapping from  to  is given in Table 5.2.2.2.1-3. | | | | | |

Table 5.2.2.2.1-7: Codebook for 3-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |
| --- | --- | --- | --- |
| *codebookMode =* 1-2, | | | |
|  |  |  |  |
|  |  |  |  |
| where .  and the mapping from  to  and  is given in Table 5.2.2.2.1-4. | | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 1-2, | | | | |
|  |  |  |  |  |
|  |  |  |  |  |
| where . | | | | |

Table 5.2.2.2.1-8: Codebook for 4-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |
| --- | --- | --- | --- |
| *codebookMode =* 1-2, | | | |
|  |  |  |  |
|  |  |  |  |
| where .  and the mapping from  to  and  is given in Table 5.2.2.2.1-4. | | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 1-2, | | | | |
|  |  |  |  |  |
|  |  |  |  |  |
| where . | | | | |

Table 5.2.2.2.1-9: Codebook for 5-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 1-2 | | | | |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| where . | | | | |

Table 5.2.2.2.1-10: Codebook for 6-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 1-2 | | | | |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| where . | | | | |

Table 5.2.2.2.1-11: Codebook for 7-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 1-2 | | | | |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| where . | | | | |

Table 5.2.2.2.1-12: Codebook for 8-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 1-2 | | | | |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| where . | | | | |

##### 5.2.2.2.2 Type I Multi-Panel Codebook

For 8 antenna ports {3000, 3001, …, 3007}, 16 antenna ports {3000, 3001, …, 3015}, and 32 antenna ports {3000, 3001, …, 3031}, and the UE configured with higher layer parameter *codebookType* set to 'typeI-MultiPanel',

- The values of , and  are configured with the higher layer parameters *ng-n1-n2*. The supported configurations of  for a given number of CSI-RS ports and the corresponding values of  are given in Table 5.2.2.2.2-1. The number of CSI-RS ports, **, is .

- When , *codebookMode* shall be set to either '1' or '2'. When , *codebookMode* shall be set to '1'.

The bitmap parameter *ng-n1-n2* forms the bit sequence  where  is the LSB and  is the MSB and where a bit value of zero indicates that PMI reporting is not allowed to correspond to any precoder associated with the bit. The number of bits is given by . Bit  is associated with all precoders based on the quantity , , , as defined below. The bitmap parameter *ri‑Restriction* forms the bit sequence  where  is the LSB and  is the MSB. When  is zero, , PMI and RI reporting are not allowed to correspond to any precoder associated with  layers.

Table 5.2.2.2.2-1: Supported configurations of  and 

|  |  |  |
| --- | --- | --- |
| Number of  CSI-RS antenna ports, |  |  |
|
| 8 | (2,2,1) | (4,1) |
| 16 | (2,4,1) | (4,1) |
| (4,2,1) | (4,1) |
| (2,2,2) | (4,4) |
| 32 | (2,8,1) | (4,1) |
| (4,4,1) | (4,1) |
| (2,4,2) | (4,4) |
| (4,2,2) | (4,4) |

Each PMI value corresponds to the codebook indices  and , where  is the vector



and  is the associated RI value. When *codebookMode* is set to '1',  is

.

When *codebookMode* is set to '2',  and  are

.

The mapping from  to  and  for 2-layer reporting is given in Table 5.2.2.2.1-3. The mapping from  to  and  for 3-layer and 4-layer reporting is given in Table 5.2.2.2.2-2.

- UE shall only use  and shall not report  if the value of *N2* is 1.

Table 5.2.2.2.2-2: Mapping of  to  and  for 3-layer and 4-layer CSI reporting

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | |  | |  | |  | |  | |
|  |  |  |  |  |  |  |  |  |  |
| 0 |  | 0 |  | 0 |  | 0 |  | 0 |  | 0 |
| 1 |  |  |  | 0 |  | 0 | 0 |  | 0 |  |
| 2 |  |  |  | 0 |  | 0 |  |  |  |  |
| 3 |  |  |  |  |  | 0 |  |  |  | 0 |

Several quantities are used to define the codebook elements. The quantities , , , , and  are given by



Furthermore, the quantities  and  () are given by



where

,

and the quantities  and  () are given by



where

.

The codebooks for 1-4 layers are given respectively in Tables 5.2.2.2.2-3, 5.2.2.2.2-4, 5.2.2.2.2-5, and 5.2.2.2.2-6.

Table 5.2.2.2.2-3: Codebook for 1-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 1, | | | | |
|  |  | , |  |  |
|  |  |  |  |  |
| where . | | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *codebookMode* = 2, | | | | | |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| where . | | | | | |

Table 5.2.2.2.2-4: Codebook for 2-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 1, | | | | |
|  |  | , |  |  |
|  |  |  |  |  |
| where  and the mapping from  to  and  is given in Table 5.2.2.2.1-3. | | | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 2, | | | | |
|  |  |  |  |  |
|  |  |  |  |  |
| where  and the mapping from  to  and  is given in Table 5.2.2.2.1-3. | | | | |

Table 5.2.2.2.2-5: Codebook for 3-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 1, | | | | |
|  |  | , |  |  |
|  |  |  |  |  |
| where  and the mapping from  to  and  is given in Table 5.2.2.2.2-2. | | | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 2, | | | | |
|  |  |  |  |  |
|  |  |  |  |  |
| where  and the mapping from  to  and  is given in Table 5.2.2.2.2-2. | | | | |

Table 5.2.2.2.2-6: Codebook for 4-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI-RS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 1, | | | | |
|  |  | , |  |  |
|  |  |  |  |  |
| where  and the mapping from  to  and  is given in Table 5.2.2.2.2-2. | | | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *codebookMode* = 2, | | | | |
|  |  |  |  |  |
|  |  |  |  |  |
| where  and the mapping from  to  and  is given in Table 5.2.2.2.2-2. | | | | |

##### 5.2.2.2.3 Type II Codebook

For 4 antenna ports {3000, 3001, …, 3003}, 8 antenna ports {3000, 3001, …, 3007}, 12 antenna ports {3000, 3001, …, 3011}, 16 antenna ports {3000, 3001, …, 3015}, 24 antenna ports {3000, 3001, …, 3023}, and 32 antenna ports {3000, 3001, …, 3031}, and the UE configured with higher layer parameter *codebookType* set to 'typeII'

- The values of and  are configured with the higher layer parameter *n1-n2-codebookSubsetRestriction*. The supported configurations of  for a given number of CSI-RS ports and the corresponding values of  are given in Table 5.2.2.2.1-2. The number of CSI-RS ports, **, is .

- The value of  is configured with the higher layer parameter *numberOfBeams*, where  when  and  when .

- The value of  is configured with the higher layer parameter *phaseAlphabetSize*, where .

- The UE is configured with the higher layer parameter *subbandAmplitude* set to 'true' or 'false'.

- The UE shall not report RI > 2.

When , where  is the associated RI value, each PMI value corresponds to the codebook indices  and  where

..

The  vectors combined by the codebook are identified by the indices  and , where



.

Let



and

 .

where the values of  are given in Table 5.2.2.2.3-1.

Then the elements of  and  are found from using the algorithm:



for 

Find the largest  in Table 5.2.2.2.3-1 such that 











When  and  are known,  is found using:

 where the indices  are assigned such that  increases as  increases

, where  is given in Table 5.2.2.2.3-1.

- If ,  and  for , and  is not reported.

- When ,  and , and  is not reported.

- When  and ,  and , and  is not reported.

- When  and ,  and, and  is not reported.

Table 5.2.2.2.3-1: Combinatorial coefficients 

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 1 | 2 | 3 | 4 |
| 0 | 0 | 0 | 0 | 0 |
| 1 | 1 | 0 | 0 | 0 |
| 2 | 2 | 1 | 0 | 0 |
| 3 | 3 | 3 | 1 | 0 |
| 4 | 4 | 6 | 4 | 1 |
| 5 | 5 | 10 | 10 | 5 |
| 6 | 6 | 15 | 20 | 15 |
| 7 | 7 | 21 | 35 | 35 |
| 8 | 8 | 28 | 56 | 70 |
| 9 | 9 | 36 | 84 | 126 |
| 10 | 10 | 45 | 120 | 210 |
| 11 | 11 | 55 | 165 | 330 |
| 12 | 12 | 66 | 220 | 495 |
| 13 | 13 | 78 | 286 | 715 |
| 14 | 14 | 91 | 364 | 1001 |
| 15 | 15 | 105 | 455 | 1365 |

The strongest coefficient on layer  is identified by .

The amplitude coefficient indicators  and  are



for . The mapping from  to the amplitude coefficient  is given in Table 5.2.2.2.3-2 and the mapping from  to the amplitude coefficient  is given in Table 5.2.2.2.3-3. The amplitude coefficients are represented by



for .

Table 5.2.2.2.3-2: Mapping of elements of :  to 

|  |  |
| --- | --- |
|  |  |
|
| 0 |  |
| 1 |  |
| 2 |  |
| 3 |  |
| 4 |  |
| 5 |  |
| 6 |  |
| 7 |  |

Table 5.2.2.2.3-3: Mapping of elements of :  to 

|  |  |
| --- | --- |
|  |  |
|
| 0 |  |
| 1 |  |

The phase coefficient indicators are



for .

The amplitude and phase coefficient indicators are reported as follows:

- The indicators , , and  (). , , and  are not reported for .

- The remaining  elements of  () are reported, where . Let  () be the number of elements of  that satisfy .

- The remaining  elements of  and  () are reported as follows:

- When *subbandAmplitude* is set to 'false',

-  for , and .  is not reported for .

- For , the elements of  corresponding to the coefficients that satisfy , , as determined by the reported elements of , are reported, where  and the remaining  elements of  are not reported and are set to .

- When *subbandAmplitude* is set to 'true',

- For , the elements of  and  corresponding to the  strongest coefficients (excluding the strongest coefficient indicated by), as determined by the corresponding reported elements of , are reported, where and . The values of  are given in Table 5.2.2.2.3-4. The remaining  elements of  are not reported and are set to . The elements of  corresponding to the  weakest non-zero coefficients are reported, where . The remaining  elements of  are not reported and are set to .

- When two elements,  and , of the reported elements of  are identical (), then element  is prioritized to be included in the set of the  strongest coefficients for  and  () reporting.

Table 5.2.2.2.3-4: Full resolution subband coefficients when *subbandAmplitude* is set to 'true'

|  |  |
| --- | --- |
|  |  |
|
| 2 | 4 |
| 3 | 4 |
| 4 | 6 |

The codebooks for 1-2 layers are given in Table 5.2.2.2.3-5, where the indices  and  are given by



for , and the quantities , , and  are given by

.

Table 5.2.2.2.3-5: Codebook for 1-layer and 2-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI‑RS

|  |  |
| --- | --- |
| Layers |  |
|
|  |  |
|  |  |
| where ,  and the mappings from  to , , , , , and  , and from to , ,  and  are as described above, including the ranges of the constituent indices of  and . | |

When the UE is configured with higher layer parameter *codebookType* set to 'typeII', thebitmap parameter *typeII-RI‑Restriction* forms the bit sequence  where  is the LSB and  is the MSB. When  is zero, , PMI and RI reporting are not allowed to correspond to any precoder associated with  layers. The bitmap parameter *n1-n2‑codebookSubsetRestriction* forms the bit sequence where bit sequences , and are concatenated to form . To define  and , first define the  vector groups  as



for

.

The UE shall be configured with restrictions for 4 vector groups indicated by  for  and identified by the group indices



for , where the indices are assigned such that  increases as  increases. The remaining vector groups are not restricted.

- If ,  for , and  is empty.

- If ,  is the binary representation of the integer  where  is the MSB and  is the LSB. is found using:

,

where  is defined in Table 5.2.2.2.3-1. The group indices  and indicators  for  may be found from  using the algorithm:



for 

Find the largest  such that 











The bit sequence  is the concatenation of the bit sequences  for , corresponding to the group indices . The bit sequence  is defined as



Bits  indicate the maximum allowed amplitude coefficient  for the vector in group  indexed by , where the maximum amplitude coefficients are given in Table 5.2.2.2.3-6. A UE that does not report parameter *amplitudeSubsetRestriction* = 'supported' in its capability signaling is not expected to be configured with  = 01 or 10.

Table 5.2.2.2.3-6: Maximum allowed amplitude coefficients for restricted vectors

|  |  |
| --- | --- |
| Bits | Maximum Amplitude Coefficient |
|
| 00 |  |
| 01 |  |
| 10 |  |
| 11 |  |

##### 5.2.2.2.4 Type II Port Selection Codebook

For 4 antenna ports {3000, 3001, …, 3003}, 8 antenna ports {3000, 3001, …, 3007}, 12 antenna ports {3000, 3001, …, 3011}, 16 antenna ports {3000, 3001, …, 3015}, 24 antenna ports {3000, 3001, …, 3023}, and 32 antenna ports {3000, 3001, …, 3031}, and the UE configured with higher layer parameter *codebookType* set to 'typeII-PortSelection'

- The number of CSI-RS ports is given by **as configured by higher layer parameter *nrofPorts*.

- The value of  is configured with the higher layer parameter *numberOfBeams* , where  when  and  when .

- The value of  is configured with the higher layer parameter *portSelectionSamplingSize*, where  and .

- The value of  is configured with the higher layer parameter *phaseAlphabetSize*, where .

- The UE is configured with the higher layer parameter *subbandAmplitude* set to 'true' or 'false'.

- The UE shall not report RI > 2.

The UE is also configured with the higher layer parameter *typeII-PortSelectionRI‑Restriction*. The bitmap parameter *typeII-PortSelectionRI‑Restriction* forms the bit sequence  where  is the LSB and  is the MSB. When  is zero, , PMI and RI reporting are not allowed to correspond to any precoder associated with  layers.

When , where  is the associated RI value, each PMI value corresponds to the codebook indices  and  where

.

The  antenna ports per polarization are selected by the index , where

.

The strongest coefficient on layer  is identified by .

The amplitude coefficient indicators  and  are



for . The mapping from  to the amplitude coefficient  is given in Table 5.2.2.2.3-2 and the mapping from  to the amplitude coefficient  is given in Table 5.2.2.2.3-3. The amplitude coefficients are represented by



for .

The phase coefficient indicators are



for .

The amplitude and phase coefficient indicators are reported as follows:

- The indicators , , and  (). , , and  are not reported for .

- The remaining  elements of  () are reported, where . Let  () be the number of elements of that satisfy .

- The remaining  elements of  and  () are reported as follows:

- When *subbandAmplitude* is set to 'false',

-  for , and .  is not reported for .

- For , the  elements of  corresponding to the coefficients that satisfy , , as determined by the reported elements of , are reported, where  and the remaining  elements of  are not reported and are set to .

- When *subbandAmplitude* is set to 'true',

- For , the elements of  and  corresponding to the  strongest coefficients (excluding the strongest coefficient indicated by), as determined by the corresponding reported elements of , are reported, where and . The values of  are given in Table 5.2.2.2.3-4. The remaining  elements of  are not reported and are set to . The elements of  corresponding to the  weakest non-zero coefficients are reported, where . The remaining  elements of  are not reported and are set to .

- When two elements,  and , of the reported elements of  are identical (), then element  is prioritized to be included in the set of the  strongest coefficients for  and  () reporting.

The codebooks for 1-2 layers are given in Table 5.2.2.2.4-1, where the quantity  is given by



and  is a -element column vector containing a value of 1 in element  and zeros elsewhere (where the first element is element 0).

Table 5.2.2.2.4-1: Codebook for 1-layer and 2-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI‑RS

|  |  |
| --- | --- |
| Layers |  |
|
|  |  |
|  |  |
| where ,  and the mappings from  to , , and  and from to , , , and  are as described above, including the ranges of the constituent indices of  and . | |

##### 5.2.2.2.5 Enhanced Type II Codebook

For 4 antenna ports {3000, 3001, …, 3003}, 8 antenna ports {3000, 3001, …, 3007}, 12 antenna ports {3000, 3001, …, 3011}, 16 antenna ports {3000, 3001, …, 3015}, 24 antenna ports {3000, 3001, …, 3023}, and 32 antenna ports {3000, 3001, …, 3031}, and UE configured with higher layer parameter *codebookType* set to ' typeII-r16'

- The values of and are configured with the higher layer parameter *n1-n2-codebookSubsetRestriction-r16*. The supported configurations of for a given number of CSI-RS ports and the corresponding values of are given in Table 5.2.2.2.1-2. The number of CSI-RS ports, , is .

- The values of , and are determined by the higher layer parameter *paramCombination-r16*, where the mapping is given in Table 5.2.2.2.5-1.

- The UE is not expected to be configured with *paramCombination-r16* equal to

- 3, 4, 5, 6, 7, or 8 when ,

- 7 or 8 when

- 7 or 8 when higher layer parameter t*ypeII-RI-Restriction-r16* is configured with for any .

- 7 or 8 when .

- The parameter is configured with the higher-layer parameter *numberOfPMISubbandsPerCQISubband*. This parameter controls the total number of precoding matrices indicated by the PMI as a function of the number of subbands in *csi-ReportingBand*, the subband size configured by the higher-level parameter *subbandSize* and of the total number of PRBs in the bandwidth part according to Table 5.2.1.4-2, as follows:

- When :

- One precoding matrix is indicated by the PMI for each subband in *csi-ReportingBand*.

- When :

- For each subband in *csi-ReportingBand* that is not the first or last subband of a BWP, two precoding matrices are indicated by the PMI: the first precoding matrix corresponds to the first PRBs of the subband and the second precoding matrix corresponds to the last PRBs of the subband.

- For each subband in *csi-ReportingBand* that is the first or last subband of a BWP

- If , one precoding matrix is indicated by the PMI corresponding to the first subband. If , two precoding matrices are indicated by the PMI corresponding to the first subband: the first precoding matrix corresponds to the first PRBs of the first subband and the second precoding matrix corresponds to the last PRBs of the first subband.

- If , one precoding matrix is indicated by the PMI corresponding to the last subband. If , two precoding matrices are indicated by the PMI corresponding to the last subband: the first precoding matrix corresponds to the first PRBs of the last subband and the second precoding matrix corresponds to the last PRBs of the last subband.

Table 5.2.2.2.5-1: Codebook parameter configurations for and

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *paramCombination-r16* |  |  | |  |
|  |  |
| 1 | 2 | ¼ | 1/8 | ¼ |
| 2 | 2 | ¼ | 1/8 | ½ |
| 3 | 4 | ¼ | 1/8 | ¼ |
| 4 | 4 | ¼ | 1/8 | ½ |
| 5 | 4 | ¼ | ¼ | ¾ |
| 6 | 4 | ½ | ¼ | ½ |
| 7 | 6 | ¼ | - | ½ |
| 8 | 6 | ¼ | - | ¾ |

- The UE shall report the RI value according to the configured higher layer parameter *typeII-RI-Restriction-r16*. The UE shall not report .

The PMI value corresponds to the codebook indices of  and  where

The precoding matrices indicated by the PMI are determined from vectors.

vectors, , are indentified by the indices , , indicated by , , obtained as in 5.2.2.2.3, where the values of are given in Table 5.2.2.2.5-4.

vectors, , , are identified by (for ) and where

which are indicated by means of the indices (for ) and , where

|  |
| --- |
|  |
| . |

The amplitude coefficient indicators and are

|  |
| --- |
|  |
|  |
|  |
|  |
|  |

for .

The phase coefficient indicator is

for

Let . The bitmap whose nonzero bits identify which coefficients in and are reported, is indicated by

|  |
| --- |
|  |
|  |
|  |

for , such that is the number of nonzero coefficients for layer and is the total number of nonzero coefficients.

The indices of , and are associated to the codebook indices in .

The mapping from to the amplitude coefficient is given in Table 5.2.2.2.5-2 and the mapping from to the amplitude coefficient is given in Table 5.2.2.2.5-3. The amplitude coefficients are represented by

|  |
| --- |
|  |
|  |
|  |

for.

Let  be the index of and be the index of which identify the strongest coefficient of layer , i.e., the element of , for and . The codebook indices of are remapped with respect to as , such that , after remapping. The index is remapped with respect to as , such that the index of the strongest coefficient is (), after remapping. The indices of , and indicate amplitude coefficients, phase coefficients and bitmap after remapping.

The strongest coefficient of layer is identified by , which is obtained as follows

for .

Table 5.2.2.2.5-2: Mapping of elements of : to

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | |  |  | | | 0 | Reserved | | 1 |  | | 2 |  | | 3 |  | | |  |  | | --- | --- | |  |  | | | 4 |  | | 5 |  | | 6 |  | | 7 |  | | |  |  | | --- | --- | |  |  | | | 8 |  | | 9 |  | | 10 |  | | 11 |  | | |  |  | | --- | --- | |  |  | | | 12 |  | | 13 |  | | 14 |  | | 15 | 1 | |

The amplitude and phase coefficient indicators are reported as follows:

- , , and . The indicators , and are not reported for .

- The indicator is reported for .

- The indicators for which and are reported.

- The indicators for which and are reported.

- The remaining indicators are not reported and the corresponding are reported.

- The remaining indicators are not reported and the corresponding are reported.

Table 5.2.2.2.5-3: Mapping of elements of : to

|  |  |
| --- | --- |
|  |  |
|
| 0 |  |
| 1 |  |
| 2 |  |
| 3 |  |
| 4 |  |
| 5 |  |
| 6 |  |
| 7 | 1 |

The elements of and are found from using the algorithm described in 5.2.2.2.3, where the values of are given in Table 5.2.2.2.5-4.

For , is identified by .

For all values of , for . The nonzero elements of , identified by are found from , for , and from and , for , using as defined in 5.2.2.2.3 and the algorithm:

for

Find the largest  in Table 5.2.2.2.5-4 such that

if

else

if

else

end if

end if

Table 5.2.2.2.5-4: Combinatorial coefficients

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** | **9** |
| 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| 1 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| 2 | 2 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| 3 | 3 | 3 | 1 | 0 | 0 | 0 | 0 | 0 | 0 |
| 4 | 4 | 6 | 4 | 1 | 0 | 0 | 0 | 0 | 0 |
| 5 | 5 | 10 | 10 | 5 | 1 | 0 | 0 | 0 | 0 |
| 6 | 6 | 15 | 20 | 15 | 6 | 1 | 0 | 0 | 0 |
| 7 | 7 | 21 | 35 | 35 | 21 | 7 | 1 | 0 | 0 |
| 8 | 8 | 28 | 56 | 70 | 56 | 28 | 8 | 1 | 0 |
| 9 | 9 | 36 | 84 | 126 | 126 | 84 | 36 | 9 | 1 |
| 10 | 10 | 45 | 120 | 210 | 252 | 210 | 120 | 45 | 10 |
| 11 | 11 | 55 | 165 | 330 | 462 | 462 | 330 | 165 | 55 |
| 12 | 12 | 66 | 220 | 495 | 792 | 924 | 792 | 495 | 220 |
| 13 | 13 | 78 | 286 | 715 | 1287 | 1716 | 1716 | 1287 | 715 |
| 14 | 14 | 91 | 364 | 1001 | 2002 | 4004 | 3432 | 3003 | 2002 |
| 15 | 15 | 105 | 455 | 1365 | 3003 | 5005 | 6435 | 6435 | 5005 |
| 16 | 16 | 120 | 560 | 1820 | 4368 | 8008 | 11440 | 12870 | 11440 |
| 17 | 17 | 136 | 680 | 2380 | 6188 | 12376 | 19448 | 24310 | 24310 |
| 18 | 18 | 153 | 816 | 3060 | 8568 | 18564 | 31824 | 43758 | 48620 |

When and are known, and are found as follows:

- If , and is not reported. , where is given in Table 5.2.2.2.5-4 and where the indices are assigned such that increases as increases.

- If , is indicated by , which is reported and given by

Only the nonzero indices , where, are reported, where the indices  are assigned such that increases as increases. Let

then , where is given in Table 5.2.2.2.5-4.

The codebooks for 1-4 layers are given in Table 5.2.2.2.5-5, where , , for and are obtained as in clause 5.2.2.2.3, and the quantities and are given by

|  |
| --- |
|  |
|  |

where , is the index associated with the precoding matrix, , and with

for.

Table 5.2.2.2.5-5: Codebook for 1-layer. 2-layer, 3-layer and 4-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI‑RS

|  |  |
| --- | --- |
| **Layers** |  |
|
|  |  |
|  |  |
|  |  |
|  |  |
| Where  and the mappings from to , , , , , , , , , , and , and from to , , , , , and are as described above, including the ranges of the constituent indices of and . | |

For coefficients with , amplitude and phase are set to zero, i.e., and .

The bitmap parameter *typeII-RI‑Restriction-r16* forms the bit sequence where is the LSB and is the MSB. When is zero, , PMI and RI reporting are not allowed to correspond to any precoder associated with layers.

The bitmap parameter *n1-n2‑codebookSubsetRestriction-r16* forms the bit sequence and configures the vector group indices as in clause 5.2.2.2.3. Bits indicate the maximum allowed average amplitude, (), with , of the coefficients associated with the vector in group indexed by , where the maximum amplitudes are given in Table 5.2.2.2.5-6 and the average coefficient amplitude is restricted as follows

for , and . A UE that does not report the parameter *amplitudeSubsetRestriction*='supported' in its capability signaling is not expected to be configured with or .

Table 5.2.2.2.5-6: Maximum allowed average coefficient amplitudes for restricted vectors

|  |  |
| --- | --- |
| Bit | Maximum  Average Coefficient Amplitude |
|
| 00 | 0 |
| 01 |  |
| 10 |  |
| 11 | 1 |

##### 5.2.2.2.6 Enhanced Type II Port Selection Codebook

For 4 antenna ports {3000, 3001, …, 3003}, 8 antenna ports {3000, 3001, …, 3007}, 12 antenna ports {3000, 3001, …, 3011}, 16 antenna ports {3000, 3001, …, 3015}, 24 antenna ports {3000, 3001, …, 3023}, and 32 antenna ports {3000, 3001, …, 3031}, and the UE configured with higher layer parameter *codebookType* set to ' typeII-PortSelection-r16 '

- The number of CSI-RS ports is configured as in Clause 5.2.2.2.4

- The value of is configured with the higher layer parameter *portSelectionSamplingSize-r16*, where and .

- The values , and are configured as in Clause 5.2.2.2.5, where the supported configurations are given in Table 5.2.2.2.6-1.

Table 5.2.2.2.6-1: Codebook parameter configurations for , and

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *paramCombination-r16* |  |  | |  |
|  |  |
| 1 | 2 | ¼ | 1/8 | ¼ |
| 2 | 2 | ¼ | 1/8 | ½ |
| 3 | 4 | ¼ | 1/8 | ¼ |
| 4 | 4 | ¼ | 1/8 | ½ |
| 5 | 4 | ¼ | ¼ | ¾ |
| 6 | 4 | ½ | ¼ | ½ |

- The UE shall report the RI value according to the configured higher layer parameter *typeII-PortSelectionRI-Restriction-r16*. The UE shall not report .

- The values of is configured as in Clause 5.2.2.2.5.

The UE is also configured with the higher layer bitmap parameter *typeII-PortSelectionRI-Restriction-r16*, which forms the bit sequence , where is the LSB and is the MSB. When is zero, , PMI and RI reporting are not allowed to correspond to any precoder associated with layers.

The PMI value corresponds to the codebook indices and where

The antenna ports are selected by the index as in clause 5.2.2.2.4.

Parameters , (for ) and are defined as in clause 5.2.2.2.5.

For layer , , the strongest coefficient the amplitude coefficient indicators and , the phase coefficient indicator and the bitmap indicator are defined and indicated as in clause 5.2.2.2.5, where the mapping from to the amplitude coefficient is given in Table 5.2.2.2.5-2 and the mapping from to the amplitude coefficient is given inTable 5.2.2.2.5-3.

The number of nonzero coefficients for layer , , and the total number of nonzero coefficients are defined as in Clause 5.2.2.2.5.

The amplitude coefficients and are represented as in clause 5.2.2.2.5.

The amplitude and phase coefficient indicators are reported as in clause 5.2.2.2.5.

Codebook indicators and are found as in clause 5.2.2.2.5.

The codebooks for 1-4 layers are given in Table 5.2.2.2.6-2, where is a -element column vector containing a value of 1 in element and zeros elsewhere (where the first element is element 0), and the quantities and are defined as in clause 5.2.2.2.5.

Table 5.2.2.2.6-2: Codebook for 1-layer. 2-layer, 3-layer and 4-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI‑RS

|  |  |
| --- | --- |
| **Layers** |  |
|
|  |  |
|  |  |
|  |  |
|  |  |
| Where ,  and the mappings from to, , , , , , , and , and from to , , , , , and are as described above, including the ranges of the constituent indices of and . | |

For coefficients with , amplitude and phase are set to zero, i.e., and .

#### 5.2.2.3 Reference signal (CSI-RS)

##### 5.2.2.3.1 NZP CSI-RS

The UE can be configured with one or more NZP CSI-RS resource set configuration(s) as indicated by the higher layer parameters *CSI-ResourceConfig,* and *NZP-CSI-RS-ResourceSet.* Each NZP CSI-RS resource set consists of *K*≥1 NZP CSI-RS resource(s).

The following parameters for which the UE shall assume non-zero transmission power for CSI-RS resource are configured via the higher layer parameter *NZP-CSI-RS-Resource, CSI-ResourceConfig* and *NZP-CSI-RS-ResourceSet* for each CSI-RS resource configuration:

- *nzp-CSI-RS-ResourceId* determines CSI-RS resource configuration identity.

- *periodicityAndOffset* defines the CSI-RS periodicity and slot offset for periodic/semi-persistent CSI-RS. All the CSI-RS resources within one set are configured with the same periodicity, while the slot offset can be same or different for different CSI-RS resources.

- *resourceMapping* defines the number of ports, CDM-type, and OFDM symbol and subcarrier occupancy of the CSI-RS resource within a slot that are given in Clause 7.4.1.5 of [4, TS 38.211].

- *nrofPorts* in *resourceMapping* defines the number of CSI-RS ports, where the allowable values are given in Clause 7.4.1.5 of [4, TS 38.211].

- *density* in *resourceMapping* defines CSI-RS frequency density of each CSI-RS port per PRB, and CSI-RS PRB offset in case of the density value of 1/2, where the allowable values are given in Clause 7.4.1.5 of [4, TS 38.211]. For density 1/2, the odd/even PRB allocation indicated in *density* is with respect to the common resource block grid.

- *cdm-Type* in *resourceMapping* defines CDM values and pattern, where the allowable values are given in Clause 7.4.1.5 of [4, TS 38.211].

*- powerControlOffset*: which is the assumed ratio of PDSCH EPRE to NZP CSI-RS EPRE when UE derives CSI feedback and takes values in the range of [-8, 15] dB with 1 dB step size.

*- powerControlOffsetSS*: which is the assumed ratio of NZP CSI-RS EPRE to SS/PBCH block EPRE.

- *scramblingID* defines scrambling ID of CSI-RSwith length of 10 bits.

- *BWP-Id* in *CSI-ResourceConfig* defines which bandwidth part the configured CSI-RS is located in.

- *repetition* in *NZP-CSI-RS-ResourceSet* is associated with a CSI-RS resource set and defines whether UE can assume the CSI-RS resources within the NZP CSI-RS Resource Set are transmitted with the same downlink spatial domain transmission filter or not as described in Clause 5.1.6.1.2. and can be configured only when the higher layer parameter *reportQuantity* associated with all the reporting settings linked with the CSI-RS resource set is set to 'cri-RSRP', 'cri-SINR' or 'none'.

- *qcl-InfoPeriodicCSI-RS* contains a reference to a *TCI-State* indicating QCL source RS(s) and QCL type(s). If the *TCI-State* is configured with a reference to an RS with 'QCL-TypeD' association, that RS may be an SS/PBCH block located in the same or different CC/DL BWP or a CSI-RS resource configured as periodic located in the same or different CC/DL BWP.

- *trs-Info* in *NZP-CSI-RS-ResourceSet* is associated with a CSI-RS resource set and for which the UE can assume that the antenna port with the same port index of the configured NZP CSI-RS resources in the *NZP-CSI-RS-ResourceSet* is the same as described in Clause 5.1.6.1.1 and can be configured when reporting setting is not configured or when the higher layer parameter *reportQuantity* associated with all the reporting settings linked with the CSI-RS resource set is set to 'none'.

All CSI-RS resources within one set are configured with same *density* and same *nrofPorts*, except for the NZP CSI-RS resources used for interference measurement.

The UE expects that all the CSI-RS resources of a resource set are configured with the same starting RB and number of RBs and the same *cdm-type*.

The bandwidth and initial common resource block (CRB) index of a CSI-RS resource within a BWP, as defined in Clause 7.4.1.5 of [4, TS 38.211], are determined based on the higher layer parameters *nrofRBs* and *startingRB*, respectively, within the CSI-FrequencyOccupation IE configured by the higher layer parameter *freqBand* within the *CSI-RS-ResourceMapping* IE. Both *nrofRBs* and *startingRB* are configured as integer multiples of 4 RBs, and the reference point for *startingRB* is CRB 0 on the common resource block grid. If the UE shall assume that the initial CRB index of the CSI-RS resource is , otherwise . If , the UE shall assume that the bandwidth of the CSI-RS resource is , otherwise . In all cases, the UE shall expect that .

#### 5.2.2.4 Channel State Information – Interference Measurement (CSI-IM)

The UE can be configured with one or more CSI-IM resource set configuration(s) as indicated by the higher layer parameter *CSI-IM-ResourceSet*. Each CSI-IM resource set consists of *K*≥1 CSI-IM resource(s).

The following parameters are configured via higher layer parameter *CSI-IM-Resource* for each CSI-IM resource configuration:

*- csi-IM-ResourceId* determines CSI-IM resource configuration identity

*- subcarrierLocation-p0* or *subcarrierLocation-p1* defines subcarrier occupancy of the CSI-IM resource within a slot for *csi-IM-ResourceElementPattern* set to 'pattern0' or 'pattern1', respectively.

*- symbolLocation-p0* or *symbolLocation-p1* defines OFDM symbol location of the CSI-IM resource within a slot for *csi-IM-ResourceElementPattern* set to 'pattern0' or 'pattern1', respectively.

*- periodicityAndOffset* defines the CSI-IM periodicity and slot offset for periodic/semi-persistent CSI-IM.

*-* f*reqBand* includes parameters to enable configuration of frequency-occupancy of CSI-IM

In each of the PRBs configured by f*reqBand,* the UE shall assume each CSI-IM resource is located in,

- resource elements , ,  and , if *csi-IM-ResourceElementPattern* is set to 'pattern0',

- resource elements , ,  and  if *csi-IM-ResourceElementPattern* is set to 'pattern1',

where and  are the configured frequency-domain location and time-domain location, respectively, given by the higher layer parameters in the above list.

#### 5.2.2.5 CSI reference resource definition

The CSI reference resource for a serving cell is defined as follows:

- In the frequency domain, the CSI reference resource is defined by the group of downlink physical resource blocks corresponding to the band to which the derived CSI relates.

- In the time domain, the CSI reference resource for a CSI reporting in uplink slot *n'* is defined by a single downlink slot *n*-*nCSI\_ref*,

- where  and and  are the subcarrier spacing configurations for DL and UL, respectively

- where for periodic and semi-persistent CSI reporting

- if a single CSI-RS/SSB resource is configured for channel measurement *nCSI\_ref* is the smallest value greater than or equal to , such that it corresponds to a valid downlink slot, or

- if multiple CSI-RS/SSB resources are configured for channel measurement *nCSI\_ref* is the smallest value greater than or equal to , such that it corresponds to a valid downlink slot.

- where for aperiodic CSI reporting, if the UE is indicated by the DCI to report CSI in the same slot as the CSI request, *nCSI\_ref* is such that the reference resource is in the same valid downlink slot as the corresponding CSI request, otherwise *nCSI\_ref* is the smallest value greater than or equal to , such that slot *n*- *nCSI\_ref* corresponds to a valid downlink slot, where *Z'* corresponds to the delay requirement as defined in Clause 5.4.

- when periodic or semi-persistent CSI-RS/CSI-IM or SSB is used for channel/interference measurements, the UE is not expected to measure channel/interference on the CSI-RS/CSI-IM/SSB whose last OFDM symbol is received up to *Z'* symbols before transmission time of the first OFDM symbol of the aperiodic CSI reporting.

A slot in a serving cell shall be considered to be a valid downlink slot if:

- it comprises at least one higher layer configured downlink or flexible symbol, and

- it does not fall within a configured measurement gap for that UE

If there is no valid downlink slot for the CSI reference resource corresponding to a CSI Report Setting in a serving cell, CSI reporting is omitted for the serving cell in uplink slot *n'*.

After the CSI report (re)configuration, serving cell activation, BWP change, or activation of SP-CSI, the UE reports a CSI report only after receiving at least one CSI-RS transmission occasion for channel measurement and CSI-RS and/or CSI-IM occasion for interference measurement no later than CSI reference resource and drops the report otherwise.

When DRX is configured, the UE reports a CSI report only if receiving at least one CSI-RS transmission occasion for channel measurement and CSI-RS and/or CSI-IM occasion for interference measurement in DRX Active Time no later than CSI reference resource and drops the report otherwise. When the UE is configured to monitor DCI format 2\_6 and if the UE configured by higher layer parameter [*PS-Periodic\_CSI\_TransmitOrNot*] to report CSI with the higher layer parameter *reportConfigType* set to ‘periodic’ when *drx-onDurationTimer* is not started, the UE shall report CSI during the time duration indicated by *drx-onDurationTimer* also outside active time according to the procedure described in Clause 5.2.1.4. When the UE is configured to monitor DCI format 2\_6 and if the UE configured by higher layer parameter [*PS\_Periodic\_L1-RSRP\_TransmitOrNot*] to report L1-RSRP with the higher layer parameter *reportConfigType* set to ‘periodic’ when *drx-onDurationTimer* is not started, the UE shall report L1-RSRP during the time duration indicated by *drx-onDurationTimer* also outside active time according to the procedure described in clause 5.2.1.4.

When deriving CSI feedback, the UE is not expected that a NZP CSI -RS resource for channel measurement overlaps with CSI-IM resource for interference measurement or NZP CSI -RS resource for interference measurement.

If configured to report CQI index, in the CSI reference resource, the UE shall assume the following for the purpose of deriving the CQI index, and if also configured, for deriving PMI and RI:

- The first 2 OFDM symbols are occupied by control signaling.

- The number of PDSCH and DM-RS symbols is equal to 12.

- The same bandwidth part subcarrier spacing configured as for the PDSCH reception

- The bandwidth as configured for the corresponding CQI report.

- The reference resource uses the CP length and subcarrier spacing configured for PDSCH reception

- No resource elements used by primary or secondary synchronization signals or PBCH.

- Redundancy Version 0.

- The ratio of PDSCH EPRE to CSI-RS EPRE is as given in Clause 4.1.

- Assume no REs allocated for NZP CSI-RS and ZP CSI-RS.

- Assume the same number of front loaded DM-RS symbols as the maximum front-loaded symbols configured by the higher layer parameter *maxLength* in *DMRS-DownlinkConfig.*

- Assume the same number of additional DM-RS symbols as the additional symbols configured by the higher layer parameter *dmrs-AdditionalPosition*.

- Assume the PDSCH symbols are not containing DM-RS.

- Assume PRB bundling size of 2 PRBs.

- The PDSCH transmission scheme where the UE may assume that PDSCH transmission would be performed with up to 8 transmission layers as defined in Clause 7.3.1.4 of [4, TS 38.211]. For CQI calculation, the UE should assume that PDSCH signals on antenna ports in the set [1000,…, 1000+ν-1] for ν layers would result in signals equivalent to corresponding symbols transmitted on antenna ports [3000,…, 3000+*P*-1], as given by

where  is a vector of PDSCH symbols from the layer mapping defined in Clause 7.3.1.4 of [4, TS 38.211],  is the number of CSI-RS ports. If only one CSI-RS port is configured, *W(i)* is 1. If the higher layer parameter *reportQuantity* in *CSI-ReportConfig* for which the CQI is reported is set to either 'cri-RI-PMI-CQI' or 'cri-RI-LI-PMI-CQI', *W(i)* is the precoding matrix corresponding to the reported PMI applicable to *x(i)*. If the higher layer parameter *reportQuantity* in *CSI-ReportConfig* for which the CQI is reported is set to 'cri-RI-CQI', *W(i)* is the precoding matrix corresponding to the procedure described in Clause 5.2.1.4.2. If the higher layer parameter *reportQuantity* in *CSI-ReportConfig* for which the CQI is reported is set to 'cri-RI-i1-CQI', *W(i)* is the precoding matrix corresponding to the reported i1 according to the procedure described in Clause 5.2.1.4.2*.*The corresponding PDSCH signals transmitted on antenna ports [3000,…,3000 + *P* - 1] would have a ratio of EPRE to CSI-RS EPRE equal to the ratio given in Clause 5.2.2.3.1.

### 5.2.3 CSI reporting using PUSCH

A UE shall perform aperiodic CSI reporting using PUSCH on serving cell c upon successful decoding of a DCI format 0\_1 or DCI format 0\_2 which triggers an aperiodic CSI trigger state.

When a DCI format 0\_1 schedules two PUSCH allocations, the aperiodic CSI report is carried on the second scheduled PUSCH. When a DCI format 0\_1 schedules more than two PUSCH allocations, the aperiodic CSI report is carried on the penultimate scheduled PUSCH.

An aperiodic CSI report carried on the PUSCH supports wideband, and sub-band frequency granularities. An aperiodic CSI report carried on the PUSCH supports Type I, Type II and Enhanced Type II CSI.

A UE shall perform semi-persistent CSI reporting on the PUSCH upon successful decoding of a DCI format 0\_1 or DCI format 0\_2 which activates a semi-persistent CSI trigger state. DCI format 0\_1 and DCI format 0\_2 contains a CSI request field which indicates the semi-persistent CSI trigger state to activate or deactivate. Semi-persistent CSI reporting on the PUSCH supports Type I, Type II with wideband, and sub-band frequency granularities and Enhanced Type II CSI. The PUSCH resources and MCS shall be allocated semi-persistently by an uplink DCI.

CSI reporting on PUSCH can be multiplexed with uplink data on PUSCH. CSI reporting on PUSCH can also be performed without any multiplexing with uplink data from the UE.

Type I CSI feedback is supported for CSI Reporting on PUSCH. Type I wideband and sub-band CSI is supported for CSI Reporting on the PUSCH. Type II CSI is supported for CSI Reporting on the PUSCH.

For Type I, Type II and Enhanced Type II CSI feedback on PUSCH, a CSI report comprises of two parts. Part 1 has a fixed payload size and is used to identify the number of information bits in Part 2. Part 1 shall be transmitted in its entirety before Part 2.

- For Type I CSI feedback, Part 1 contains RI (if reported), CRI (if reported), CQI for the first codeword (if reported). Part 2 contains PMI (if reported) and contains the CQI for the second codeword (if reported) when RI (if reported) is larger than 4.

- For Type II CSI feedback, Part 1 contains RI (if reported), CQI, and an indication of the number of non-zero wideband amplitude coefficients per layer for the Type II CSI (see Clause 5.2.2.2.3). The fields of Part 1 – RI (if reported), CQI, and the indication of the number of non-zero wideband amplitude coefficients for each layer – are separately encoded. Part 2 contains the PMI of the Type II CSI. Part 1 and 2 are separately encoded.

- For Enhanced Type II CSI feedback, Part 1 contains RI, CQI, and an indication of the overall number of non-zero amplitude coefficients across layers for the Enhanced Type II CSI (see Clause 5.2.2.2.5). The fields of Part 1 – RI, CQI, and the indication of the overall number of non-zero amplitude coefficients across layers – are separately encoded. Part 2 contains the PMI of the Enhanced Type II CSI. Part 1 and 2 are separately encoded.

A Type II CSI report that is carried on the PUSCH shall be computed independently from any Type II CSI report that is carried on the PUCCH formats 3 or 4 (see Clause 5.2.4 and 5.2.2).

When the higher layer parameter *reportQuantity* is configured with one of the values 'cri-RSRP' or 'ssb-Index-RSRP', the CSI feedback consists of a single part.

For both Type I and Type II reports configured for PUCCH but transmitted on PUSCH, the determination of the payload for CSI part 1 and CSI part 2 follows that of PUCCH as described in Clause 5.2.4.

When CSI reporting on PUSCH comprises two parts, the UE may omit a portion of the Part 2 CSI. Omission of Part 2 CSI is according to the priority order shown in Table 5.2.3-1, where  is the number of CSI reports configured to be carried on the PUSCH. Priority 0 is the highest priority and priority  is the lowest priority and the CSI report *n* corresponds to the CSI report with the *n*th smallest Prii,CSI(*y,k,c,s*) value among the  CSI reports as defined in Clause 5.2.5. The subbands for a given CSI report *n* indicated by the higher layer parameter *csi-ReportingBand* are numbered continuously in increasing order with the lowest subband of *csi-ReportingBand* as subband 0. When omitting Part 2 CSI information for a particular priority level, the UE shall omit all of the information at that priority level.

- For Enhanced Type II reports, for a given CSI report , each reported element of indices and , indexed by and , is associated with a priority value , with with , , and , and where is defined in Clause 5.2.2.2.5. The element with the highest priority has the lowest associated value . Omission of Part 2 CSI is according to the priority order shown in Table 5.2.3-2, where

- Group 0 includes indices , and ().

- Group 1 includes indices (if reported), , the highest priority elements of , , the highest priority elements of and the highest priority elements of ().

- Group 2 includes the lowest priority elements of , the lowest priority elements of and the lowest priority elements of ().

Table 5.2.3-1: Priority reporting levels for Part 2 CSI

|  |
| --- |
| Priority 0:  For CSI reports 1 to , Group 0 CSI for CSI reports configured as ‘typeII-r16’ or ‘typeII-PortSelection-r16’; Part 2 wideband CSI for CSI reports configured otherwise |
| Priority 1:  Group 1 CSI for CSI report 1, if configured as ‘typeII-r16’ or ‘typeII-PortSelection-r16’; Part 2 subband CSI of even subbands for CSI report 1, if configured otherwise |
| Priority 2:  Group 2 CSI for CSI report 1, if configured as ‘typeII-r16’ or ‘typeII-PortSelection-r16’; Part 2 subband CSI of odd subbands for CSI report 1, if configured otherwise |
| Priority 3:  Group 1 CSI for CSI report 2, if configured as ‘typeII-r16’ or ‘typeII-PortSelection-r16’; Part 2 subband CSI of even subbands for CSI report 2, if configured otherwise |
| Priority 4:  Group 2 CSI for CSI report 2, if configured as ‘typeII-r16’ or ‘typeII-PortSelection-r16’. Part 2 subband CSI of odd subbands for CSI report 2, if configured otherwise |
| ⁞ |
| Priority :  Group 1 CSI for CSI report , if configured as ‘typeII-r16’ or ‘typeII-PortSelection-r16’; Part 2 subband CSI of even subbands for CSI report , if configured otherwise |
| Priority :  Group 2 CSI for CSI report , if configured as ‘typeII-r16’ or ‘typeII-PortSelection-r16’; Part 2 subband CSI of odd subbands for CSI report , if configured otherwise |

When the UE is scheduled to transmit a transport block on PUSCH multiplexed with a CSI report(s), Part 2 CSI is omitted only when  is larger than , where parameters , , , , , , , ,  and are defined in Clause 6.3.2.4 of [5, TS 38.212].

Part 2 CSI is omitted level by level, beginning with the lowest priority level until the lowest priority level is reached which causes the  to be less than or equal to .

When part 2 CSI is transmitted on PUSCH with no transport block, lower priority bits are omitted until Part 2 CSI code rate, which is given by where , , are given in clause 6.3.2.4 of [5, 38.212] before HARQ-ACK puncturing part 2 CSI if any, is below a threshold code rate lower than one, where



- is the CSI offset value from Table 9.3-2 of [6, TS 38.213]

- *R* is signaled code rate in DCI

If the UE is in an active semi-persistent CSI reporting configuration on PUSCH, the CSI reporting is deactivated when either the downlink BWP or the uplink BWP is changed. Another activation command is required to enable the semi-persistent CSI reporting.

### 5.2.4 CSI reporting using PUCCH

A UE is semi-statically configured by higher layers to perform periodic CSI Reporting on the PUCCH. A UE can be configured by higher layers for multiple periodic CSI Reports corresponding to multiple higher layer configured CSI Reporting Settings, where the associated CSI Resource Settings are higher layer configured. Periodic CSI reporting on PUCCH formats 2, 3, 4 supports Type I CSI with wideband granularity.

A UE shall perform semi-persistent CSI reporting on the PUCCH applied starting from the first slot that is after slot when the UE would transmit a PUCCH with HARQ-ACK information in slot *n* corresponding to the PDSCH carrying the activation command described in clause 6.1.3.16 of [10, TS 38.321]where ** is the SCS configuration for the PUCCH. The activation command will contain one or more Reporting Settings where the associated CSI Resource Settings are configured. Semi-persistent CSI reporting on the PUCCH supports Type I CSI. Semi-persistent CSI reporting on the PUCCH format 2 supports Type I CSI with wideband frequency granularity. Semi-persistent CSI reporting on PUCCH formats 3 or 4 supports Type I CSI with wideband and sub-band frequency granularities and Type II CSI Part 1.

When the PUCCH carry Type I CSI with wideband frequency granularity, the CSI payload carried by the PUCCH format 2 and PUCCH formats 3, or 4 are identical and the same irrespective of RI (if reported), CRI (if reported). For type I CSI sub-band reporting on PUCCH formats 3, or 4, the payload is split into two parts. The first part contains RI (if reported), CRI (if reported), CQI for the first codeword. The second part contains PMI and contains the CQI for the second codeword when RI > 4.

A semi-persistent report carried on the PUCCH formats 3 or 4 supports Type II CSI feedback, but only Part 1 of Type II CSI feedback (See Clause 5.2.2 and 5.2.3). Supporting Type II CSI reporting on the PUCCH formats 3 or 4 is a UE capability *type2-SP-CSI-Feedback-LongPUCCH*. A Type II CSI report (Part 1 only) carried on PUCCH formats 3 or 4 shall be calculated independently of any Type II CSI reports carried on the PUSCH (see Clause 5.2.3).

When the UE is configured with CSI Reporting on PUCCH formats 2, 3 or 4, each PUCCH resource is configured for each candidate UL BWP.

If the UE is in an active semi-persistent CSI reporting configuration on PUCCH and has not received a deactivation command, the CSI reporting takes place when the BWP in which the reporting is configured to take place is the active BWP, otherwise the CSI reporting is suspended.

A UE is not expected to report CSI with a total number of UCI bits and CRC bits larger than 115 bits when configured with PUCCH format 4. For CSI reports transmitted on a PUCCH, if all CSI reports consist of one part, the UE may omit a portion of CSI reports. Omission of CSI is according to the priority order determined from the Prii,CSI(*y,k,c,s*) value as defined in Clause 5.2.5. CSI report is omitted beginning with the lowest priority level until the CSI report code rate is less or equal to the one configured by the higher layer parameter *maxCodeRate*.

If any of the CSI reports consist of two parts, the UE may omit a portion of Part 2 CSI. Omission of Part 2 CSI is according to the priority order shown in Table 5.2.3-1. Part 2 CSI is omitted beginning with the lowest priority level until the Part 2 CSI code rate is less or equal to the one configured by higher layer parameter *maxCodeRate*.

### 5.2.5 Priority rules for CSI reports

CSI reports are associated with a priority value where

-  for aperiodic CSI reports to be carried on PUSCH  for semi-persistent CSI reports to be carried on PUSCH,  for semi-persistent CSI reports to be carried on PUCCH and  for periodic CSI reports to be carried on PUCCH;

-  for CSI reports carrying L1-RSRP or L1-SINR and  for CSI reports not carrying L1-RSRP or L1-SINR;

- *c* is the serving cell index and is the value of the higher layer parameter *maxNrofServingCells*;

- *s* is the *reportConfigID* andis the value of the higher layer parameter *maxNrofCSI-ReportConfigurations.*

A first CSI report is said to have priority over second CSI report if the associated  value is lower for the first report than for the second report.

Two CSI reports are said to collide if the time occupancy of the physical channels scheduled to carry the CSI reports overlap in at least one OFDM symbol and are transmitted on the same carrier. When a UE is configured to transmit two colliding CSI reports,

- if *y* values are different between the two CSI reports, the following rules apply except for the case when one of the *y* value is 2 and the other *y* value is 3 (for CSI reports transmitted on PUSCH, as described in Clause 5.2.3; for CSI reports transmitted on PUCCH, as described in Clause 5.2.4):

- The CSI report with higher  value shall not be sent by the UE.

- otherwise, the two CSI reports are multiplexed or either is dropped based on the priority values, as described in Clause 9.2.5.2 in [6, TS 38.213].

If a semi-persistent CSI report to be carried on PUSCH overlaps in time with PUSCH data transmission in one or more symbols on the same carrier, and if the earliest symbol of these PUSCH channels starts no earlier than N2+d2,1 symbols after the last symbol of the DCI scheduling the PUSCH where d2,1 is the maximum of the d2,1 associated with the PUSCH carrying semi-persistent CSI report and the PUSCH with data transmission, the CSI report shall not be transmitted by the UE. Otherwise, if the timeline requirement is not satisfied this is an error case.

If a UE would transmit a first PUSCH that includes semi-persistent CSI reports and a second PUSCH that includes an UL-SCH and the first PUSCH transmission would overlap in time with the second PUSCH transmission, the UE does not transmit the first PUSCH and transmits the second PUSCH. The UE expects that the first and second PUSCH transmissions satisfy the above timing conditions for PUSCH transmissions that overlap in time when at least one of the first or second PUSCH transmissions is in response to a DCI format detection by the UE.

## 5.3 UE PDSCH processing procedure time

If the first uplink symbol of the PUCCH which carries the HARQ-ACK information, as defined by the assigned HARQ-ACK timing *K1* and the PUCCH resource to be used and including the effect of the timing advance, starts no earlier than at symbol *L1*, where *L1* is defined as the next uplink symbol with its CP starting after  after the end of the last symbol of the PDSCH carrying the TB being acknowledged, then the UE shall provide a valid HARQ-ACK message.

*- N1* is based on *µ* of table 5.3-1 and table 5.3-2 for UE processing capability 1 and 2 respectively, where *µ* corresponds to the one of (*µPDCCH*, *µPDSCH*, *µUL*) resulting with the largest *Tproc,1*, where the *µPDCCH* corresponds to the subcarrier spacing of the PDCCH scheduling the PDSCH, the *µPDSCH* corresponds to the subcarrier spacing of the scheduled PDSCH, and *µUL* corresponds to the subcarrier spacing of the uplink channel with which the HARQ-ACK is to be transmitted, and κ is defined in clause 4.1 of [4, TS 38.211].

*-* If the PDSCH DM-RS position for the additional DM-RS in Table 7.4.1.1.2-3 in clause 7.4.1.1.2 of [4, TS 38.211] is then *N1,0=14* inTable 5.3-1*,* otherwise *N1,0=13.*

- If the UE is configured with multiple active component carriers, the first uplink symbol which carries the HARQ-ACK information further includes the effect of timing difference between the component carriers as given in [11, TS 38.133].

- For the PDSCH mapping type A as given in clause 7.4.1.1 of [4, TS 38.211]: if the last symbol of PDSCH is on the *i-*th symbol of the slot where *i* < 7, then *d1,1 = 7 - i*, otherwise *d1,1 = 0*

- For UE processing capability 1: If the PDSCH is mapping type B as given in clause 7.4.1.1 of [4, TS 38.211], and

- if the number of PDSCH symbols allocated is *L* ≥ 7, then *d1,1* = 0,

- if the number of PDSCH symbols allocated is *L* ≥ 4 and *L* ≤ 6, then *d1,1* = 7- *L.*

- if the number of PDSCH symbols allocated is *L* = *3* then *d1,1 = 3 +* min *(d,1)*, where *d* is the number of overlapping symbols of the scheduling PDCCH and the scheduled PDSCH.

- if the number of PDSCH symbols allocated is 2, then *d1,1* = 3*+d*, where *d* is the number of overlapping symbols of the scheduling PDCCH and the scheduled PDSCH.

- For UE processing capability 2: If the PDSCH is mapping type B as given in clause 7.4.1.1 of [4, TS 38.211],

- if the number of PDSCH symbols allocated is *L* ≥ 7, then *d1,1* = 0,

- if the number of PDSCH symbols allocated is *L* ≥ 3 and *L* ≤ 6, then *d1,1* is the number of overlapping symbols of the scheduling PDCCH and the scheduled PDSCH,

- if the number of PDSCH symbols allocated is 2,

- if the scheduling PDCCH was in a 3-symbol CORESET and the CORESET and the PDSCH had the same starting symbol, then *d1,1* = 3,

- otherwise *d1,1* is the number of overlapping symbols of the scheduling PDCCH and the scheduled PDSCH.

- For UE processing capability 2 with scheduling limitation when *µPDSCH* = 1, if the scheduled RB allocation exceeds 136 RBs, the UE defaults to capability 1 processing time. The UE may skip decoding a number of PDSCHs with last symbol within 10 symbols before the start of a PDSCH that is scheduled to follow Capability 2, if any of those PDSCHs are scheduled with more than 136 RBs with 30kHz SCS and following Capability 1 processing time.

- For a UE that supports capability 2 on a given cell, the processing time according to UE processing capability 2 is applied if the high layer parameter *processingType2Enabled* in *PDSCH-ServingCellConfig* is configured for the cell and set to *enable*.

- If this PUCCH resource is overlapping with another PUCCH or PUSCH resource, then HARQ-ACK is multiplexed following the procedure in clause 9.2.5 of [6, TS 38.213], otherwise the HARQ-ACK message is transmitted on PUCCH.

Otherwise the UE may not provide a valid HARQ-ACK corresponding to the scheduled PDSCH. The value of *Tproc,1* is used both in the case of normal and extended cyclic prefix.

Table 5.3-1: PDSCH processing time for PDSCH processing capability 1

|  |  |  |
| --- | --- | --- |
|  | PDSCH decoding time *N1* [symbols] | |
| *dmrs-AdditionalPosition* = pos0 in  *DMRS-DownlinkConfig* in both of  *dmrs-DownlinkForPDSCH-MappingTypeA*, *dmrs-DownlinkForPDSCH-MappingTypeB* | *dmrs-AdditionalPosition* ≠ pos0 in  *DMRS-DownlinkConfig* in either of  *dmrs-DownlinkForPDSCH-MappingTypeA*, *dmrs-DownlinkForPDSCH-MappingTypeB*  *or if the higher layer parameter is not configured* |
| 0 | 8 | *N1,0* |
| 1 | 10 | 13 |
| 2 | 17 | 20 |
| 3 | 20 | 24 |

Table 5.3-2: PDSCH processing time for PDSCH processing capability 2

|  |  |
| --- | --- |
|  | PDSCH decoding time *N1* [symbols] |
| *dmrs-AdditionalPosition* = pos0 in  *DMRS-DownlinkConfig* in both of  *dmrs-DownlinkForPDSCH-MappingTypeA*, *dmrs-DownlinkForPDSCH-MappingTypeB* |
| 0 | 3 |
| 1 | 4.5 |
| 2 | 9 for frequency range 1 |

### 5.3.1 Application delay of the minimum scheduling offset restriction

When the UE is scheduled with DCI format 0\_1 or 1\_1 with a [‘Minimum applicable scheduling offset indicator’]field, it shall determine the *K*0min and *K*2min values to be applied, while the previously applied *K*0min and *K*2min values are applied until the new values take effect after application delay. Change of applied minimum scheduling offset restriction indication carried by DCI in slot *n*, shall be applied in slot *n*+*X* of the scheduling cell.

When the DCI format 0\_1 or 1\_1 with [‘Minimum applicable scheduling offset indicator’**]** field indicating a change to the applied *K*0min or *K*2min is contained within the first three symbols of the slot, the value of application delay *X* is determined by, where *K*0minOld is the currently applied *K*0min value of the active DL BWP in the scheduled cell, and *Zµ* is determined by the subcarrier spacing of the active DL BWP in the scheduling cell, and given in Table 5.3.1-1 and *µ*PDCCH and *µ*PDSCH are the sub-carrier spacing configurations for PDCCH and PDSCH, respectively

When the DCI format 0\_1 or 1\_1 with [‘Minimum applicable scheduling offset indicator’**]** field is received outside the first [three] symbols of the slot, value of *Zµ* from Table 5.3.1-1 is incremented by one before determining the application delay *X*.

Table 5.3.1-1: Definition of *Zµ*

|  |  |
| --- | --- |
| *µ* | *Zµ* |
| 0 | [1] |
| 1 | [1] |
| 2 | [2] |
| 3 | [2] |

## 5.4 UE CSI computation time

When the *CSI request* field on a DCI triggers a CSI report(s) on PUSCH, the UE shall provide a valid CSI report for the *n*-th triggered report,

- if the first uplink symbol to carry the corresponding CSI report(s) including the effect of the timing advance, starts no earlier than at symbol *Zref* , and

- if the first uplink symbol to carry the *n*-th CSI report including the effect of the timing advance, starts no earlier than at symbol *Z'ref(n),*

where *Zref* is defined as the next uplink symbol with its CP starting  after the end of the last symbol of the PDCCH triggering the CSI report(s), and where *Z'ref(n),* is defined as the next uplink symbol with its CP starting after the end of the last symbol in time of the latest of: aperiodic CSI-RS resource for channel measurements, aperiodic CSI-IM used for interference measurements, and aperiodic NZP CSI-RS for interference measurement, when aperiodic CSI-RS is used for channel measurement for the *n*-th triggered CSI report.

If the PUSCH indicated by the DCI is overlapping with another PUCCH or PUSCH, then the CSI report(s) are multiplexed following the procedure in clause 9.2.5 of [6, TS 38.213] and clause 5.2.5 when applicable, otherwise the CSI report(s) are transmitted on the PUSCH indicated by the DCI.

When the *CSI request* field on a DCI triggers a CSI report(s) on PUSCH, if the first uplink symbol to carry the corresponding CSI report(s) including the effect of the timing advance, starts earlier than at symbol *Zref*,

- the UE may ignore the scheduling DCI if no HARQ-ACK or transport block is multiplexed on the PUSCH.

When the *CSI request* field on a DCI triggers a CSI report(s) on PUSCH, if the first uplink symbol to carry the *n*-th CSI report including the effect of the timing advance, starts earlier than at symbol *Z'ref(n),*

- the UE may ignore the scheduling DCI if the number of triggered reports is one and no HARQ-ACK or transport block is multiplexed on the PUSCH

- Otherwise, the UE is not required to update the CSI for the *n*-th triggered CSI report.

*Z,* *Z'* and *µ* are defined as:

and , where *M* is the number of updated CSI report(s) according to Clause 5.2.1.6, corresponds to the *m*-th updated CSI report and is defined as

- of the table 5.4-1 if the CSI is triggered without a PUSCH with either transport block or HARQ-ACK or both when *L* = 0 CPUs are occupied (according to Clause 5.2.1.6) and the CSI to be transmitted is a single CSI and corresponds to wideband frequency-granularity where the CSI corresponds to at most 4 CSI-RS ports in a single resource without CRI report and where *CodebookType* is set to 'typeI-SinglePanel' or where *reportQuantity* is set to 'cri-RI-CQI', or

- of the table 5.4-2 if the CSI to be transmitted corresponds to wideband frequency-granularity where the CSI corresponds to at most 4 CSI-RS ports in a single resource without CRI report and where *CodebookType* is set to 'typeI-SinglePanel' or where *reportQuantity* is set to 'cri-RI-CQI', or

- of the table 5.4-2 if the CSI to be transmitted corresponds to wideband frequency-granularity where the *reportQuantity* is set to 'ssb-Index-SINR', or *reportQuantity* is set to 'cri-SINR', or

- of the table 5.4-2 if *reportQuantity* is set to 'cri-RSRP' or 'ssb-Index-RSRP', is according to UE reported capability *beamReportTiming*  and *KBl* is according to UE reported capability *beamSwitchTiming* as defined in [13, TS 38.306], or

- of table 5.4-2 otherwise.

*- µ* of table 5.4-1 and table 5.4-2 corresponds to the min (*µPDCCH*, *µCSI-RS, µUL*) where the *µPDCCH* corresponds to the subcarrier spacing of the PDCCH with which the DCI was transmitted and *µUL* corresponds to the subcarrier spacing of the PUSCH with which the CSI report is to be transmitted and *µCSI-RS* corresponds to the minimum subcarrier spacing of the aperiodic CSI-RS triggered by the DCI

Table 5.4-1: CSI computation delay requirement 1

|  |  |  |
| --- | --- | --- |
|  | *Z1* [symbols] | |
| *Z1* | *Z'1* |
| 0 | 10 | 8 |
| 1 | 13 | 11 |
| 2 | 25 | 21 |
| 3 | 43 | 36 |

Table 5.4-2: CSI computation delay requirement 2

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | *Z1* [symbols] | | *Z2* [symbols] | | *Z3* [symbols] | |
| *Z1* | *Z'1* | *Z2* | *Z'2* | *Z3* | *Z'3* |
| 0 | 22 | 16 | 40 | 37 | 22 | *X*0 |
| 1 | 33 | 30 | 72 | 69 | 33 | *X*1 |
| 2 | 44 | 42 | 141 | 140 | min(44,*X*2+ KB1) | *X*2 |
| 3 | 97 | 85 | 152 | 140 | min(97, *X*3+ KB2) | *X*3 |

## 5.5 UE PDSCH reception preparation time with cross carrier scheduling with different subcarrier spacings for PDCCH and PDSCH

This clause applies only if the PDCCH carrying the scheduling DCI is received on one carrier with one OFDM subcarrier spacing, and the PDSCH scheduled to be received by the DCI is on another carrier with another OFDM subcarrier spacing.

If the µPDCCH < µPDSCH, the UE is expected to receive the scheduled PDSCH, if the first symbol in the PDSCH allocation, including the DM-RS, as defined by the slot offset *K0* and the start and length indicator *SLIV* of the scheduling DCI starts no earlier than the first symbol of the PDSCH slot starting at least *Npdsch* PDCCH symbols after the end of the PDCCH scheduling the PDSCH, not taking into account the effect of receive timing difference between the scheduling cell and the scheduled cell.

If the µPDCCH > µPDSCH, the UE is expected to receive the scheduled PDSCH, if the first symbol in the PDSCH allocation, including the DM-RS, as defined by the slot offset *K0* and the start and length indicator *SLIV* of the scheduling DCI starts no earlier than *Npdsch* PDCCH symbols after the end of the PDCCH scheduling the PDSCH, not taking into account the effect of receive timing difference between the scheduling cell and the scheduled cell.

Table 5.5-1: *Npdsch* as a function of the subcarrier spacing of the scheduling PDCCH

|  |  |
| --- | --- |
| ***µPDCCH*** | ***Npdsch* [symbols]** |
| 0 | 4 |
| 1 | 5 |
| 2 | 10 |
| 3 | 14 |

# 6 Physical uplink shared channel related procedure

## 6.1 UE procedure for transmitting the physical uplink shared channel

PUSCH transmission(s) can be dynamically scheduled by an UL grant in a DCI, or the transmission can correspond to a configured grant Type 1 or Type 2. The configured grant Type 1 PUSCH transmission is semi-statically configured to operate upon the reception of higher layer parameter of *configuredGrantConfig* including *rrc-ConfiguredUplinkGrant* without the detection of an UL grant in a DCI. The configured grant Type 2 PUSCH transmission is semi-persistently scheduled by an UL grant in a valid activation DCI according to Clause 10.2 of [6, TS 38.213] after the reception of higher layer parameter *configuredGrantConfig* not including *rrc-ConfiguredUplinkGrant*. If *Configuredgrantconfig-ToAddModList-r16* is configured, more than one configured grant configuration of configured grant Type 1 and/or configured grant Type 2 may be active at the same time on an active BWP of a serving cell.

For the PUSCH transmission corresponding to a Type 1 configured grant or a Type 2 configured grant activated by DCI format 0\_0 or 0\_1, the parameters applied for the transmission are provided by *configuredGrantConfig* except for *dataScramblingIdentityPUSCH*, *txConfig*, *codebookSubset*, *maxRank*, *scaling* of *UCI-OnPUSCH,* which are provided by *pusch-Config*. For the PUSCH transmission corresponding to a Type 2 configured grant activated by DCI format 0\_2, the parameters applied for the transmission are provided by *configuredGrantConfig* except for *dataScramblingIdentityPUSCH*, *txConfig*, *codebookSubset-ForDCIFormat0\_2*, *maxRank-ForDCIFormat0\_2*, *scaling* of *UCI-OnPUSCH* provided by *pusch-Config* [as well as DCI format 0\_2 specific handling with respect resource allocation of clause 6.1.2.2, TBA].If the UE is provided with *transformPrecoder* in *configuredGrantConfig*, the UE applies the higher layer parameter *tp-pi2BPSK*, if provided in *pusch-Config*, according to the procedure described in Clause 6.1.4 for the PUSCH transmission corresponding to a configured grant.

For the PUSCH retransmission scheduled by a PDCCH with CRC scrambled by CS-RNTI with NDI=1, the parameters in *pusch-Config* are applied for the PUSCH transmission except for *p0-NominalWithoutGrant, p0-PUSCH-Alpha, powerControlLoopToUse,* *pathlossReferenceIndex* described in Clause 7.1 of [6, TS 38.213], *mcs-Table, mcs-TableTransformPrecoder* described in Clause 6.1.4.1 and *transformPrecoder* described in Clause 6.1.3.

For a UE configured with two uplinks in a serving cell, PUSCH retransmission for a TB on the serving cell is not expected to be on a different uplink than the uplink used for the PUSCH initial transmission of that TB.

A UE shall upon detection of a PDCCH with a configured DCI format 0\_0, 0\_1 or 0\_2 transmit the corresponding PUSCH as indicated by that DCI. Upon detection of a DCI format 0\_1 or 0\_2 with "UL-SCH indicator" set to "0" and with a non-zero "CSI request" where the associated "reportQuantity" in *CSI-ReportConfig* set to "none" for all CSI report(s) triggered by "CSI request" in this DCI format 0\_1 or 0\_2, the UE ignores all fields in this DCI except the "CSI request" and the UE shall not transmit the corresponding PUSCH as indicated by this DCI format 0\_1 or 0\_2. For any HARQ process ID(s) in a given scheduled cell, the UE is not expected to transmit a PUSCH that overlaps in time with another PUSCH. For any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start a first PUSCH transmission starting in symbol *j* by a PDCCH ending in symbol *i*, the UE is not expected to be scheduled to transmit a PUSCH starting earlier than the end of the first PUSCH by a PDCCH that ends later than symbol *i*. The UE is not expected to be scheduled to transmit another PUSCH by DCI format 0\_0, 0\_1 or 0\_2 scrambled by C-RNTI or MCS-C-RNTI for a given HARQ process until after the end of the expected transmission of the last PUSCH for that HARQ process.

If a UE is configured by higher layer parameter *PDCCH-Config* that contains two different values of *CORESETPoolIndex* in *ControlResourceSet* for the active BWP of a serving cell and PDCCHs that schedule two non-overlapping in time domain PUSCHs are associated to different *ControlResourceSets* having different values of *CORESETPoolIndex,* for any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start a first PUSCH transmission starting in symbol *j* by a PDCCH associated with a value of *CORESETpoolIndex* ending in symbol *i*, the UE can be scheduled to transmit a PUSCH starting earlier than the end of the first PUSCH by a PDCCH associated with a different value of *CORESETpoolIndex* that ends later than symbol *i*.

A UE is not expected to be scheduled by a PDCCH ending in symbol to transmit a PUSCH on a given serving cell overlapping in time with a transmission occasion, where the UE is allowed to transmit a PUSCH with configured grant according to [10, TS38.321], starting in a symbol on the same serving cell if the end of symbol is not at least symbols before the beginning of symbol . The value in symbols is determined according to the UE processing capability defined in Clause 6.4, and and the symbol duration are based on the minimum of the subcarrier spacing corresponding to the PUSCH with configured grant and the subcarrier spacing of the PDCCH scheduling the PUSCH.

[If [a UE reports the capability of intra-UE prioritization], and if a PUSCH corresponding to a configured grant and a PUSCH scheduled by a PDCCH on a serving cell are partially or fully overlapping in time,

*-* If the PUSCH corresponding to the configured grant has *priority* in *configuredGrantConfig* set to 1 (i.e., high priority), and the PUSCH scheduled by the PDCCH is indicated as low priority by having the [priority indicator] field in the scheduling DCI set to 0 or by not having the [priority indicator] field present in the scheduling DCI, the UE is expected to transmit the PUSCH corresponding to the configured grant, and cancel the PUSCH transmission scheduled by the PDCCH at latest starting at the first symbol of the PUSCH corresponding to the configured grant.

*-* Otherwise, the UE shall cancel the PUSCH transmission corresponding to the configured grant at latest starting *M* symbols after the end of the last symbol of the PDCCH carrying the DCI scheduling the PUSCH, and transmit the PUSCH scheduled by the PDCCH, where

- *M = Tproc,2 +d1, where Tproc,2* is given by clause 6.4 for the corresponding PUSCH timing capability assuming *d2,1*= 0 and *d1* is determined by the reported UE capability [XXXXX],

- In this case, the UE is not expected to be scheduled for the PUSCH by the PDCCH where the PUSCH starts earlier than *N* symbols after the end of the last symbol of the PDCCH, where

- *N = Tproc,2* + *d2*, where *Tproc,2* is the PUSCH preparation time of the PUSCH scheduled by the PDCCH using the associated PUSCH timing capability according to clause 6.4 and *d2* is determined by the reported UE capability [YYYYY].

*-* In case of PUSCH repetitions, the overlapping handling is performed for each PUSCH repetition separately.

*-* The UE is not expected to be scheduled for another PUSCH by a PDCCH where this PUSCH starts no earlier than the end of the prioritized transmitted PUSCH and before the end of the time domain allocation of the cancelled PUSCH.]

A UE is not expected to be scheduled by a PDCCH ending in symbol to transmit a PUSCH on a given serving cell for a given HARQ process, if there is a transmission occasion where the UE is allowed to transmit a PUSCH with configured grant according to [10, TS38.321] with the same HARQ process on the same serving cell starting in a symbol after symbol , and if the gap between the end of PDCCH and the beginning of symbol is less than symbols. The value in symbols is determined according to the UE processing capability defined in Clause 6.4, and and the symbol duration are based on the minimum of the subcarrier spacing corresponding to the PUSCH with configured grant and the subcarrier spacing of the PDCCH scheduling the PUSCH.

For PUSCH scheduled by DCI format 0\_0 on a cell, the UE shall transmit PUSCH according to the spatial relation, if applicable, corresponding to the dedicated PUCCH resource with the lowest ID within the active UL BWP of the cell, as described in Clause 9.2.1 of [6, TS 38.213].

For PUSCH scheduled by DCI format 0\_0 on a cell and if the higher layer parameter *enableDefaultBeamPlForPUSCH0\_0* is set ‘enabled’, the UE is not configured with PUCCH resources on the active UL BWP and the UE is in RRC connected mode, the UE shall transmit PUSCH according to the spatial relation, if applicable, with a reference to the RS with ‘QCL-Type-D’ corresponding to the QCL assumption of the CORESET with the lowest ID.

For PUSCH scheduled by DCI format 0\_0 on a cell and if the higher layer parameter *enableDefaultBeamPlForPUSCH0\_0* is set ‘enabled’, the UE is configured with PUCCH resources on the active UL BWP where all the PUCCH resource(s) are not configured with any spatial relation and the UE is in RRC connected mode, the UE shall transmit PUSCH according to the spatial relation, if applicable, with a reference to the RS with ‘QCL-Type-D’ corresponding to the QCL assumption of the CORESET with the lowest ID in case CORESET(s) are configured on the CC.

For uplink, 16 HARQ processes per cell is supported by the UE.

### 6.1.1 Transmission schemes

Two transmission schemes are supported for PUSCH: codebook based transmission and non-codebook based transmission. The UE is configured with codebook based transmission when the higher layer parameter *txConfig* in *pusch-Config* is set to 'codebook', the UE is configured non-codebook based transmission when the higher layer parameter *txConfig* is set to 'nonCodebook'. If the higher layer parameter *txConfig* is not configured, the UE is not expected to be scheduled by DCI format 0\_1 or 0\_2. If PUSCH is scheduled by DCI format 0\_0, the PUSCH transmission is based on a single antenna port. Except if the higher layer parameter *enableDefaultBeamPlForPUSCH0\_0* is set 'enabled', the UE shall not expect PUSCH scheduled by DCI format 0\_0 in a BWP without configured PUCCH resource with *PUCCH-SpatialRelationInfo* in frequency range 2 in RRC connected mode.

#### 6.1.1.1 Codebook based UL transmission

For codebook based transmission, PUSCH can be scheduled by DCI format 0\_0, DCI format 0\_1, DCI format 0\_2 or semi-statically configured to operate according to Clause 6.1.2.3. If this PUSCH is scheduled by DCI format 0\_1, DCI format 0\_2, or semi-statically configured to operate according to Clause 6.1.2.3, the UE determines its PUSCH transmission precoder based on SRI, TPMI and the transmission rank, where the SRI, TPMI and the transmission rank are given by DCI fields of SRS resource indicator and Precoding information and number of layers in clause 7.3.1.1.2 and 7.3.1.1.3 of [5, TS 38.212] for DCI format 0\_1 and 0\_2 or given by *srs-ResourceIndicator* and *precodingAndNumberOfLayers* according to clause 6.1.2.3. The *SRS-ResourceSet(s)* applicable for PUSCH scheduled by DCI format 0\_1 and DCI format 0\_2 are defined by the entries of the higher layer parameter *srs-ResourceSetToAddModList* and *srs-ResourceSetToAddModList-ForDCIFormat0\_2* in *SRS-config*, respectively. The TPMI is used to indicate the precoder to be applied over the layers {0…*ν*-1} and that corresponds to the SRS resource selected by the SRI when multiple SRS resources are configured, or if a single SRS resource is configured TPMI is used to indicate the precoder to be applied over the layers {0…*ν*-1} and that corresponds to the SRS resource. The transmission precoder is selected from the uplink codebook that has a number of antenna ports equal to higher layer parameter *nrofSRS-Ports* in SRS-Config, as defined in Clause 6.3.1.5 of [4, TS 38.211]. When the UE is configured with the higher layer parameter *txConfig* set to 'codebook', the UE is configured with at least one SRS resource. The indicated SRI in slot *n* is associated with the most recent transmission of SRS resource identified by the SRI, where the SRS resource is prior to the PDCCH carrying the SRI.

For codebook based transmission, the UE determines its codebook subsets based on TPMI and upon the reception of higher layer parameter *codebookSubset* in *pusch-Config* for PUSCH associated with DCI format 0\_1 and *codebookSubset-ForDCIFormat0\_2* in *pusch-Config* for PUSCH associated with DCI format 0\_2 which may be configured with *'*fullyAndPartialAndNonCoherent*'*, or *'*partialAndNonCoherent*'*, or 'nonCoherent' depending on the UE capability. The maximum transmission rank may be configured by the higher layer parameter *maxRank* in *pusch-Config* for PUSCH scheduled with DCI format 0\_1 and *maxRank-ForDCIFormat0\_2* for PUSCH scheduled with DCI format 0\_2*.*

A UE reporting its UE capability of 'partialAndNonCoherent' transmission shall not expect to be configured by either *codebookSubset* or *codebookSubset-ForDCIFormat0\_2* with 'fullyAndPartialAndNonCoherent*'*.

A UE reporting its UE capability of 'nonCoherent' transmission shall not expect to be configured by either *codebookSubset* or *codebookSubset-ForDCIFormat0\_2* with *'*fullyAndPartialAndNonCoherent*'* or with *'*partialAndNonCoherent'.

A UE shall not expect to be configured with the higher layer parameter *codebookSubset* or the higher layer parameter or *codebookSubset-ForDCIFormat0\_2* set to *'*partialAndNonCoherent' when higher layer parameter *nrofSRS-Ports* in an *SRS-ResourceSet* with *usage* set to 'codebook' indicates that two SRS antenna ports are configured.

For codebook based transmission, the UE may be configured with a single *SRS-ResourceSet* with *usage* set to 'codebook' and only one SRS resource can be indicated based on the SRI from within the SRS resource set. The maximum number of configured SRS resources for codebook based transmission is 2. If aperiodic SRS is configured for a UE, the SRS request field in DCI triggers the transmission of aperiodic SRS resources.

The UE shall transmit PUSCH using the same antenna port(s) as the SRS port(s) in the SRS resource indicated by the DCI format 0\_1 or 0\_2 or by *configuredGrantConfig* according to clause 6.1.2.3.

The DM-RS antenna ports  in Clause 6.4.1.1.3 of [4, TS38.211] are determined according to the ordering of DM-RS port(s) given by Tables 7.3.1.1.2-6 to 7.3.1.1.2-23 in Clause 7.3.1.1.2 of [5, TS 38.212].

When multiple SRS resources are configured by *SRS-ResourceSet* with *usage* set to 'codebook', the UE shall expect that higher layer parameters *nrofSRS-Ports* in *SRS-Resource* in *SRS-ResourceSet* shall be configured with the same value for all these SRS resources.

A UE can be configured to operate in either Mode 1 or Mode 2 upon reception of the higher layer parameter *ULFPTxModes*.

- For UL transmission Mode 1:

- the UE can be configured with one or two SRS resources with same number of SRS ports within an SRS resource set with *usage* set to ‘codebook’.

- For UL transmission Mode 2:

- the UE can be configured with one SRS resource or multiple SRS resources with same or different number of SRS ports within an SRS resource set with *usage* set to ‘*codebook*’.

- up to 2 different spatial relations (*maxNumberConfiguredSpatialRelations)* can be configured for all SRS resources with usage set to ‘codebook’.

- a maximum of 4 SRS resources are supported to an SRS resource set with *usage* set to ‘codebook’

#### 6.1.1.2 Non-Codebook based UL transmission

For non-codebook based transmission, PUSCH can be scheduled by DCI format 0\_0, DCI format 0\_1, DCI format 0\_2 or semi-statically configured to operate according to Clause 6.1.2.3. If this PUSCH is scheduled by DCI format 0\_1, DCI format 0\_2, or semi-statically configured to operate according to Clause 6.1.2.3, the UE can determine its PUSCH precoder and transmission rank based on the SRI when multiple SRS resources are configured, where the SRI is given by the SRS resource indicator in DCI according to clause 7.3.1.1.2 and 7.3.1.1.3 of [5, 38.212] for DCI format 0\_1 and DCI format 0\_2, or the SRI is given by *srs-ResourceIndicator* according to clause 6.1.2.3. The *SRS-ResourceSet(s)* applicable for PUSCH scheduled by DCI format 0\_1 and DCI format 0\_2 are defined by the entries of the higher layer parameter *srs-ResourceSetToAddModList* and *srs-ResourceSetToAddModList-ForDCIFormat0\_2* in *SRS-config*, respectively. The UE shall use one or multiple SRS resources for SRS transmission, where, in a SRS resource set, the maximum number of SRS resources which can be configured to the UE for simultaneous transmission in the same symbol and the maximum number of SRS resources are UE capabilities. The SRS resources transmitted simultaneously occupy the same RBs. Only one SRS port for each SRS resource is configured. Only one SRS resource set can be configured with higher layer parameter *usage* in *SRS-ResourceSet* set to 'nonCodebook'. The maximum number of SRS resources that can be configured for non-codebook based uplink transmission is 4. The indicated SRI in slot *n* is associated with the most recent transmission of SRS resource(s) identified by the SRI, where the SRS transmission is prior to the PDCCH carrying the SRI.

For non-codebook based transmission, the UE can calculate the precoder used for the transmission of SRS based on measurement of an associated NZP CSI-RS resource. A UE can be configured with only one NZP CSI-RS resource for the SRS resource set with higher layer parameter usage in *SRS-ResourceSet* set to 'nonCodebook' if configured.

- If aperiodic SRS resource set is configured, the associated NZP-CSI-RS is indicated via SRS request field in DCI format 0\_1 and 1\_1, as well as DCI format 0\_2 (if SRS request field is present) and DCI format 1\_2 (if SRS request field is present), where *AperiodicSRS-ResourceTrigger* and *AperiodicSRS-ResourceTriggerList* (indicating the association between aperiodic SRS triggering state(s) and SRS resource sets), triggered SRS resource(s) *srs-ResourceSetId*, *csi-RS* (indicating the associated *NZP-CSI-RS-ResourceId*) are higher layer configured in *SRS-ResourceSet*. The *SRS-ResourceSet(s)* associated with the SRS request by DCI format 0\_1 and 1\_1 are defined by the entries of the higher layer parameter *srs-ResourceSetToAddModList* and the *SRS-ResourceSet(s)* associated with the SRS request by DCI format 0\_2 and 1\_2 are defined by the entries of the higher layer parameter *srs-ResourceSetToAddModList-ForDCIFormat0\_2*. A UE is not expected to update the SRS precoding information if the gap from the last symbol of the reception of the aperiodic NZP-CSI-RS resource and the first symbol of the aperiodic SRS transmission is less than 42 OFDM symbols.

- If the UE configured with aperiodic SRS associated with aperiodic NZP CSI-RS resource, the presence of the associated CSI-RS is indicated by the SRS request field if the value of the SRS request field is not '00' as in Table 7.3.1.1.2-24 of [5, TS 38.212] and if the scheduling DCI is not used for cross carrier or cross bandwidth part scheduling. The CSI-RS is located in the same slot as the SRS request field. If the UE configured with aperiodic SRS associated with aperiodic NZP CSI-RS resource, any of the TCI states configured in the scheduled CC shall not be configured with 'QCL-TypeD'.

- If periodic or semi-persistent SRS resource set is configured, the *NZP-CSI-RS-ResourceId* for measurement is indicated via higher layer parameter *associatedCSI-RS* in *SRS-ResourceSet*.

The UE shall perform one-to-one mapping from the indicated SRI(s) to the indicated DM-RS ports(s) and their corresponding PUSCH layers {0 … ν-1} given by DCI format 0\_1 or by *configuredGrantConfig* according to clause 6.1.2.3 in increasing order.

The UE shall transmit PUSCH using the same antenna ports as the SRS port(s) in the SRS resource(s) indicated by SRI(s) given by DCI format 0\_1 or by *configuredGrantConfig* according to clause 6.1.2.3, where the SRS port in (*i*+1)-th SRS resource in the SRS resource set is indexed as .

The DM-RS antenna ports  in Clause 6.4.1.1.3 of [4, TS 38.211] are determined according to the ordering of DM-RS port(s) given by Tables 7.3.1.1.2-6 to 7.3.1.1.2-23 in Clause 7.3.1.1.2 of [5, TS 38.212].

For non-codebook based transmission, the UE does not expect to be configured with both *spatialRelationInfo* for SRS resource and *associatedCSI-RS* in *SRS-ResourceSet* for SRS resource set.

For non-codebook based transmission, the UE can be scheduled with DCI format 0\_1 when at least one SRS resource is configured in *SRS-ResourceSet* with *usage* set to 'nonCodebook'.

### 6.1.2 Resource allocation

#### 6.1.2.1 Resource allocation in time domain

When the UE is scheduled to transmit a transport block and no CSI report, or the UE is scheduled to transmit a transport block and a CSI report(s) on PUSCH by a DCI, the *Time domain resource assignment* field value *m* of the DCI provides a row index *m* + 1to an allocated table. The determination of the used resource allocation table is defined in Clause 6.1.2.1.1. The indexed row defines the slot offset *K2*, the start and length indicator *SLIV*, or directly the start symbol *S* and the allocation length *L*, the PUSCH mapping type, and the number of repetitions (if *numberofrepetitions* is present in the resource allocation table) to be applied in the PUSCH transmission.

When the UE is scheduled to transmit a PUSCH with no transport block and with a CSI report(s) by a *CSI request* field on a DCI, the *Time domain resource assignment* field value *m* of the DCI provides a row index *m* + 1to an allocated table which is defined by the higher layer configured *pusch-TimeDomainAllocationList* in *pusch-Config*. The indexed row defines the start and length indicator SLIV, and the PUSCH mapping type to be applied in the PUSCH transmission and the *K2* value is determined as , where  are the corresponding list entries of the higher layer parameter

- [*reportSlotOffsetList-r16-ForDCIFormat0\_2*, if PUSCH is scheduled by DCI format 0\_2;

- *reportSlotOffsetList-r16-ForDCIFormat0\_1*, if PUSCH is scheduled by DCI format 0\_1 and *reportSlotOffsetList-r16-ForDCIFormat0\_1* is configured];

- *reportSlotOffsetList*, [otherwise;]

in *CSI-ReportConfig* for the  triggered CSI Reporting Settings and  is the *(m+1)*th entry of .

- The slot *Ks* where the UE shall transmit the PUSCH is determined by *K2* as *Ks* = where *n* is the slot with the scheduling DCI, K*2* is based on the numerology of PUSCH, and  and  are the subcarrier spacing configurations for PUSCH and PDCCH, respectively,

- and the  for the {scheduling, scheduled} carrier pair is defined in clause 4.5 of [4, TS 38.211], and

- for PUSCH scheduled by DCI format 0\_1, if *PUSCHRepTypeIndicator-ForDCIFormat0\_1* is set to ‘*pusch-RepTypeB*’, the UE applies PUSCH repetition Type B procedure when determining the time domain resource allocation. For PUSCH scheduled by DCI format 0\_2, if *PUSCHRepTypeIndicator-ForDCIFormat0\_2* is set to ‘*pusch-RepTypeB*’, the UE applies PUSCH repetition Type B procedure when determining the time domain resource allocation. Otherwise, the UE applies PUSCH repetition Type A procedure when determining the time domain resource allocation for PUSCH scheduled by PDCCH.

- For PUSCH repetition Type A, the starting symbol *S* relative to the start of the slot, and the number of consecutive symbols *L* counting from the symbol *S* allocated for the PUSCH are determined from the start and length indicator *SLIV* of the indexed row:

if  then



else



where, and

- For PUSCH repetition Type B, the starting symbol *S* relative to the start of the slot, and the number of consecutive symbols *L* counting from the symbol *S* allocated for the PUSCH are provided by *startSymbol* and *length* of the indexed row of the resource allocation table, respectively.

- For PUSCH repetition Type A, the PUSCH mapping type is set to Type A or Type B as defined in Clause 6.4.1.1.3 of [4, TS 38.211] as given by the indexed row.

- For PUSCH repetition Type B, the PUSCH mapping type is set to Type B.

The UE shall consider the *S* and *L* combinations defined in table 6.1.2.1-1 as valid PUSCH allocations

Table 6.1.2.1-1: Valid *S* and *L* combinations

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| PUSCH mapping type | Normal cyclic prefix | | | Extended cyclic prefix | | |
| *S* | *L* | *S+L* | *S* | *L* | *S+L* |
| Type A | 0 | {4,…,14} | {4,…,14} (repetitionType A only) | 0 | {4,…,12} | {4,…,12} |
| Type B | {0,…,13} | {1,…,14} | {1,…,14} for repetition Type A, {1,…,27} for repetition Type B | {0,…, 11} | {1,…,12} | {1,…,12} |

For PUSCH repetition Type A, when transmitting PUSCH scheduled by DCI format 0\_1 or 0\_2 in PDCCH with CRC scrambled with C-RNTI, MCS-C-RNTI, or CS-RNTI with NDI=1, the number of repetitions *K* is determined as

- if *numberofrepetitions* is present in the resource allocation table, the number of repetitions K is equal to *numberofrepetitions*;

- elseif the UE is configured with *pusch-AggregationFactor*, the number of repetitions *K* is equal to *pusch-AggregationFactor*;

- otherwise *K=1*.

For PUSCH repetition Type A, in case *K>1,* the same symbol allocation is applied across the *K* consecutive slots and the PUSCH is limited to a single transmission layer. The UE shall repeat the TB across the *K* consecutive slots applying the same symbol allocation in each slot. The redundancy version to be applied on the *n*th transmission occasion of the TB, where n = 0, 1, … *K*-1, is determined according to table 6.1.2.1-2.

Table 6.1.2.1-2: Redundancy version for PUSCH transmission

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *rvid* indicated by the DCI scheduling the PUSCH | *rvid* to be applied to *n*th transmission occasion (repetition Type A) or *n*th actual repetition (repetition Type B) | | | |
| *n* mod 4 = 0 | *n* mod 4 = 1 | *n* mod 4 = 2 | *n* mod 4 = 3 |
| 0 | 0 | 2 | 3 | 1 |
| 2 | 2 | 3 | 1 | 0 |
| 3 | 3 | 1 | 0 | 2 |
| 1 | 1 | 0 | 2 | 3 |

When transmitting MsgA PUSCH on a non-initial UL BWP, if the UE is configured with *startSymbolAndLengthMsgAPO*, the UE shall determine the *S* and *L* from *startSymbolAndLengthMsgAPO*.

When transmitting MsgA PUSCH, if the UE is not configured with *startSymbolAndLengthMsgAPO*, and if the TDRA list *PUSCH-TimeDomainResourceAllocationList* is provided in *PUSCH-ConfigCommon*, the UE shall use *msgA-timeDomainAllocation* to indicate which values are used in the list. If *PUSCH-TimeDomainResourceAllocationList* is not provided in *PUSCH-ConfigCommon*, the UE shall use parameters *S* and *L* from table 6.1.2.1.1-2 where *msgA-timeDomainAllocation* indicates which values are used in the list. The time offset for PUSCH transmission is described in [6, TS38.213].

For PUSCH repetition Type A, a PUSCH transmission in a slot of a multi-slot PUSCH transmission is omitted according to the conditions in Clause 11.1 of [6, TS38.213].

For PUSCH repetition Type B, the number of nominal repetitions is given by *numberofrepetitions*. For the *n*-th nominal repetition, *n* = *0*, …, *numberofrepetitions* - 1,

- The slot where the nominal repetition starts is given by , and the starting symbol relative to the start of the slot is given by .

- The slot where the nominal repetition ends is given by , and the ending symbol relative to the start of the slot is given by .

Here is the slot where the PUSCH transmission starts, and is the number of symbols per slot as defined in Clause 4.3.2 of [4, TS38.211].

For PUSCH repetition Type B, the UE determines invalid symbol(s) for PUSCH repetition Type B transmission as follows:

- A symbol that is indicated as downlink by *tdd-UL-DL-ConfigurationCommon* or *tdd-UL-DL-ConfigurationDedicated* is considered as an invalid symbol for PUSCH repetition Type B transmission.

- [If a UE is configured with higher layer parameter *SlotFormatInficator,* the] UE may be configured with the higher layer parameter *InvalidSymbolPattern*, which provides a symbol level bitmap spanning one or two slots (higher layer parameter *symbols* given by *InvalidSymbolPattern*). A bit value equal to 1 in the symbol level bitmap *symbols* indicates that the corresponding symbol is an invalid symbol for PUSCH repetition Type B transmission. The UE may be additionally configured with a time-domain pattern (higher layer parameter *periodicityAndPattern* given by *InvalidSymbolPattern*), where each bit of *periodicityAndPattern* corresponds to a unit equal to a duration of the symbol level bitmap *symbols*, and a bit value equal to 1 indicates that the symbol level bitmap *symbols* is present in the unit. The *periodicityAndPattern* can be {1, 2, 4, 5, 8, 10, 20 or 40} units long, but maximum of 40ms. The first symbol of *periodicityAndPattern* every 40ms/P periods is a first symbol in frame 𝑛𝑓 mod 4 = 0, where P is the duration of *periodicityAndPattern* in units of ms. When *periodicityAndPattern* is not configured, for a symbol level bitmap spanning two slots, the bits of the first and second slots correspond respectively to even and odd slots of a radio frame, and for a symbol level bitmap spanning one slot, the bits of the slot correspond to every slot of a radio frame. If *InvalidSymbolPattern* is configured, when the UE applies the invalid symbol pattern is determined as follows:

- if *InvalidSymbolPatternIndicator-ForDCIFormat0\_1* is configured when the PUSCH is scheduled by DCI format 0\_1, or if *InvalidSymbolPatternIndicator-ForDCIFormat0\_2* is configured when the PUSCH is scheduled by DCI format 0\_2,

- if [invalid symbol pattern indicator] field is set 1, the UE applies the invalid symbol pattern;

- otherwise, the UE does not apply the invalid symbol pattern;

- otherwise, the UE applies the invalid symbol pattern.

For PUSCH repetition Type B, after determining the invalid symbol(s) for PUSCH repetition type B transmission for each of the *K* nominal repetitions, the remaining symbols are considered as potentially valid symbols for PUSCH repetition Type B transmission. [If the number of potentially valid symbols for PUSCH repetition type B transmission is greater than zero for a nominal repetition, the nominal repetition consists of one or more actual repetitions, where each actual repetition consists of a consecutive set of potentially valid symbols that can be used for PUSCH repetition Type B transmission within a slot.] An actual repetition is omitted according to the conditions in Clause 11.1 of [6, TS38.213]. The redundancy version to be applied on the *n*th actual repetition (with the counting including the actual repetitions that are omitted) is determined according to table 6.1.2.1-2.

If *pusch-TimeDomainAllocationList* in *pusch-Config* contains row indicating resource allocation for two to eight contiguous PUSCHs, *K2* indicates the slot where UE shall transmit the first PUSCH of the multiple PUSCHs. Each PUSCH has a separate SLIV and mapping type. The number of scheduled PUSCHs is signalled by the number of indicated valid SLIVs in the row of the *pusch-TimeDomainAllocationList* signalled in DCI format 0\_1.

When the UE configured with [*minimumSchedulingOffset*] in active UL BWP it applies a minimum scheduling offset restriction indicated by the [‘Minimum applicable scheduling offset indicator’] field in DCI format 0\_1 or 1\_1. When the UE configured with [*minimumSchedulingOffset*] in active UL BWP and it has not received [‘Minimum applicable scheduling offset indicator’] field in DCI format 0\_1 or 1\_1, the UE shall apply a minimum scheduling offset restriction indicated based on [‘Minimum applicable scheduling offset indicator’] value ‘0’. When the *minimum scheduling offset restriction* is applied the UE is not expected to be scheduled with a DCI in slot *n* to transmit a PUSCH scheduled with C-RNTI, CS-RNTI or MCS-C-RNTI with *K*2 smaller than the applicable minimum scheduling offset restriction *K*2min in slot *n*. The minimum scheduling restriction is not applied when PUSCH transmission is scheduled by RAR UL grant for RACH procedure, or when PUSCH is scheduled with TC-RNTI. The application delay of the change of the minimum scheduling offset restriction is determined in Section 5.3.1.

##### 6.1.2.1.1 Determination of the resource allocation table to be used for PUSCH

Table 6.1.2.1.1-1, Table 6.1.2.1.1-1A and Table 6.1.2.1.1-1B define which PUSCH time domain resource allocation configuration to apply.

Table 6.1.2.1.1-4 defines the subcarrier spacing specific values *j*. *j* is used in determination of in conjunction to table 6.1.2.1.1-2, for normal CP or table 6.1.2.1.1.-3 for extended CP, where is the subcarrier spacing configurations for PUSCH.

Table 6.1.2.1.1-5 defines the additional subcarrier spacing specific slot delay value for the first transmission of PUSCH scheduled by the RAR or by the fallback RAR. When the UE transmits a PUSCH scheduled by RAR or by the fallback RAR, the *Δ* value specific to the PUSCH subcarrier spacing *µPUSCH* is applied in addition to the *K2* value.

Table 6.1.2.1.1-1: Applicable PUSCH time domain resource allocation for common search space and DCI format 0\_0 in UE specific search space

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| RNTI | PDCCH search space | *pusch-ConfigCommon* includes *pusch-TimeDomainAllocationList* | *pusch-Config* includes *pusch-TimeDomainAllocationList* | PUSCH time domain resource allocation to apply |
| PUSCH scheduled by MAC RAR as described in clause 8.2 of [6, TS 38.213] or MAC fallback RAR as described in clause X.Y of [6, 38.213] or for MsgA PUSCH transmission | | No | - | Default A |
| Yes |  | *pusch-TimeDomainAllocationList* provided in *pusch-ConfigCommon* |
| C-RNTI, MCS-C-RNTI, TC-RNTI, CS-RNTI | Any common search space associated with CORESET 0 | No | - | Default A |
| Yes |  | *pusch-TimeDomainAllocationList* provided in *pusch-ConfigCommon* |
| C-RNTI, MCS-C-RNTI, TC-RNTI, CS-RNTI, SP-CSI-RNTI | Any common search space not associated with CORESET 0,  DCI format 0\_0 in  UE specific search space | No | No | Default A |
| Yes | No | *pusch-TimeDomainAllocationList* provided in *pusch-ConfigCommon* |
| No/Yes | Yes | *pusch-TimeDomainAllocationList* provided in *pusch-Config* |

Table 6.1.2.1.1-1A: Applicable PUSCH time domain resource allocation for DCI format 0\_1 in UE specific search space scrambled with C-RNTI, MCS-C-RNTI, CS-RNTI or SP-CSI-RNTI

|  |  |  |  |
| --- | --- | --- | --- |
| *pusch-ConfigCommon* includes *pusch-TimeDomainAllocationList* | *pusch-Config* includes *pusch-TimeDomainAllocationList* | *pusch-Config* includes *pusch-TimeDomainAllocationList* *-ForDCIformat0\_1* | PUSCH time domain resource allocation to apply |
| No | No | No | Default A |
| Yes | No | No | *pusch-TimeDomainAllocationList* provided in *pusch-ConfigCommon* |
| No/Yes | Yes | No | *pusch-TimeDomainAllocationList* provided in *pusch-Config* |
| No/Yes | No/Yes | Yes | *pusch-TimeDomainAllocationList-ForDCIformat0\_1* provided in *pusch-Config* |

Table 6.1.2.1.1-1B: Applicable PUSCH time domain resource allocation for DCI format 0\_2 in UE specific search space scrambled with C-RNTI, MCS-C-RNTI, CS-RNTI or SP-CSI-RNTI

|  |  |  |  |
| --- | --- | --- | --- |
| *pusch-ConfigCommon* includes *pusch-TimeDomainAllocationList* | *pusch-Config* includes *pusch-TimeDomainAllocationList* | *pusch-Config* includes *pusch-TimeDomainAllocationList* *-ForDCIformat0\_2* | PUSCH time domain resource allocation to apply |
| No | No | No | Default A |
| Yes | No | No | *pusch-TimeDomainAllocationList* provided in *pusch-ConfigCommon* |
| No/Yes | Yes | No | *pusch-TimeDomainAllocationList* provided in *pusch-Config* |
| No/Yes | No/Yes | Yes | *pusch-TimeDomainAllocationList-ForDCIformat0\_2* provided in *pusch-Config* |

Table 6.1.2.1.1-2: Default PUSCH time domain resource allocation A for normal CP

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Row index | PUSCH mapping type |  | *S* | *L* |
| 1 | Type A | *j* | 0 | 14 |
| 2 | Type A | *j* | 0 | 12 |
| 3 | Type A | *j* | 0 | 10 |
| 4 | Type B | *j* | 2 | 10 |
| 5 | Type B | *j* | 4 | 10 |
| 6 | Type B | *j* | 4 | 8 |
| 7 | Type B | *j* | 4 | 6 |
| 8 | Type A | *j*+1 | 0 | 14 |
| 9 | Type A | *j*+1 | 0 | 12 |
| 10 | Type A | *j*+1 | 0 | 10 |
| 11 | Type A | *j*+2 | 0 | 14 |
| 12 | Type A | *j*+2 | 0 | 12 |
| 13 | Type A | *j*+2 | 0 | 10 |
| 14 | Type B | *j* | 8 | 6 |
| 15 | Type A | *j*+3 | 0 | 14 |
| 16 | Type A | *j*+3 | 0 | 10 |

Table 6.1.2.1.1-3: Default PUSCH time domain resource allocation A for extended CP

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Row index | PUSCH mapping type | *K2* | *S* | *L* |
| 1 | Type A | *j* | 0 | 8 |
| 2 | Type A | *j* | 0 | 12 |
| 3 | Type A | *j* | 0 | 10 |
| 4 | Type B | *j* | 2 | 10 |
| 5 | Type B | *j* | 4 | 4 |
| 6 | Type B | *j* | 4 | 8 |
| 7 | Type B | *j* | 4 | 6 |
| 8 | Type A | *j*+1 | 0 | 8 |
| 9 | Type A | *j*+1 | 0 | 12 |
| 10 | Type A | *j*+1 | 0 | 10 |
| 11 | Type A | *j*+2 | 0 | 6 |
| 12 | Type A | *j*+2 | 0 | 12 |
| 13 | Type A | *j*+2 | 0 | 10 |
| 14 | Type B | *j* | 8 | 4 |
| 15 | Type A | *j*+3 | 0 | 8 |
| 16 | Type A | *j*+3 | 0 | 10 |

Table 6.1.2.1.1-4: Definition of value *j*

|  |  |
| --- | --- |
| *µPUSCH* | *j* |
| 0 | 1 |
| 1 | 1 |
| 2 | 2 |
| 3 | 3 |

Table 6.1.2.1.1-5: Definition of value *Δ*

|  |  |
| --- | --- |
| *µPUSCH* | *Δ* |
| 0 | 2 |
| 1 | 3 |
| 2 | 4 |
| 3 | 6 |

#### 6.1.2.2 Resource allocation in frequency domain

The UE shall determine the resource block assignment in frequency domain using the resource allocation field in the detected PDCCH DCI except for a PUSCH transmission scheduled by a RAR UL grant or fallbackRAR UL grant, in which case the frequency domain resource allocation is determined according to clause 8.3 of [6, 38.213] or clause X.Y of [6, 38.213] respectively. Three uplink resource allocation schemes type 0, type 1 and type 2 are supported. Uplink resource allocation scheme type 0 is supported for PUSCH only when transform precoding is disabled. Uplink resource allocation scheme type 1 and type 2 are supported for PUSCH for both cases when transform precoding is enabled or disabled.

If the scheduling DCI is configured to indicate the uplink resource allocation type as part of the *Frequency domain resource* assignment field by setting a higher layer parameter r*esourceAllocation* in *pusch-Config* to 'dynamicSwitch', for DCI format 0\_1 or setting a higher layer parameter *resourceAllocation-ForDCIFormat0\_2* in *pusch-Config* to 'dynamicswitch' for DCI format 0\_2, the UE shall use uplink resource allocation type 0 or type 1 as defined by this DCI field. Otherwise the UE shall use the uplink frequency resource allocation type as defined by the higher layer parameter *resourceAllocation* for DCI format 0\_1 or the higher layer parameter *resourceAllocation-ForDCIFormat0\_2* for DCI format 0\_2, except if *useInterlacePUSCH-Dedicated* is set to ‘enabled’, in which case uplink type 2 resource allocation is used.

The UE shall assume that when the scheduling PDCCH is received with DCI format 0\_0, then uplink resource allocation type 1 is used, except when any of the higher layer parameters *useInterlacePUSCH-Common* or *useInterlacePUSCH-Dedicated* are set to 'enabled' in which case uplink resource allocation type 2 is used.

The UE expects that either none or both of *useInterlacePUSCH-Common* and *useInterlacePUSCH-Dedicated* is set to 'enabled'.

The UE expects that either none or both of *useInterlacePUSCH-Common* and *useInterlacePUCCH-Common* is set to 'enabled'.

If a bandwidth part indicator field is not configured in the scheduling DCI or the UE does not support active bandwidth part change via DCI, the RB indexing for uplink type 0, type 1 and type 2 resource allocation is determined within the UE's active bandwidth part. If a bandwidth part indicator field is configured in the scheduling DCI and the UE supports active bandwidh part change via DCI, the RB indexing for uplink type 0, type 1, type 2 resource allocation is determined within the UE's bandwidth part indicated by bandwidth part indicator field value in the DCI. The UE shall upon detection of PDCCH intended for the UE determine first the uplink bandwidth part and then the resource allocation within the bandwidth part. RB numbering starts from the lowest RB in the determined uplink bandwidth part.

##### 6.1.2.2.1 Uplink resource allocation type 0

In uplink resource allocation of type 0, the resource block assignment information includes a bitmap indicating the Resource Block Groups (RBGs) that are allocated to the scheduled UE where a RBG is a set of consecutive virtual resource blocks defined by higher layer parameter *rbg-Size* configured in *pusch-Config* and the size of the bandwidth part as defined in Table 6.1.2.2.1-1.

Table 6.1.2.2.1-1: Nominal RBG size *P*

|  |  |  |
| --- | --- | --- |
| Bandwidth Part Size | Configuration 1 | Configuration 2 |
| 1 – 36 | *2* | 4 |
| 37 – 72 | 4 | 8 |
| 73 – 144 | 8 | 16 |
| 145 – 275 | 16 | 16 |

The total number of RBGs () for a uplink bandwidth part *i* of sizePRBs is given by  where

- the size of the first RBG is ,

- the size of the last RBG is if and *P* otherwise.

- the size of all other RBG is *P*.

The bitmap is of size bits with one bitmap bit per RBG such that each RBG is addressable. The RBGs shall be indexed in the order of increasing frequency of the bandwidth part and starting at the lowest frequency. The order of RBG bitmap is such that RBG 0 to RBG are mapped from MSB to LSB of the bitmap. The RBG is allocated to the UE if the corresponding bit value in the bitmap is 1, the RBG is not allocated to the UE otherwise.

In frequency range 1, only 'almost contiguous allocation' defined in [8, TS 38.101-1] is allowed as non-contiguous allocation per component carrier for UL RB allocation for CP-OFDM.

In frequency range 2, non-contiguous allocation per component carrier for UL RB allocation for CP-OFDM is not supported.

##### 6.1.2.2.2 Uplink resource allocation type 1

In uplink resource allocation of type 1, the resource block assignment information indicates to a scheduled UE a set of contiguously allocated non-interleaved virtual resource blocks within the active bandwidth part of size  PRBs except for the case when DCI format 0\_0 is decoded in any common search space in which case the size of the initial UL bandwidth part  shall be used.

An uplink type 1 resource allocation field consists of a resource indication value (*RIV*) corresponding to a starting virtual resource block () and a length in terms of contiguously allocated resource blocks. The resource indication value is defined by

if  then



else



where≥ 1 and shall not exceed.

When the DCI size for DCI format 0\_0 in USS is derived from the initial UL BWP with size  but applied to another active BWP with size of , an uplink type 1 resource block assignment field consists of a resource indication value (*RIV*) corresponding to a starting resource block and a length in terms of virtually contiguously allocated resource blocks .

The resource indication value is defined by

if  then



else



where, and where shall not exceed .

If , *K* is the maximum value from set {1, 2, 4, 8} which satisfies ; otherwise *K* = 1.

When the scheduling grant is received with DCI format 0\_2, an uplink type 1 resource allocation field consists of [TBD]. [If the resource allocation indicates the corresponding PUSCH is mapped to RB index , the UE shall assume the PUSCH is also mapped to PRB indexes to .]

##### 6.1.2.2.3 Uplink resource allocation type 2

In uplink resource allocation of type 2, the resource block assignment information defined in [5, TS 38.212] indicates to a UE a set of up to *M* interlace indices, and a set of up to *N* RB sets, where *M* and interlace indexing are defined in Clause 4.4.4.6 in [4, TS 38.211]. The UE shall determine the resource allocation in frequency domain as an intersection of the resource blocks of the indicated interlaces and the indicated set of RB sets and intra-cell guard bands defined in Clause 7 between the indicated RB sets, if any.

For µ=0, the resource block assignment information indicates to a UE a set of allocated interlace indices resource blocks. The resource allocation field in the scheduling grant consists of a resource indication value (*RIV*). For , the resource indication value corresponds to the starting interlace index *m0* and the number of contiguous interlace indices (). The resource indication value is defined by:

if then

else

For , the resource indication value corresponds to the starting interlace index *m0* and the set of values  according to Table 6.1.2.2.3-1.

Table 6.1.2.2.3-1: *m0* and  for .

|  |  |  |
| --- | --- | --- |
|  | *m0* |  |
| 0 | 0 | {0, 5} |
| 1 | 0 | {0, 1, 5, 6} |
| 2 | 1 | {0, 5} |
| 3 | 1 | {0, 1, 2, 3, 5, 6, 7, 8} |
| 4 | 2 | {0, 5} |
| 5 | 2 | {0, 1, 2, 5, 6, 7} |
| 6 | 3 | {0, 5} |
| 7 | 4 | {0, 5} |

For µ=1, the resource block assignment information includes a bitmap indicating the interlaces that are allocated to the scheduled UE. The bitmap is of size *M* bits with one bitmap bit per interlace such that each interlace is addressable, where *M* and interlace indexing is defined in Section 4.4.4.6 in [4, TS 38.211]. The order of interlace bitmap is such that interlace 0 to interlace are mapped from MSB to LSB of the bitmap. An interlace is allocated to the UE if the corresponding bit value in the bitmap is 1; otherwise the interlace is not allocated to the UE.

For both µ=0 and µ=1, bits in the resource block assignment information indicate to a UE a set of contiguously allocated RB sets for PUSCH scheduled by DCI 0\_1 and Type 1 and Type 2 configured grant. The resource allocation field consists of a resource indication value (*RIVRBset*). For , the resource indication value corresponds to the starting RB set () and the number of contiguous RB sets . The resource indication value is defined by;

if then

else

#### 6.1.2.3 Resource allocation for uplink transmission with configured grant

When PUSCH resource allocation is semi-statically configured by higher layer parameter *configuredGrantConfig* in *BWP-UplinkDedicated* information element, and the PUSCH transmission corresponding to a configured grant, the following higher layer parameters are applied in the transmission:

- For Type 1 PUSCH transmissions with a configured grant, the following parameters are given in *configuredGrantConfig* unless mentioned otherwise:

- For the determination of the PUSCH repetition type, if the higher layer parameter *PUSCHRepTypeIndicator-ForType1Configuredgrant* is configured and set to ‘*pusch-RepTypeB*’, PUSCH repetition type B is applied; otherwise, PUSCH repetition type A is applied;

- For PUSCH repetition type A, the selection of the time domain resource allocation table follows the rules for DCI format 0\_0 on UE specific search space, as defined in Clause 6.1.2.1.1.

- For PUSCH repetition type B, the selection of the time domain resource allocation table is as follows:

- If PUSCHRepTypeIndicator-ForDCIFormat0\_1 in pusch-Config is configured and set to ‘pusch-RepTypeB’, PUSCH-TimeDomainResourceAllocationList-ForDCIformat0\_1 in pusch-Config is used;

- Otherwise, PUSCH-TimeDomainResourceAllocationList-ForDCIformat0\_2 in pusch-Config is used.

- It is not expected that PUSCHRepTypeIndicator-ForType1Configuredgrant is configured with 'pusch-RepTypeB' when none of PUSCHRepTypeIndicator-ForDCIFormat0\_1 and PUSCHRepTypeIndicator-ForDCIFormat0\_2 in pusch-Config is set to 'pusch-RepTypeB'.

- The higher layer parameter *timeDomainAllocation* value *m* provides a row index m+1 pointing to the determined time domain resource allocation table, where the start symbol and length are determined following the procedure defined in Clause 6.1.2;

- Frequency domain resource allocation is determined by the *N* LSB bits in the higher layer parameter *frequencyDomainAllocation*, forming a bit sequence , where is the LSB, according to the procedure in Clause 6.1.2.2 and *N* is determined as the size of frequency domain resource assignment field in DCI format 0\_1 for a given resource allocation type indicated by *resourceAllocation,* except if *useInterlacePUSCH-Dedicated* is set to 'enabled', in which case uplink type 2 resource allocation is used*;*

- The *IMCS* is provided by higher layer parameter *mcsAndTBS;*

- Number of DM-RS CDM groups, DM-RS ports, SRS resource indication and DM-RS sequence initialization are determined as in Clause 7.3.1.1 of [5, TS 38.212], and the antenna port value, the bit value for DM-RS sequence initialization, precoding information and number of layers, SRS resource indicator are provided by *antennaPort, dmrs-SeqInitialization, precodingAndNumberOfLayers*, and *srs-ResourceIndicator* respectively;

- When frequency hopping is enabled, the frequency offset between two frequency hops can be configured by higher layer parameter *frequencyHoppingOffset.*

- For Type 2 PUSCH transmissions with a configured grant: the resource allocation follows the higher layer configuration according to [10, TS 38.321], and UL grant received on the DCI.

- The PUSCH repetition type and the time domain resource allocation table are determined by the PUSCH repetition type and the time domain resource allocation table associated with the UL grant received on the DCI, respectively, as defined in Clause 6.1.2.1.

For PUSCH transmissions with a Type 1 or Type 2 configured grant, the number of (nominal) repetitions *K* to be applied to the transmitted transport block is provided by the indexed row in the time domain resource allocation table if *numberofrepetitions* is present in the table; otherwise *K* is provided by the higher layer configured parameters *repK.*

The UE shall not transmit anything on the resources configured by *configuredGrantConfig* if the higher layers did not deliver a transport block to transmit on the resources allocated for uplink transmission without grant.

A set of allowed periodicities *P* are defined in [12, TS 38.331]. The higher layer parameter *cg-nrofSlots-r16*, provides the number of consecutive slots in which the same combination of start symbol and length and PUSCH mapping type applies within a configured grant period. The higher layer parameter *cg-nrofPUSCH-InSlot-r16* provides the number of consecutive PUSCH allocations within a slot, where the first PUSCH allocation follows the higher layer parameter *timeDomainAllocation*, and the remaining PUSCH allocations have the same length and the PUSCH mapping type, and are appended following the previous allocations without any gaps. The same combination of start symbol and PUSCH mapping time repeats over the consecutively allocated slots.

For operation with shared spectrum channel access where a UE is performing uplink transmission with configured grants in contiguous OFDM symbols on all resource blocks of an RB set, for the first such UL transmission the UE randomly determines a duration of a cyclic prefix extension *Text* to be applied for transmission according to [4, TS 38.211] from a set of values configured by higher layers according to the following rule:

- If the first such UL transmission is within a channel occupancy initiated by the gNB (defined in Clause 4 of [16, TS 37.213]), the set of values is determined by *cg-StartingFullBW-InsideCOT*;

- otherwise, the set of values is determined by *cg-StartingFullBW-OutsideCOT-r16*.

For operation with shared spectrum channel access where a UE is performing uplink transmission with configured grants in contiguous OFDM symbols on fewer than all resource blocks of an RB set, for the first such UL transmission the UE determines a duration of a cyclic prefix extension *Text* to be applied for transmission according to [4, TS 38.211] according to the following rule:

- If the first such UL transmission is within a channel occupancy initiated by the gNB (defined in Clause 4 of [16, TS 37.213]), the *Text* is equal to *cg-StartingPartialBW-InsideCOT*;

- otherwise, the *Text* is equal to *cg-StartingPartialBW-OutsideCOT-r16.*

6.1.2.3.1 Transport Block repetition for uplink transmissions of PUSCH repetition Type A with a configured grant

The procedures described in this clause apply to PUSCH transmissions of PUSCH repetition Type A with a Type 1 or Type 2 configured grant.

The higher layer parameter *repK-RV* defines the redundancy version pattern to be applied to the repetitions. If the parameter *repK-RV* is not provided in the *configuredGrantConfig*, the redundancy version for uplink transmissions with a configured grant shall be set to 0. Otherwise, for the *n*th transmission occasion among *K* repetitions, *n*=1, 2, …, *K*, it is associated with *(mod(n-1,4)+1)th* value in the configured RV sequence. If a configured grant configuration is configured with *Configuredgrantconfig-StartingfromRV0* set to *‘off’*, the initial transmission of a transport block may only start at the first transmission occasion of the *K* repetitions. Otherwise, the initial transmission of a transport block may start at

- the first transmission occasion of the *K* repetitions if the configured RV sequence is {0,2,3,1},

- any of the transmission occasions of the *K* repetitions that are associated with RV=0 if the configured RV sequence is {0,3,0,3},

- any of the transmission occasions of the *K* repetitions if the configured RV sequence is {0,0,0,0}, except the last transmission occasion when *K≥8*.

For any RV sequence, the repetitions shall be terminated after transmitting *K* repetitions, or at the last transmission occasion among the *K* repetitions within the period *P*, or from the starting symbol of the repetition that overlaps with a PUSCH with the same HARQ process scheduled by DCI format 0\_0, 0\_1 or 0\_2, whichever is reached first. The UE is not expected to be configured with the time duration for the transmission of *K* repetitions larger than the time duration derived by the periodicity *P*. If the UE determines that, for a transmission occasion, the number of symbols available for the PUSCH transmission in a slot is smaller than transmission duration *L*, the UE does not transmit the PUSCH in the transmission occasion.

For both Type 1 and Type 2 PUSCH transmissions with a configured grant, when *K >* 1*,* the UE shall repeat the TB across the *K* consecutive slots applying the same symbol allocation in each slot, except if the UE is provided with higher layer parameters *cg-nrofSlots-r16* and *cg-nrofPUSCH-InSlot-r16*, in which case the UE repeats the TB in the *repK* earliest consecutive transmission occasion candidates within the same configuration. A Type 1 or Type 2 PUSCH transmission with a configured grant in a slot is omitted according to the conditions in Clause 11.1 of [6, TS38.213].

6.1.2.3.2 Transport Block repetition for uplink transmissions of PUSCH repetition Type B with a configured grant

The procedures described in this Clause apply to PUSCH transmissions of PUSCH repetition type B with a Type 1 or Type 2 configured grant.

For PUSCH transmissions with a Type 1 or Type 2 configured grant, the nominal repetitions and the actual repetitions are determined according to the procedures for PUSCH repetition Type B defined in Clause 6.1.2.1. The higher layer configured parameters *repK-RV* defines the redundancy version pattern to be applied to the repetitions. If the parameter *repK-RV* is not provided in the *configuredGrantConfig*, the redundancy version for each actual repetition with a configured grant shall be set to 0. Otherwise, for the *n*th transmission occasion among all the actual repetitions (including the actual repetitions that are omitted) of the *K* nominal repetitions, it is associated with *(mod(n-1,4)+1)th* value in the configured RV sequence. If a configured grant configuration is configured with *Configuredgrantconfig-StartingfromRV0* set to *‘off’*, the initial transmission of a transport block may only start at the first transmission occasion of the actual repetitions. Otherwise, the initial transmission of a transport block may start at

- the first transmission occasion of the actual repetitions if the configured RV sequence is {0,2,3,1},

- any of the transmission occasions of the actual repetitions that are associated with RV=0 if the configured RV sequence is {0,3,0,3},

- any of the transmission occasions of the actual repetitions if the configured RV sequence is {0,0,0,0}, except the actual repetitions within the last nominal repetition when *K≥8*.

For any RV sequence, the repetitions shall be terminated after transmitting K nominal repetitions, or at the last transmission occasion among the *K* nominal repetitions within the period *P*, or from the starting symbol of a repetition that overlaps with a PUSCH with the same HARQ process scheduled by DCI format 0\_0, 0\_1 or 0\_2, whichever is reached first. The UE is not expected to be configured with the time duration for the transmission of *K* nominal repetitions larger than the time duration derived by the periodicity *P*.

### 6.1.3 UE procedure for applying transform precoding on PUSCH

For a PUSCH scheduled by RAR UL grant, or for a PUSCH scheduled by fallbackRAR UL grant, or for a PUSCH scheduled by DCI format 0\_0 with CRC scrambled by TC-RNTI, the UE shall consider the transform precoding either 'enabled' or 'disabled' according to the higher layer configured parameter *msg3-transformPrecoder.*

For a MsgA PUSCH, the UE shall consider the transform precoding either 'enabled' or 'disabled' according to the higher layer configured parameter *msgA-transformPrecoder.* If higher layer parameter *msgA-transformPrecoder* is not configured, the UE shall consider the transform precoding either 'enabled' or 'disabled' according to the higher layer configured parameter *msg3-transformPrecoder.*

For PUSCH transmission scheduled by a PDCCH with CRC scrambled by CS-RNTI with NDI=1, C-RNTI, or MCS-C-RNTI or SP-CSI-RNTI:

- If the DCI with the scheduling grant was received with DCI format 0\_0, the UE shall, for this PUSCH transmission, consider the transform precoding either enabled or disabled according to the higher layer configured parameter *msg3-transformPrecoder*.

- If the DCI with the scheduling grant was not received with DCI format 0\_0

- If the UE is configured with the higher layer parameter *transformPrecoder* in *pusch-Config*, the UE shall, for this PUSCH transmission, consider the transform precoding either enabled or disabled according to this parameter.

- If the UE is not configured with the higher layer parameter *transformPrecoder* in *pusch-Config*, the UE shall, for this PUSCH transmission, consider the transform precoding either enabled or disabled according to the higher layer configured parameter *msg3-transformPrecoder*.

For PUSCH transmission with a configured grant

- If the UE is configured with the higher layer parameter *transformPrecoder* in *configuredGrantConfig*, the UE shall, for this PUSCH transmission, consider the transform precoding either enabled or disabled according to this parameter.

- If the UE is not configured with the higher layer parameter *transformPrecoder* in *configuredGrantConfig*, the UE shall, for this PUSCH transmission, consider the transform precoding either enabled or disabled according to the higher layer configured parameter *msg3-transformPrecoder*.

### 6.1.4 Modulation order, redundancy version and transport block size determination

To determine the modulation order, target code rate, redundancy version and transport block size for the physical uplink shared channel, the UE shall first

- read the 5-bit modulation and coding scheme field in the DCI scheduling PUSCH or provided in a DCI activating a configured grant Type 2 PUSCH, or as provided by *mcsAndTBS* as described in Clause 6.1.2.3 for a configured grant Type 1 PUSCH to determine the modulation order  and target code rate (*R*) based on the procedure defined in Clause 6.1.4.1

- read redundancy version field (*rv*) in the DCI to determine the redundancy version for PUSCH scheduled by DCI, or determine the redundancy version according to Clause 6.1.2.3.1 for configured grant Type 1 and Type 2 PUSCH,

and second

- use the number of layers , the total number of allocated PRBs  to determine the transport block size based on the procedure defined in Clause 6.1.4.2.

Within a cell group, a UE is not required to handle PUSCH(s) transmissions in slot *sj* in serving cell-*j*, and for *j* = 0,1,2.. *J-1*, slot *sj* overlapping with any given point in time, if the following condition is not satisfied at that point in time:

,

where

*- J* is the number of configured serving cells belong to a frequency range

- for the *j-th* serving cell,

*- M* is the number of TB(s) transmitted in slot-*sj*.

*- Tslotμ(j)* =10-3/2*μ(j*), where *μ(j)* is the numerology for PUSCH(s) in slot *sj* of the *j*-th serving cell.

- for the *m*-th TB,

*- A* is the number of bits in the transport block as defined in Clause 6.2.1 [5, TS 38.212]

*- C* is the total number of code blocks for the transport block defined in Clause 5.2.2 [5, TS 38.212].

- is the number of scheduled code blocks for the transport block as defined in Clause 5.4.2.1 [5,38.212]

- [Mbps] is computed as the maximum data rate summed over all the carriers in the frequency range for any signaled band combination and feature set consistent with the configured servings cells, where the data rate value is given by the formula in Clause 4.1.2 in [13, TS 38.306], including the scaling factor *f(i).*

For a *j*-th serving cell, if higher layer parameter *processingType2Enabled* of *PUSCH-ServingCellConfig* is configured for the serving cell and set to *enable,* or if at least one *IMCS > W* for a PUSCH, where *W* = 28 for MCS tables 5.1.3.1-1 and 5.1.3.1-3, and *W* = 27 for MCS tables 5.1.3.1-2, 6.1.4.1-1, and 6.1.4.1-2, the UE is not required to handle PUSCH transmissions, if the following condition is not satisfied:

where

- is the number of symbols assigned to the PUSCH

- *M* is the number of TB in the PUSCH

- where μ is the numerology of the PUSCH

- for the *m*-th TB,

- *A* is the number of bits in the transport block as defined in Clause 6.2.1 [5, TS 38.212]

- *C* is the total number of code blocks for the transport block defined in Clause 5.2.2 [5, TS 38.212]

- is the number of scheduled code blocks for the transport block as defined in Clause 5.4.2.1 [5, TS 38.212]

- [Mbps] is computed as the maximum data rate for a carrier in the frequency band of the serving cell for any signaled band combination and feature set consistent with the serving cell, where the data rate value is given by the formula in Clause 4.1.2 in [13, TS 38.306], including the scaling factor *f(i).*

#### 6.1.4.1 Modulation order and target code rate determination

For a PUSCH scheduled by RAR UL grant or

for a PUSCH scheduled by a fallbackRAR UL grant or

for a MsgA PUSCH transmission, or

for a PUSCH scheduled by a DCI format 0\_0 with CRC scrambled by C-RNTI, MCS-C-RNTI, TC-RNTI, CS-RNTI, or

for a PUSCH scheduled by a DCI format 0\_1 for DCI format 0\_2 with CRC scrambled by C-RNTI, MCS-C-RNTI, CS-RNTI, SP-CSI-RNTI, or

for a PUSCH with configured grant using CS-RNTI, and

if transform precoding is disabled for this PUSCH transmission according to Clause 6.1.3

- if *mcs-Table-ForDCIFormat0\_2* in *pusch-Config* is set to 'qam256', and PUSCH is scheduled by a PDCCH with DCI format 0\_2 with CRC scrambled by C-RNTI or SP-CSI-RNTI,

- the UE shall use *IMCS* and Table 5.1.3.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel;

- elseif the UE is not configured with MCS-C-RNTI, *mcs-Table-ForDCIFormat0\_2* in *pusch-Config* is set to 'qam64LowSE', and the PUSCH is scheduled by a PDCCH by a PDCCH with DCI format 0\_2 with CRC scrambled by C-RNTI or SP-CSI-RNTI,

- the UE shall use *IMCS* and Table 5.1.3.1-3 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif *mcs-Table* in *pusch-Config* is set to 'qam256', and PUSCH is scheduled by a PDCCH with DCI format 0\_1 with CRC scrambled by C-RNTI or SP-CSI-RNTI,

- the UE shall use *IMCS* and Table 5.1.3.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif the UE is not configured with MCS-C-RNTI, *mcs-Table* in *pusch-Config* is set to 'qam64LowSE', and the PUSCH is scheduled by a PDCCH with a DCI format other than DCI format 0\_2 in a UE-specific search space with CRC scrambled by C-RNTI or SP-CSI-RNTI,

- the UE shall use *IMCS* and Table 5.1.3.1-3 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif the UE is configured with MCS-C-RNTI, and the PUSCH is scheduled by a PDCCH with CRC scrambled by MCS-C-RNTI,

- the UE shall use *IMCS* and Table 5.1.3.1-3 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif *mcs-Table* in *configuredGrantConfig* is set to 'qam256',

- if PUSCH is scheduled by a PDCCH with CRC scrambled by CS-RNTI or

- if PUSCH is transmitted with configured grant

- the UE shall use *IMCS* and Table 5.1.3.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif *mcs-Table* in *configuredGrantConfig* is set to 'qam64LowSE',

- if PUSCH is scheduled by a PDCCH with CRC scrambled by CS-RNTI or

- if PUSCH is transmitted with configured grant,

- the UE shall use *IMCS* and Table 5.1.3.1-3 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif for a MsgA PUSCH transmission,

- the UE shall use higher layer parameter *MsgA-MCS* for *IMCS* and Table 5.1.3.1-1 to determine the Target code rate (*R*) used in the physical uplink shared channel.

- the UE shall use *q=2* for determining modulation order *Qm* in Table 5.1.3.1-1.

- else

- the UE shall use *IMCS* and Table 5.1.3.1-1 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

else

- if *mcs-TableTransformPrecoder-ForDCIFormat0\_2* in *pusch-Config* is set to 'qam256', and PUSCH is scheduled by a PDCCH with DCI format 0\_2 with CRC scrambled by C-RNTI or SP-CSI-RNTI,

- the UE shall use *IMCS* and Table 5.1.3.1.-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif the UE is not configured with MCS-C-RNTI, *mcs-Table-ForDCIFormat0\_2* in *pusch-Config* is set to 'qam64LowSE', and the PUSCH is scheduled by a PDCCH with DCI format 0\_2 with CRC scrambled by C-RNTI or SP-CSI-RNTI,

- the UE shall use *IMCS* and Table 6.1.4.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif *mcs-TableTransformPrecoder* in *pusch-Config* is set to 'qam256', and PUSCH is scheduled by a PDCCH with DCI format 0\_1 with CRC scrambled by C-RNTI or SP-CSI-RNTI,

- the UE shall use *IMCS* and Table 5.1.3.1.-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif the UE is not configured with MCS-C-RNTI, *mcs-TableTransformPrecoder* in *pusch-Config* is set to 'qam64LowSE', and the PUSCH is scheduled by a PDCCH with a DCI format other than DCI format 0\_2 in a UE-specific search space with CRC scrambled by C-RNTI or SP-CSI-RNTI,

- the UE shall use *IMCS* and Table 6.1.4.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif the UE is configured with MCS-C-RNTI, and the PUSCH is scheduled by a PDCCH with CRC scrambled by MCS-C-RNTI,

- the UE shall use *IMCS* and Table 6.1.4.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif *mcs-TableTransformPrecoder* in *configuredGrantConfig* is set to 'qam256',

- if PUSCH is scheduled by a PDCCH with CRC scrambled by CS-RNTI or

- if PUSCH is transmitted with configured grant,

- the UE shall use *IMCS* and Table 5.1.3.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif *mcs-TableTransformPrecoder* in *configuredGrantConfig* is set to 'qam64LowSE',

- if PUSCH is scheduled by a PDCCH with CRC scrambled by CS-RNTI or

- if PUSCH is transmitted with configured grant,

- the UE shall use *IMCS* and Table 6.1.4.1-2 to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

- elseif for a MsgA PUSCH transmission,

- the UE shall use higher layer parameter *MsgA-MCS* for *IMCS* and Table 6.1.4.1-1 to determine the Target code rate (*R*) used in the physical uplink shared channel.

- the UE shall use *q=2* for determining modulation order *Qm* in Table 6.1.4.1-1.

- else

- the UE shall use *IMCS* and Table 6.1.4.1-1to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical uplink shared channel.

end

For Table 6.1.4.1-1 and Table 6.1.4.1-2, if higher layer parameter *tp-pi2BPSK* is configured, *q* = 1 otherwise *q*=2.

Table 6.1.4.1-1: MCS index table for PUSCH with transform precoding and 64QAM

|  |  |  |  |
| --- | --- | --- | --- |
| MCS Index *IMCS* | Modulation Order  *Qm* | Target code Rate R x 1024 | Spectral  efficiency |
| **0** | q | 240/ q | 0.2344 |
| **1** | q | 314/ q | 0.3066 |
| **2** | 2 | 193 | 0.3770 |
| **3** | 2 | 251 | 0.4902 |
| **4** | 2 | 308 | 0.6016 |
| **5** | 2 | 379 | 0.7402 |
| **6** | 2 | 449 | 0.8770 |
| **7** | 2 | 526 | 1.0273 |
| **8** | 2 | 602 | 1.1758 |
| **9** | 2 | 679 | 1.3262 |
| **10** | ~~4~~ | 340 | 1.3281 |
| **11** | 4 | 378 | 1.4766 |
| **12** | 4 | 434 | 1.6953 |
| **13** | 4 | 490 | 1.9141 |
| **14** | 4 | 553 | 2.1602 |
| **15** | 4 | 616 | 2.4063 |
| **16** | 4 | 658 | 2.5703 |
| **17** | 6 | 466 | 2.7305 |
| **18** | 6 | 517 | 3.0293 |
| **19** | 6 | 567 | 3.3223 |
| **20** | 6 | 616 | 3.6094 |
| **21** | 6 | 666 | 3.9023 |
| **22** | 6 | 719 | 4.2129 |
| **23** | 6 | 772 | 4.5234 |
| **24** | 6 | 822 | 4.8164 |
| **25** | 6 | 873 | 5.1152 |
| **26** | 6 | 910 | 5.3320 |
| **27** | 6 | 948 | 5.5547 |
| **28** | q | reserved | |
| **29** | 2 | reserved | |
| **30** | 4 | reserved | |
| **31** | 6 | reserved | |

Table 6.1.4.1-2: MCS index table 2 for PUSCH with transform precoding and 64QAM

|  |  |  |  |
| --- | --- | --- | --- |
| MCS Index *IMCS* | Modulation Order  *Qm* | Target code Rate R x 1024 | Spectral  efficiency |
| **0** | *q* | 60/*q* | 0.0586 |
| **1** | *q* | 80/*q* | 0.0781 |
| **2** | *q* | 100/*q* | 0.0977 |
| **3** | *q* | 128/*q* | 0.1250 |
| **4** | *q* | 156/*q* | 0.1523 |
| **5** | *q* | 198/*q* | 0.1934 |
| **6** | 2 | 120 | 0.2344 |
| **7** | 2 | 157 | 0.3066 |
| **8** | 2 | 193 | 0.3770 |
| **9** | 2 | 251 | 0.4902 |
| **10** | 2 | 308 | 0.6016 |
| **11** | 2 | 379 | 0.7402 |
| **12** | 2 | 449 | 0.8770 |
| **13** | 2 | 526 | 1.0273 |
| **14** | 2 | 602 | 1.1758 |
| **15** | 2 | 679 | 1.3262 |
| **16** | 4 | 378 | 1.4766 |
| **17** | 4 | 434 | 1.6953 |
| **18** | 4 | 490 | 1.9141 |
| **19** | 4 | 553 | 2.1602 |
| **20** | 4 | 616 | 2.4063 |
| **21** | 4 | 658 | 2.5703 |
| **22** | 4 | 699 | 2.7305 |
| **23** | 4 | 772 | 3.0156 |
| **24** | 6 | 567 | 3.3223 |
| **25** | 6 | 616 | 3.6094 |
| **26** | 6 | 666 | 3.9023 |
| **27** | 6 | 772 | 4.5234 |
| **28** | q | reserved | |
| **29** | 2 | reserved | |
| **30** | 4 | reserved | |
| **31** | 6 | reserved | |

#### 6.1.4.2 Transport block size determination

For a PUSCH scheduled by RAR UL grant or

for a PUSCH scheduled by fallbackRAR UL grant or

for a PUSCH scheduled by a DCI format 0\_0 with CRC scrambled by C-RNTI, MCS-C-RNTI, TC-RNTI, CS-RNTI, or

for a PUSCH scheduled by a DCI format 0\_1 or DCI format 0\_2 with CRC scrambled by C-RNTI, MCS-C-RNTI, CS-RNTI, SP-CSI-RNTI, or

for a PUSCH transmission with configured grant, or

for a MsgA PUSCH transmission,

if

- and transform precoding is disabled and Table 5.1.3.1-2 is used, or

-  and transform precoding is disabled and a table other than Table 5.1.3.1-2 is used, or

-  and transform precoding is enabled, the UE shall first determine the TBS as specified below:

The UE shall first determine the number of REs (*NRE*) within the slot:

- A UE first determines the number of REs allocated for PUSCH within a PRB  by

- , where is the number of subcarriers in the frequency domain in a physical resource block,  is the number of symbols *L* of the PUSCH allocation according to Clause 6.1.2.1 for scheduled PUSCH of Clause 6.1.2.3 for configured PUSCH,  is the number of REs for DM-RS per PRB in the allocated duration including the overhead of the DM-RS CDM groups without data, as described for PUSCH with a configured grant in Clause 6.1.2.3 or as indicated by DCI format 0\_1 or DCI format 0\_2 or as described for DCI format 0\_0 in Clause 6.2.2, and  is the overhead configured by higher layer parameter *xOverhead* in*PUSCH-ServingCellConfig*. If the  is not configured (a value from 6, 12, or 18), the  is assumed to be 0. For Msg3 transmission the  is always set to 0.

- A UE determines the total number of REs allocated for PUSCH  by where  is the total number of allocated PRBs for the UE.

- Next, proceed with steps 2-4 as defined in Clause 5.1.3.2

else if

-  and transform precoding is disabled and Table 5.1.3.1-2 is used, or

-  and transform precoding is enabled,

- the TBS is assumed to be as determined from the DCI transported in the latest PDCCH for the same transport block using . If there is no PDCCH for the same transport block using , and if the initial PUSCH for the same transport block is transmitted with configured grant,

- the TBS shall be determined from *configuredGrantConfig* for a configured grant Type 1 PUSCH.

- the TBS shall be determined from the most recent PDCCH scheduling a configured grant Type 2 PUSCH.

else

- the TBS is assumed to be as determined from the DCI transported in the latest PDCCH for the same transport block using . If there is no PDCCH for the same transport block using , and if the initial PUSCH for the same transport block is transmitted with configured grant,

- the TBS shall be determined from *configuredGrantConfig* for a configured grant Type 1 PUSCH.

- the TBS shall be determined from the most recent PDCCH scheduling a configured grant Type 2 PUSCH.

### 6.1.5 Code block group based PUSCH transmission

#### 6.1.5.1 UE procedure for grouping of code blocks to code block groups

If a UE is configured to transmit code block group (CBG) based transmissions by receiving the higher layer parameter *codeBlockGroupTransmission* in *PUSCH-ServingCellConfig*, the UE shall determine the number of CBGs for a PUSCH transmission as

,

where *N* is the maximum number of CBGs per transport block as configured by *maxCodeBlockGroupsPerTransportBlock* in *PUSCH-ServingCellConfig*, and *C* is the number of code blocks in the PUSCH according to the procedure defined in Clause 6.2.3 of [5, TS 38.212].

Define , , and .

If , CBG *m*, , consists of code blocks with indices . CBG *m*, , consists of code blocks with indices .

#### 6.1.5.2 UE procedure for transmitting code block group based transmissions

If a UE is configured to transmit code block group based transmissions by receiving the higher layer parameter *codeBlockGroupTransmission* in *PUSCH-ServingCellConfig*,

- For an initial transmission of a TB as indicated by the *New Data Indicator* field of the scheduling DCI, the UE may expect that the *CBGTI* field indicates all the CBGs of the TB are to be transmitted, and the UE shall include all the code block groups of the TB.

- For a retransmission of a TB as indicated by the *New Data Indicator* field of the scheduling DCI, the UE shall include only the CBGs indicated by the *CBGTI* field of the scheduling DCI.

A bit value of 0' in the *CBGTI* field indicates that the corresponding CBG is not to be transmitted and 1' indicates that it is to be transmitted. The order of *CBGTI* field bits is such that the CBGs are mapped in order from CBG#0 onwards starting from the MSB.

## 6.2 UE reference signal (RS) procedure

### 6.2.1 UE sounding procedure

The UE may be configured with one or more Sounding Reference Signal (SRS) resource sets as configured by the higher layer parameter *SRS-ResourceSet*. For each SRS resource set, a UE may be configured with SRS resources (higher layer parameter *SRS-Resource*), where the maximum value of K is indicated by UE capability[13, 38.306] except when SRS is configured with the higher layer parameter [SRS-for-positioning] in which case the maximum value of K is 16. The SRS resource set applicability is configured by the higher layer parameter *usage* in *SRS-ResourceSet.* When the higher layer parameter *usage* is set to 'beamManagement'*,* only one SRS resource in each of multiple SRS sets may be transmitted at a given time instant, but the SRS resources in different SRS resource sets with the same time domain behaviour in the same BWP may be transmitted simultaneously.

For aperiodic SRS at least one state of the DCI field is used to select at least one out of the configured SRS resource set(s).

The following SRS parameters are semi-statically configurable by higher layer parameter *SRS-Resource*.

- *srs-ResourceId* determines SRS resource configuration identity.

- Number of SRS ports as defined by the higher layer parameter *nrofSRS-Ports* and described in Clause 6.4.1.4 of [4, TS 38.211]. If not configured, *nrofSRS-Ports* is 1.

*-* Time domain behaviour of SRS resource configuration as indicated by the higher layer parameter *resourceType*, which may be periodic, semi-persistent, aperiodic SRS transmission as defined in Clause 6.4.1.4 of [4, TS 38.211].

- Slot level periodicity and slot level offset as defined by the higher layer parameters *periodicityAndOffset-p* or *periodicityAndOffset-sp* for an SRS resource of type periodic or semi-persistent. The UE is not expected to be configured with SRS resources in the same SRS resource set *SRS-ResourceSet* with different slot level periodicities. For an *SRS-ResourceSet* configured with higher layer parameter *resourceType* set to 'aperiodic', a slot level offset is defined by the higher layer parameter *slotOffset*.

- Number of OFDM symbols in the SRS resource, starting OFDM symbol of the SRS resource within a slot including repetition factor R as defined by the higher layer parameter *resourceMapping* and described in Clause 6.4.1.4 of [4, TS 38.211]. If *R* is not configured, then *R* is equal to the number of OFDM symbols in the SRS resource.

- SRS bandwidth and , as defined by the higher layer parameter *freqHopping* and described in Clause 6.4.1.4 of [4, TS 38.211]. If not configured, then= 0.

- Frequency hopping bandwidth, , as defined by the higher layer parameter *freqHopping* and described in Clause 6.4.1.4 of [4, TS 38.211]. If not configured, then = 0.

- Defining frequency domain position and configurable shift, as defined by the higher layer parameters *freqDomainPosition* and *freqDomainShift, respectively,* and described in Clause 6.4.1.4 of [4, TS 38.211]. If *freqDomainPosition* is not configured, *freqDomainPosition* is zero.

- Cyclic shift, as defined by the higher layer parameter *cyclicShift-n2*, *cyclicShift-n4, or cyclicShift-n8* for transmission comb value 2, 4 and 8, respectively, and described in Clause 6.4.1.4 of [4, TS 38.211].

- Transmission comb value as defined by the higher layer parameter *transmissionComb* described in Clause 6.4.1.4 of [4, TS 38.211].

- Transmission comb offset as defined by the higher layer parameter *combOffset-n2*, *combOffset-n4*, or *combOffset-n8* for transmission comb value 2, 4, or 8 respectively, and described in Clause 6.4.1.4 of [4, TS 38.211].

- SRS sequence ID as defined by the higher layer parameter *sequenceId* in Clause 6.4.1.4 of [4].

- The configuration of the spatial relation between a reference RS and the target SRS, where the higher layer parameter *spatialRelationInfo*, if configured, contains the ID of the reference RS. The reference RS may be an SS/PBCH block, CSI-RS configured on serving cell indicated by higher layer parameter *servingCellId* if present, same serving cell as the target SRS otherwise, or an SRS configured on uplink BWP indicated by the higher layer parameter *uplinkBWP*, and serving cell indicated by the higher layer parameter *servingCellId* if present, same serving cell as the target SRS otherwise. When SRS is configured by the higher layer parameter [SRS-for-positioning] the reference RS may also be a DL PRS configured on a serving cell, an SS/PBCH block or a DL PRS of a non-serving cell indicated by a higher layer parameter.

The UE may be configured by the higher layer parameter *resourceMapping* in *SRS-Resource* with an SRS resource occupying  adjacent symbols within the last 6 symbols of the slot, where all antenna ports of the SRS resources are mapped to each symbol of the resource. When the SRS is configured with the higher layer parameter [SRS-for-positioning] the higher layer parameter *resourceMapping* in *SRS-Resource* with an SRS resource occupying adjacent symbols anywhere within the slot.

If a UE is not configured with [intraUEPrioritization] and PUSCH and SRS are transmitted in the same slot on a serving cell, the UE may only be configured to transmit SRS after the transmission of the PUSCH and the corresponding DM-RS.

If a UE is configured with [intraUEPrioritization] and a PUSCH transmission would overlap in time with an SRS transmission on a serving cell, the UE does not transmit the SRS in the overlapping symbol(s).

For a UE configured with one or more SRS resource configuration(s), and when the higher layer parameter *resourceType* in *SRS-Resource* is set to 'periodic':

- if the UE is configured with the higher layer parameter *spatialRelationInfo* containing the ID of a reference'ssb-Index', the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the reception of the reference SS/PBCH block, if the higher layer parameter *spatialRelationInfo* contains the ID of a reference 'csi-RS-Index', the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the reception of the reference periodic CSI-RS or of the reference semi-persistent CSI-RS, if the higher layer parameter *spatialRelationInfo* containing the ID of a reference 'srs', the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the transmission of the reference periodic SRS. When the SRS is configured by the higher layer parameter [SRS-for-positioning] and if the higher layer parameter *spatialRelationInfo* contains the ID of a reference ’*DL-PRS-ResourceId*’, the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the reception of the reference DL PRS.

For a UE configured with one or more SRS resource configuration(s), and when the higher layer parameter *resourceType* in *SRS-Resource* is set to 'semi-persistent':

- when a UE receives an activation command, as described in clause 6.1.3.17 of [10, TS 38.321], for an SRS resource, and when the UE would transmit a PUCCH with HARQ-ACK information in slot *n* corresponding to the PDSCH carrying the activation command is transmitted in slot n, the corresponding actions in [10, TS 38.321] and the UE assumptions on SRS transmission corresponding to the configured SRS resource set shall be applied starting from the first slot that is after slot where ** is the SCS configuration for the PUCCH. The activation command also contains spatial relation assumptions provided by a list of references to reference signal IDs, one per element of the activated SRS resource set. Each ID in the list refers to a reference SS/PBCH block, NZP CSI-RS resource configured on serving cell indicated by *Resource Serving Cell ID* field in the activation command if present, same serving cell as the SRS resource set otherwise, or SRS resource configured on serving cell and uplink bandwidth part indicated by Resource *Serving Cell ID* field and *Resource BWP ID* field in the activation command if present, same serving cell and bandwidth part as the SRS resource set otherwise. When the SRS is configured with the higher layer parameter [SRS-for-positioning], each ID in the list of reference signal IDs may also refer to a reference SS/PBCH block of a non-serving cell or DL PRS of a serving or non-serving cell indicated by a higher layer parameter.

- if an SRS resource in the activated resource set is configured with the higher layer parameter *spatialRelationInfo*, the UE shall assume that the ID of the reference signal in the activation command overrides the one configured in *spatialRelationInfo.*

- when a UE receives a deactivation command [10, TS 38.321] for an activated SRS resource set, and when the UE would transmit a PUCCH with HARQ-ACK information in slot *n* corresponding to the PDSCH carrying the deactivation command, the corresponding actions in [10, TS 38.321] and UE assumption on cessation of SRS transmission corresponding to the deactivated SRS resource set shall apply starting from the first slot that is after slot where ** is the SCS configuration for the PUCCH.

- if the UE is configured with the higher layer parameter *spatialRelationInfo* containing the ID of a reference 'ssb-Index', the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the reception of the reference SS/PBCH block, if the higher layer parameter *spatialRelationInfo* contains the ID of a reference 'csi-RS-Index', the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the reception of the reference periodic CSI-RS or of the reference semi-persistent CSI-RS, if the higher layer parameter *spatialRelationInfo* contains the ID of a reference 'srs', the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the transmission of the reference periodic SRS or of the reference semi-persistent SRS. When the SRS is configured by the higher layer parameter [SRS-for-positioning] and if the higher layer parameter *spatialRelationInfo* contains the ID of a reference ’*DL-PRS-ResourceId*’, the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the reception of the reference DL PRS.

If the UE has an active semi-persistent SRS resource configuration and has not received a deactivation command, the semi-persistent SRS configuration is considered to be active in the UL BWP which is active, otherwise it is considered suspended.

For a UE configured with one or more SRS resource configuration(s), and when the higher layer parameter *resourceType* in *SRS-Resource* is set to 'aperiodic':

- the UE receives a configuration of SRS resource sets,

- the UE receives a downlink DCI, a group common DCI, or an uplink DCI based command where a codepoint of the DCI may trigger one or more SRS resource set(s). For SRS in a resource set with usage set to 'codebook' or 'antennaSwitching', the minimal time interval between the last symbol of the PDCCH triggering the aperiodic SRS transmission and the first symbol of SRS resource is *N2*. Otherwise, the minimal time interval between the last symbol of the PDCCH triggering the aperiodic SRS transmission and the first symbol of SRS resource is *N2* + 14. The minimal time interval in units of OFDM symbols is counted based on the minimum subcarrier spacing between the PDCCH and the aperiodic SRS.

- If the UE receives the DCI triggering aperiodic SRS in slot *n*, the UE transmits aperiodic SRS in each of the triggered SRS resource set(s) in slot  where

*- k* is configured via higher layer parameter *slotOffset* for each triggered SRS resources set and is based on the subcarrier spacing of the triggered SRS transmission, *µSRS* and *µPDCCH* are the subcarrier spacing configurations for triggered SRS and PDCCH carrying the triggering command respectively;

- and the  for the {scheduling, scheduled} carrier pair is defined in [4, TS 38.211] clause 4.5.

- if the UE is configured with the higher layer parameter *spatialRelationInfo* containing the ID of a reference 'ssb-Index', the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the reception of the reference SS/PBCH block, if the higher layer parameter *spatialRelationInfo* contains the ID of a reference 'csi-RS-Index', the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the reception of the reference periodic CSI-RS or of the reference semi-persistent CSI-RS, or of the latest reference aperiodic CSI-RS. If the higher layer parameter *spatialRelationInfo* contains the ID of a reference 'srs', the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the transmission of the reference periodic SRS or of the reference semi-persistent SRS or of the reference aperiodic SRS. When the SRS is configured by the higher layer parameter [SRS-for-positioning] and if the higher layer parameter *spatialRelationInfo* contains the ID of a reference ‘*DL-PRS-ResourceId*’, the UE shall transmit the target SRS resource with the same spatial domain transmission filter used for the reception of the reference DL PRS.

- when a UE receives an spatial relation update command, as described in clause 6.1.3.xx of [10, TS 38.321], for an SRS resource, and when the HARQ-ACK corresponding to the PDSCH carrying the update command is transmitted in slot n, the corresponding actions in [10, TS 38.321] and the UE assumptions on updating spatial relation for the SRS resource shall be applied for SRS transmission starting from the first slot that is after slot The update command contains spatial relation assumptions provided by a list of references to reference signal IDs, one per element of the updated SRS resource set. Each ID in the list refers to a reference SS/PBCH block, NZP CSI-RS resource configured on serving cell indicated by *Resource Serving Cell ID* field in the update command if present, same serving cell as the SRS resource set otherwise, or SRS resource configured on serving cell and uplink bandwidth part indicated by Resource *Serving Cell ID* field and *Resource BWP ID* field in the update command if present, same serving cell and bandwidth part as the SRS resource set otherwise.] When the UE is configured with the higher layer parameter *usage* in *SRS-ResourceSet* set to 'antennaSwitching', the UE shall not expect to be configured with different spatial relations for SRS resources in the same SRS resource set.

The UE is not expected to be configured with different time domain behavior for SRS resources in the same SRS resource set. The UE is also not expected to be configured with different time domain behavior between SRS resource and associated SRS resources set.

The SRS request field [5, TS38.212] in DCI format 0\_1, 1\_1, 0\_2 (if SRS request field is present), 1\_2 (if SRS request field is present) indicates the triggered SRS resource set given in Table 7.3.1.1.2-24 of [5, TS 38.212]. The 2-bit SRS request field [5, TS38.212] in DCI format 2\_3 indicates the triggered SRS resource set given in Clause 7.3 of [5, TS 38.212] if the UE is configured with higher layer parameter *srs-TPC-PDCCH-Group* set to 'typeB', or indicates the SRS transmission on a set of serving cells configured by higher layers if the UE is configured with higher layer parameter *srs-TPC-PDCCH-Group* set to 'typeA'.

For PUCCH and SRS on the same carrier, a UE shall not transmit SRS when semi-persistent and periodic SRS are configured in the same symbol(s) with PUCCH carrying only CSI report(s), or only L1-RSRP report(s), or only L1-SINR report(s). A UE shall not transmit SRS when semi-persistent or periodic SRS is configured or aperiodic SRS is triggered to be transmitted in the same symbol(s) with PUCCH carrying HARQ-ACK, link recovery request (as defined in clause 9.2.4 of [6, 38.213]) and/or SR. In the case that SRS is not transmitted due to overlap with PUCCH, only the SRS symbol(s) that overlap with PUCCH symbol(s) are dropped. PUCCH shall not be transmitted when aperiodic SRS is triggered to be transmitted to overlap in the same symbol with PUCCH carrying semi-persistent/periodic CSI report(s) or semi-persistent/periodic L1-RSRP report(s) only, or only L1-SINR report(s).

In case of intra-band carrier aggregation or in inter-band CA band-band combination where simultaneous SRS and PUCCH/PUSCH transmissions are not allowed, a UE is not expected to be configured with SRS from a carrier and PUSCH/UL DM-RS/UL PT-RS/PUCCH formats from a different carrier in the same symbol.

In case of intra-band carrier aggregation or in inter-band CA band-band combination where simultaneous SRS and PRACH transmissions are not allowed, a UE shall not transmit simultaneously SRS resource(s) from a carrier and PRACH from a different carrier.

In case a SRS resource with *resourceType* set as 'aperiodic' is triggered on the OFDM symbol(s) configured with periodic/semi-persistent SRS transmission, the UE shall transmit the aperiodic SRS resource and only the periodic/semi-persistent SRS symbol(s) overlapping within the symbol(s) are dropped, while the periodic/semi-persistent SRS symbol(s) that are not overlapped with the aperiodic SRS resource are transmitted. In case a SRS resource with *resourceType* set as 'semi-persistent' is triggered on the OFDM symbol(s) configured with periodic SRS transmission, the UE shall transmit the semi-persistent SRS resource and only the periodic SRS symbol(s) overlapping within the symbol(s) are dropped, while the periodic SRS symbol(s) that are not overlapped with the semi-persistent SRS resource are transmitted.

When the UE is configured with the higher layer parameter *usage* in *SRS-ResourceSet* set to 'antennaSwitching', and a guard period of Y symbols is configured according to Clause 6.2.1.2, the UE shall use the same priority rules as defined above during the guard period as if SRS was configured.

When a *spatialRelationInfo* is activated/updated for a semi-persistent or aperiodic SRS resource by a MAC CE for a set of CCs/BWPs, where the applicable list of CCs is indicated by higher layer parameter [*applicableCellList*], the *spatialRelationInfo* is applied for the semi-persistent or aperiodic SRS resource(s) with the same SRS resource ID for all the BWPs in the indicated CCs.

When the higher layer parameter *enableDefaultBeamPlForSRS* is set ‘enabled’, and if the higher layer parameter *spatialRelationInfo* for the SRS resource, except for the SRS resource with the higher layer parameter *usage* in SRS-ResourceSet set to 'beamManagement' or for the SRS resource with the higher layer parameter *usage* in SRS-ResourceSet set to ‘nonCodebook’ with configuration of *associatedCSI-RS*, is not configured in FR2 and if the UE is not configured with higher layer parameter(s) *pathlossReferenceRS*, the UE shall transmit the target SRS resource

- with the same spatial domain transmission filter used for the reception of the CORESET with the lowest *controlResourceSetId* in the active DL BWP in the CC.

- with the same spatial domain transmission filter used for the reception of the activated TCI state with the lowest ID applicable to PDSCH in the active DL BWP of the CC if the UE is not configured with any CORESET in the CC

#### 6.2.1.1 UE SRS frequency hopping procedure

For a given SRS resource, the UE is configured with repetition factor R∈{1,2,4} by higher layer parameter *resourceMapping* in *SRS-Resource* where *R*≤*Ns*. When frequency hopping within an SRS resource in each slot is not configured (*R=Ns*), each of the antenna ports of the SRS resource in each slot is mapped in all the  symbols to the same set of subcarriers in the same set of PRBs. When frequency hopping within an SRS resource in each slot is configured without repetition (*R=1*), according to the SRS hopping parameters , and defined in Clause 6.4.1.4 of [4, TS 38.211], each of the antenna ports of the SRS resource in each slot is mapped to different sets of subcarriers in each OFDM symbol, where the same transmission comb value is assumed for different sets of subcarriers. When both frequency hopping and repetition within an SRS resource in each slot are configured (*Ns=4, R=2*), each of the antenna ports of the SRS resource in each slot is mapped to the same set of subcarriers within each pair of R adjacent OFDM symbols, and frequency hopping across the two pairs is according to the SRS hopping parameters , and .

A UE may be configured  adjacent symbol aperiodic SRS resource with intra-slot frequency hopping within a bandwidth part, where the full hopping bandwidth is sounded with an equal-size subband across  symbols when frequency hopping is configured with *R=1*. A UE may be configured  adjacent symbols aperiodic SRS resource with intra-slot frequency hopping within a bandwidth part, where the full hopping bandwidth is sounded with an equal-size subband across two pairs of *R* adjacent OFDM symbols, when frequency hopping is configured with *R=2*. Each of the antenna ports of the SRS resource is mapped to the same set of subcarriers within each pair of R adjacent OFDM symbols of the resource.

A UE may be configured symbol periodic or semi-persistent SRS resource with inter-slot hopping within a bandwidth part, where the SRS resource occupies the same symbol location in each slot. A UE may be configured symbol periodic or semi-persistent SRS resource with intra-slot and inter-slot hopping within a bandwidth part, where the N-symbol SRS resource occupies the same symbol location(s) in each slot. For *Ns=4*, when frequency hopping is configured with *R=2*, intra-slot and inter-slot hopping is supported with each of the antenna ports of the SRS resource mapped to different sets of subcarriers across two pairs of *R* adjacent OFDM symbol(s) of the resource in each slot. Each of the antenna ports of the SRS resource is mapped to the same set of subcarriers within each pair of *R* adjacent OFDM symbols of the resource in each slot. For *Ns= R*, when frequency hopping is configured, inter-slot frequency hopping is supported with each of the antenna ports of the SRS resource mapped to the same set of subcarriers in *R* adjacent OFDM symbol(s) of the resource in each slot.

#### 6.2.1.2 UE sounding procedure for DL CSI acquisition

When the UE is configured with the higher layer parameter *usage* in *SRS-ResourceSet* set as 'antennaSwitching', the UE may be configured with only one of the following configurations depending on the indicated UE capability *supportedSRS-TxPortSwitch* ('t1r2' for 1T2R, 't1r1-t1r2' for 1T=1R/1T2R, 't2r4' for 2T4R, 't1r4' for 1T4R, 't1r1-t1r2-t1r4' for 1T=1R/1T2R/1T4R, 't1r4-t2r4' for 1T4R/2T4R, 't1r1-t1r2-t2r2-t2r4' for 1T=1R/1T2R/2T=2R/2T4R, 't1r1-t1r2-t2r2-t1r4-t2r4' for 1T=1R/1T2R/2T=2R/1T4R/2T4R, 't1r1' for 1T=1R, 't2r2' for 2T=2R, 't1r1-t2r2' for 1T=1R/2T=2R, 't4r4' for 4T=4R, or 't1r1-t2r2-t4r4' for 1T=1R/2T=2R/4T=4R):

- For 1T2R, up to two SRS resource sets configured with a different value for the higher layer parameter *resourceType* in *SRS-ResourceSet* set, where each set has two SRS resources transmitted in different symbols, each SRS resource in a given set consisting of a single SRS port, and the SRS port of the second resource in the set is associated with a different UE antenna port than the SRS port of the first resource in the same set, or

- For 2T4R, up to two SRS resource sets configured with a different value for the higher layer parameter *resourceType* in *SRS-ResourceSet* set, where each SRS resource set has two SRS resources transmitted in different symbols, each SRS resource in a given set consisting of two SRS ports, and the SRS port pair of the second resource is associated with a different UE antenna port pair than the SRS port pair of the first resource, or

- For 1T4R, zero or one SRS resource set configured with higher layer parameter *resourceType* in *SRS-ResourceSet* set to 'periodic' or 'semi-persistent' with four SRS resources transmitted in different symbols, each SRS resource in a given set consisting of a single SRS port, and the SRS port of each resource is associated with a different UE antenna port, and

- For 1T4R, zero or two SRS resource sets each configured with higher layer parameter *resourceType* in *SRS-ResourceSet* set to 'aperiodic' and with a total of four SRS resources transmitted in different symbols of two different slots, and where the SRS port of each SRS resource in the given two sets is associated with a different UE antenna port. The two sets are each configured with two SRS resources, or one set is configured with one SRS resource and the other set is configured with three SRS resources. The UE shall expect that the two sets are both configured with the same values of the higher layer parameters *alpha*, *p0*, *pathlossReferenceRS*, and *srs-PowerControlAdjustmentStates* in *SRS-ResourceSet*. The UE shall expect that the value of the higher layer parameter *aperiodicSRS-ResourceTrigger* or the value of an entry in *AperiodicSRS-ResourceTriggerList* in each *SRS-ResourceSet* is the same, and the value of the higher layer parameter *slotOffset* in each *SRS-ResourceSet* is different. Or,

- For 1T=1R, or 2T=2R, or 4T=4R, up to two SRS resource sets each with one SRS resource, where the number of SRS ports for each resource is equal to 1, 2, or 4.

The UE is configured with a guard period of Y symbols, in which the UE does not transmit any other signal, in the case the SRS resources of a set are transmitted in the same slot. The guard period is in-between the SRS resources of the set.

The UE shall expect to be configured with the same number of SRS ports for all SRS resources in the SRS resource set(s) with higher layer parameter *usage* set as 'antennaSwitching'.

For 1T2R, 1T4R or 2T4R, the UE shall not expect to be configured or triggered with more than one SRS resource set with higher layer parameter *usage* set as 'antennaSwitching' in the same slot. For 1T=1R, 2T=2R or 4T=4R, the UE shall not expect to be configured or triggered with more than one SRS resource set with higher layer parameter *usage* set as 'antennaSwitching' in the same symbol.

The value of *Y* is defined by Table 6.2.1.2-1.

Table 6.2.1.2-1: The minimum guard period between two SRS resources of an SRS resource set for antenna switching

|  |  |  |
| --- | --- | --- |
|  |  | *Y* [symbol] |
| 0 | 15 | 1 |
| 1 | 30 | 1 |
| 2 | 60 | 1 |
| 3 | 120 | 2 |

#### 6.2.1.3 UE sounding procedure between component carriers

For a carrier of a serving cell with slot formats comprised of DL and UL symbols, not configured for PUSCH/PUCCH transmission, the UE shall not transmit SRS whenever SRS transmission (including any interruption due to uplink or downlink RF retuning time [11, TS 38.133] as defined by higher layer parameters *switchingTimeUL* and *switchingTimeDL* of *srs-SwitchingTimeNR)* on the carrier of the serving cell and PUSCH/PUCCH transmission carrying HARQ-ACK/positive SR/RI/CRI and/or PRACH happen to overlap in the same symbol and that can result in uplink transmissions beyond the UE's indicated uplink carrier aggregation capability included in [13, TS 38.306].

For a carrier of a serving cell with slot formats comprised of DL and UL symbols, not configured for PUSCH/PUCCH transmission, the UE shall not transmit a periodic/semi-persistent SRS whenever periodic/semi-persistent SRS transmission (including any interruption due to uplink or downlink RF retuning time [11, TS 38.133] as defined by higher layer parameters *switchingTimeUL* and *switchingTimeDL* of *srs-SwitchingTimeNR)* on the carrier of the serving cell and PUSCH transmission carrying aperiodic CSI happen to overlap in the same symbol and that can result in uplink transmissions beyond the UE's indicated uplink carrier aggregation capability included in [13, TS 38.306].

For a carrier of a serving cell with slot formats comprised of DL and UL symbols, not configured for PUSCH/PUCCH transmission, the UE shall drop PUCCH/PUSCH transmission carrying periodic CSI comprising only CQI/PMI, and/or SRS transmission on another serving cell configured for PUSCH/PUCCH transmission whenever the transmission and SRS transmission (including any interruption due to uplink or downlink RF retuning time [11, TS 38.133] as defined by higher layer parameters *switchingTimeUL* and *switchingTimeDL* of *srs-SwitchingTimeNR)* on the serving cell happen to overlap in the same symbol and that can result in uplink transmissions beyond the UE's indicated uplink carrier aggregation capability included in [13, TS 38.306].

For a carrier of a serving cell with slot formats comprised of DL and UL symbols, not configured for PUSCH/PUCCH transmission, the UE shall drop PUSCH transmission carrying aperiodic CSI comprising only CQI/PMI whenever the transmission and aperiodic SRS transmission (including any interruption due to uplink or downlink RF retuning time [11, TS 38.133]) as defined by higher layer parameters *switchingTimeUL* and *switchingTimeDL* of *srs-SwitchingTimeNR)* on the carrier of the serving cell happen to overlap in the same symbol and that can result in uplink transmissions beyond the UE's indicated uplink carrier aggregation capability included in [13, TS 38.306].

For an aperiodic SRS triggered in DCI format 2\_3 and if the UE is configured with higher layer parameter *srs-TPC-PDCCH-Group* set to 'typeA', and given by *SRS-CarrierSwitching,* without PUSCH/PUCCH transmission, the order of the triggered SRS transmission on the serving cells follow the order of the serving cells in the indicated set of serving cells configured by higher layers, where the UE in each serving cell transmits the configured one or two SRS resource set(s) with higher layer parameter *usage* set to 'antennaSwitching' and higher layer parameter *resourceType* in *SRS-ResourceSet* set to 'aperiodic'.

For an aperiodic SRS triggered in DCI format 2\_3 and if the UE is configured with higher layer parameter *srs-TPC-PDCCH-Group* set to 'typeB' without PUSCH/PUCCH transmission, the order of the triggered SRS transmission on the serving cells follow the order of the serving cells with aperiodic SRS triggered in the DCI, and the UE in each serving cell transmits the configured one or two SRS resource set(s) with higher layer parameter *usage* set to 'antennaSwitching' and higher layer parameter *resourceType* in *SRS-ResourceSet* set to 'aperiodic'.

A UE can be configured with SRS resource(s) on a carrier *c1* with slot formats comprised of DL and UL symbols and not configured for PUSCH/PUCCH transmission. For carrier *c1*, the UE is configured with higher layer parameter *srs-SwitchFromServCellIndex* and *srs-SwitchFromCarrier* the switching from carrier *c2* which is configured for PUSCH/PUCCH transmission. During SRS transmission on carrier *c1* (including any interruption due to uplink or downlink RF retuning time [11, TS 38.133] as defined by higher layer parameters *switchingTimeUL* and *switchingTimeDL* of *srs-SwitchingTimeNR*), the UE temporarily suspends the uplink transmission on carrier *c2*.

If the UE is not configured for PUSCH/PUCCH transmission on carrier *c1* with slot formats comprised of DL and UL symbols, and if the UE is not capable of simultaneous reception and transmission on carrier *c1*and serving cell *c2*, the UE is not expected to be configured or indicated with SRS resource(s) such that SRS transmission on carrier *c1* (including any interruption due to uplink or downlink RF retuning time [11, TS 38.133] as defined by higher layer parameters *switchingTimeUL* and *switchingTimeDL* of *srs-SwitchingTimeNR*) would collide with the REs corresponding to the SS/PBCH blocks configured for the UE or the slots belonging to a control resource set indicated by *MIB* or *SIB1* on serving cell *c2*.

For *n*-th (*n ≥* 1) aperiodic SRS transmission on a cell *c*, upon detection of a positive SRS request on a grant, the UE shall commence this SRS transmission on the configured symbol and slot provided

- it is no earlier than the summation of

- the maximum time duration between the two durations spanned by N OFDM symbols of the numerology of cell *c* and the cell carrying the grant respectively, and

- the UL or DL RF retuning time [11, TS 38.133] as defined by higher layer parameters *switchingTimeUL* and *switchingTimeDL* of *srs-SwitchingTimeNR,*

- it does not collide with any previous SRS transmissions, or interruption due to UL or DL RF retuning time.

otherwise, *n*-th SRS transmission is dropped, where N is the reported capability as the minimum time interval in unit of symbols, between the DCI triggering and aperiodic SRS transmission.

In case of inter-band carrier aggregation, a UE can simultaneously transmit SRS and PUCCH/PUSCH across component carriers in different bands subject to the UE's capability.

In case of inter-band carrier aggregation, a UE can simultaneously transmit PRACH and SRS across component carriers in different bands subject to UE's capability.

#### 6.2.1.4 UE sounding procedure for positioning purposes

When the SRS is configured by the higher layer parameter [SRS-for-positioning] and if the higher layer parameter *spatialRelationInfo* is configured*,* it contains the ID of the configuration fields of a reference RS according to Clause 6.3.2 of [TS 38.331]. The reference RS can be an SRS configured by the higher layer parameter *SRS-Config* or [SRS-for-positioning], CSI-RS, SS/PBCH block, or a DL PRS configured on a serving cell or a SS/PBCH block or a DL PRS configured on a non-serving cell.

The UE is not expected to transmit multiple SRS resources with different spatial relations in the same OFDM symbol.

If the UE is not configured with the higher layer parameter *spatialRelationInfo* the UE may use a fixed spatial domain transmission filter for transmissions of the SRS configured by the higher layer parameter [SRS-for-positioning] across multiple SRS resources or it may use a different spatial domain transmission filter across multiple SRS resources.

The UE is only expected to transmit an SRS configured the by the higher layer parameter [SRS-for-positioning] within the active UL BWP of the UE.

When the configuration of SRS is done by the higher layer parameter [SRS-for-positioning], the UE can only be provided with a single RS source in *spatialRelationInfo* per SRS resource.

If an SRS configured by the higher parameter [SRS-for-positioning] collides with a scheduled PUSCH, the SRS is dropped in the symbols where the collision occurs.

### 6.2.2 UE DM-RS transmission procedure

When transmitted PUSCH is neither scheduled by DCI format 0\_1 with CRC scrambled by C-RNTI, CS-RNTI, SP-CSI-RNTI or MCS-C-RNTI, nor corresponding to a configured grant, nor being a PUSCH for Type-2 random access procedure. the UE shall use single symbol front-loaded DM-RS of configuration type 1 on DM-RS port 0 and the remaining REs not used for DM-RS in the symbols are not used for any PUSCH transmission except for PUSCH with allocation duration of 2 or less OFDM symbols with transform precoding disabled, additional DM-RS can be transmitted according to the scheduling type and the PUSCH duration as specified in Table 6.4.1.1.3-3 of [4, TS38.211] for frequency hopping disabled and as specified in Table 6.4.1.1.3-6 of [4, TS38.211] for frequency hopping enabled, and

If frequency hopping is disabled:

- The UE shall assume *dmrs-AdditionalPosition* equals to 'pos2' and up to two additional DM-RS can be transmitted according to PUSCH duration, or

If frequency hopping is enabled:

- The UE shall assume *dmrs-AdditionalPosition* equals to 'pos1' and up to one additional DM-RS can be transmitted according to PUSCH duration.

When transmitted PUSCH is scheduled by activation DCI format 0\_0 with CRC scrambled by CS-RNTI, the UE shall use single symbol front-loaded DM-RS of configuration type provided by higher layer parameter *dmrs-Type* in *configuredGrantConfig* on DM-RS port 0 and the remaining REs not used for DM-RS in the symbols are not used for any PUSCH transmission except for PUSCH with allocation duration of 2 or less OFDM symbols with transform precoding disabled, and additional DM-RS with *dmrs-AdditionalPosition* from *configuredGrantConfig* can be transmitted according to the scheduling type and the PUSCH duration as specified in Table 6.4.1.1.3-3 of [4, TS38.211] for frequency hopping disabled and as specified in Table 6.4.1.1.3-6 of [4, TS38.211] for frequency hopping enabled.

For the UE-specific reference signals generation as defined in Clause 6.4.1.1 of [4, TS 38.211], a UE can be configured by higher layers with one or two scrambling identity(s), *i* = 0,1 which are the same for both PUSCH mapping Type A and Type B.

When transmitted PUSCH is scheduled by DCI format 0\_1 with CRC scrambled by C-RNTI, CS-RNTI, SP-CSI-RNTI or MCS-C-RNTI, or corresponding to a configured grant, or being a PUSCH for Type-2 random access procedure,

- the UE may be configured with higher layer parameter *dmrs-Type* in *DMRS-UplinkConfig*, and the configured DM-RS configuration type is used for transmitting PUSCH in as defined in Clause 6.4.1.1 of [4, TS 38.211]. For MsgA PUSCH transmissions, *dmrs-Type* is type 1.

- the UE may be configured with the maximum number of front-loaded DM-RS symbols for PUSCH by higher layer parameter *maxLength* in *DMRS-UplinkConfig,* or by higher layer parameter *msgA-MaxLength* in *msgA-DMRS-Configuration*,*.*

- if *maxLength* is not configured, single-symbol DM-RS can be scheduled for the UE by DCI or configured by the configured grant configuration, and the UE can be configured with a number of additional DM-RS for PUSCH by higher layer parameter *dmrs-AdditionalPosition,* which can be 'pos0', 'pos1', 'pos2', 'pos3'.

- if *MsgA-maxLength* is not configured, single-symbol DM-RS can be scheduled for the UE by DCI or configured by the configured grant configuration, and the UE can be configured with a number of additional DM-RS for PUSCH for Type-2 random access procedure by higher layer parameter by *msgA-DMRS-Configuration*, which can be 'pos0', 'pos1', 'pos2', 'pos3'.

- if *maxLength* or MsgA*maxLength* is configured, either single-symbol DM-RS or double symbol DM-RS can be scheduled for the UE by DCI or configured by the configured grant configuration, and the UE can be configured with a number of additional DM-RS for PUSCH by higher layer parameter *dmrs-AdditionalPosition,* which can be 'pos0' or 'pos1'. For PUSCH for Type-2 random access procedure the UE can be configured with a number of additional DM-RS for PUSCH by higher layer parameter *msgA-dmrs-AdditionalPosition,* which can be 'pos0', 'pos1', 'pos2', 'pos3'.

- and, the UE shall transmit a number of additional DM-RS as specified in Table 6.4.1.1.3-3 and Table 6.4.1.1.3-4 in -Clause 6.4.1.1.3 of [4, TS 38.211].

If a UE transmitting PUSCH is configured with the higher layer parameter *phaseTrackingRS* in *DMRS-UplinkConfig*, the UE may assume that the following configurations are not occurring simultaneously for the transmitted PUSCH

- any DM-RS ports among 4-7 or 6-11 for DM-RS configurations type 1 and type 2, respectively are scheduled for the UE and PT-RS is transmitted from the UE.

For PUSCH scheduled by DCI format 0\_1, by activation DCI format 0\_1 with CRC scrambled by CS-RNTI, or configured by configured grant Type 1 configuration, the UE shall assume the DM-RS CDM groups indicated in Tables 7.3.1.1.2-6 to 7.3.1.1.2-23 of Clause 7.3.1.1 of [5, TS38.212] are not used for data transmission, where "1", "2" and "3" for the number of DM-RS CDM group(s) correspond to CDM group 0, {0,1}, {0,1,2}, respectively.

For PUSCH scheduled by DCI format 0\_0 or by activation DCI format 0\_0 with CRC scrambled by CS-RNTI, the UE shall assume the number of DM-RS CDM groups without data is 1 which corresponds to CDM group 0 for the case of PUSCH with allocation duration of 2 or less OFDM symbols with transform precoding disabled, the UE shall assume that the number of DM-RS CDM groups without data is 3 which corresponds to CDM group {0,1,2} for the case of PUSCH scheduled by activation DCI format 0\_0 and the *dmrs-Type* in *cg-DMRS-Configuration* equal to 'type2' and the PUSCH allocation duration being more than 2 OFDM symbols, and the UE shall assume that the number of DM-RS CDM groups without data is 2 which corresponds to CDM group {0,1} for all other cases.

For MsgA PUSCH transmission, if the UE is not configured with *msgAPUSCHDMRSCDMgroup,* the UEshall assume that 2 DM-RS CDM groups are configured. Otherwise, *msgAPUSCHDMRSCDMgroup* indicates which DM-RS CDM group to use from the set of {0,1}.

For MsgA PUSCH transmission, if the UE is not configured with *msgAPUSCHNrOfPort,* the UEshall assume that 4 ports are configured per DM-RS CDM groups. Otherwise, *msgAPUSCHNrOfPort* with value of 0 indicates one port per DM-RS CDM group, while a value of 1 indicated two ports per DM-RS CDM group.

For uplink DM-RS with PUSCH, the UE may assume the ratio of PUSCH EPRE to DM-RS EPRE ( [dB]) is given by Table 6.2.2-1 according to the number of DM-RS CDM groups without data. The DM-RS scaling factor  specified in clause 6.4.1.1.3 of [4, TS 38.211] is given by .

Table 6.2.2-1: The ratio of PUSCH EPRE to DM-RS EPRE

|  |  |  |
| --- | --- | --- |
| Number of DM-RS CDM groups without data | DM-RS configuration type 1 | DM-RS configuration type 2 |
| 1 | 0 dB | 0 dB |
| 2 | -3 dB | -3 dB |
| 3 | - | -4.77 dB |

For PUSCH repetition Type B, the DM-RS transmission procedure is applied for each actual repetition separately based on the allocation duration of the actual repetition.

### 6.2.3 UE PT-RS transmission procedure

If a UE is not configured with the higher layer parameter *phaseTrackingRS* in *DMRS-UplinkConfig*, the UE shall not transmit PT-RS. ThePTRS is only present on PUSCH scheduled by PDCCH with CRC scrambled by MCS-C-RNTI, C-RNTI, CS-RNTI, SP-CSI-RNTI and on PUSCH corresponding to a configured grant. For PUSCH repetition Type B, the PT-RS transmission procedure is applied for each actual repetition separately based on the allocation duration of the actual repetition.

#### 6.2.3.1 UE PT-RS transmission procedure when transform precoding is not enabled

When transform precoding is not enabled and if a UE is configured with the higher layer parameter *phaseTrackingRS* in *DMRS-UplinkConfig,*

- the higher layer parameters *timeDensity* and *frequencyDensity* in *PTRS-UplinkConfig* indicate the threshold values *ptrs-MCSi*, *i*=1,2,3 and *NRB,i* , *i*=0,1, as shown in Table 6.2.3.1-1 and Table 6.2.3.1-2, respectively.

- if either or both higher layer parameters *timeDensity* and/or *frequencyDensity* in *PTRS-UplinkConfig* are configured, the UE shall assume the PT-RS antenna ports' presence and pattern are a function of the corresponding scheduled MCS and scheduled bandwidth in a corresponding bandwidth part as shown in Table 6.2.3.1-1 and Table 6.2.3.1-2, respectively,

- if the higher layer parameter *timeDensity* is not configured, the UE shall assume *LPT-RS* = 1.

- if the higher layer parameter *frequencyDensity* is not configured, the UE shall assume *KPT-RS* = 2.

- if none of the higher layer parameters *timeDensity* and *frequencyDensity* in *PTRS-UplinkConfig* are configured, the UE shall assume *LPT-RS* = 1 and *KPT-RS* = 2.

Table 6.2.3.1-1: Time density of PT-RS as a function of scheduled MCS

|  |  |
| --- | --- |
| Scheduled MCS | Time density() |
| IMCS < ptrs-MCS1 | PT-RS is not present |
| ptrs-MCS1  IMCS < ptrs-MCS2 | 4 |
| ptrs-MCS2  IMCS < ptrs-MCS3 | 2 |
| ptrs-MCS3  IMCS < ptrs-MCS4 | 1 |

Table 6.2.3.1-2: Frequency density of PT-RS as a function of scheduled bandwidth

|  |  |
| --- | --- |
| Scheduled bandwidth | Frequency density () |
| NRB < NRB0 | PT-RS is not present |
| NRB0  NRB < NRB1 | 2 |
| NRB1  NRB | 4 |

The higher layer parameter *PTRS-UplinkConfig* provides the parameters *ptrs-MCSi*, *i*=1,2,3 andwith values in 0-29 when MCS Table 5.1.3.1-1 is used and 0-28 when MCS Table 5.1.3.1-2 is used, respectively. *ptrs-MCS4* is not explicitly configured by higher layers but assumed 29 when MCS Table 5.1.3.1-1 is used and 28 when MCS Table 5.1.3.1-2 is used. The higher layer parameter *PTRS-UplinkConfig* provides the parameters *NRBi**i*=0,1with values in range 1-276.

If the higher layer parameter *PTRS-UplinkConfig* indicates that the time density thresholds *ptrs-MCSi* = *ptrs-MCSi+1*, then the time density *LPTRS* of the associated row where both these thresholds appear in Table 6.2.3.1-1 is disabled. If the higher layer parameter *frequencyDensity* in *PTRS-UplinkConfig* indicates that the frequency density thresholds *NRB,i* = *NRB,i+1*, then the frequency density *KPTRS* of the associated row where both these thresholds appear in Table 6.2.3.1-2 is disabled.

If either or both of the parameters PT-RS time density (*LPT-RS*) and PT-RS frequency density (*KPT-RS*), shown in Table 6.2.3.1-1 and Table 6.2.3.1-2, indicates that are configured as 'PT-RS not present', the UE shall assume that PT-RS is not present.

When a UE is scheduled to transmit PUSCH with allocation duration of 2 symbols or less, and if *LPT-RS* is set to 2 or 4, the UE shall not transmit PT-RS. When a UE is scheduled to transmit PUSCH with allocation duration of 4 symbols or less, and if *LPT-RS* is set to 4, the UE shall not transmit PT-RS.

When a UE is scheduled to transmit PUSCH for retransmission, if the UE is scheduled with *IMCS* > *V*, where *V* = 28 for MCS table 1 and *V* = 27 for MCS table 2, respectively, the MCS for PT-RS time-density determination is obtained from the DCI for the same transport block in the initial transmission, which is smaller than or equal to V.

The maximum number of configured PT-RS ports is given by the higher layer parameter *maxNrofPorts* in *PTRS-UplinkConfig.* The UE is not expected to be configured with a larger number of UL PT-RS ports than it has reported need for.

If a UE has reported the capability of supporting full-coherent UL transmission, the UE shall expect the number of UL PT-RS ports to be configured as one if UL-PTRS is configured.

For codebook or non-codebook based UL transmission, the association between UL PT-RS port(s) and DM-RS port(s) is signalled by *PTRS-DMRS association* field in DCI format 0\_1. For a PUSCH corresponding to a configured grant Type 1 transmission, the UE may assume the association between UL PT-RS port(s) and DM-RS port(s) defined by value 0 in Table 7.3.1.1.2-25 or value "00" in Table 7.3.1.1.1.2-26 described in Clause 7.3.1 of [5, TS38.212].

For PUSCH scheduled by DCI format 0\_0 or by activation DCI format 0\_0, the UL PT-RS port is associated to DM-RS port 0.

For non-codebook based UL transmission, the actual number of UL PT-RS port(s) to transmit is determined based on SRI(s) in DCI format 0\_1 or higher layer parameter *sri-ResourceIndicator* in *rrc-ConfiguredUplinkGrant*. A UE is configured with the PT-RS port index for each configured SRS resource by the higher layer parameter *ptrs-PortIndex* configured by *SRS-Config* if the UE is configured with the higher layer parameter *phaseTrackingRS in DMRS-UplinkConfig*. If the PT-RS port index associated with different SRIs are the same, the corresponding UL DM-RS ports are associated to the one UL PT-RS port.

For partial-coherent and non-coherent codebook based UL transmission, the actual number of UL PT-RS port(s) is determined based on TPMI and/or number of layers which are indicated by *Precoding information and number of layers* field in DCI format 0\_1 or configured by higher layer parameter *precodingAndNnumberOfLayers*:

- if the UE is configured with the higher layer parameter *maxNrofPorts* in *PTRS-UplinkConfig* set to 'n2', the actual UL PT-RS port(s) and the associated transmission layer(s) are derived from indicated TPMI as:

- PUSCH antenna port 1000 and 1002 in indicated TPMI share PT-RS port 0, and PUSCH antenna port 1001 and 1003 in indicated TPMI share PT-RS port 1.

- UL PT-RS port 0 is associated with the UL layer [x] of layers which are transmitted with PUSCH antenna port 1000 and PUSCH antenna port 1002 in indicated TPMI, and UL PT-RS port 1 is associated with the UL layer [y] of layers which are transmitted with PUSCH antenna port 1001 and PUSCH antenna port 1003 in indicated TPMI, where [x] and/or [y] are given by DCI parameter *PTRS-DMRS association* as shown in DCI format 0\_1 described in Clause 7.3.1 of [5, TS38.212].

When the UE is scheduled with *Qp*={1,2} PT-RS port(s) in uplink and the number of scheduled layers is ,

- If the UE is configured with higher layer parameter *ptrs-Power*, the PUSCH to PT-RS power ratio per layer per RE  is given by , where  is shown in the Table 6.2.3.1-3 according to the higher layer parameter *ptrs-Power*, the PT-RS scaling factor  specified in clause 6.4.1.2.2.1 of [4, TS 38.211] is given by and also on the *Precoding Information and Number of Layers* field in DCI.

- The UE shall assume *ptrs-Power* in *PTRS-UplinkConfig* is set to state "00" in Table 6.2.3.1-3 if not configured or in case of non-codebook based PUSCH.

Table 6.2.3.1-3: Factor related to PUSCH to PT-RS power ratio per layer per RE 

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *UL-PTRS-power /* |  | The number of PUSCH layers ( ) | | | | | | |
| 1 | 2 | | 3 | | 4 | | |
| All cases | Full coherent | Partial and non- coherent and non-codebook based | Full coherent | Partial and non- coherent and non-codebook based | Full coherent | Partial coherent | Non-coherent and non-codebook based |
| 00 | 0 | 3 | 3*Qp*-3 | 4.77 | 3*Qp*-3 | 6 | 3*Qp* | 3*Qp*-3 |
| 01 | 0 | 3 | 3 | 4.77 | 4.77 | 6 | 6 | 6 |
| 10 | Reserved | | | | | | | |
| 11 | Reserved | | | | | | | |

#### 6.2.3.2 UE PT-RS transmission procedure when transform precoding is enabled

When transform precoding is enabled and if a UE is configured with the higher layer parameter *transformPrecoderEnabled* in *PTRS-UplinkConfig,*

- the UE shall be configured with the higher layer parameters *sampleDensity* and the UE shall assume the PT-RS antenna ports' presence and PT-RS group pattern are a function of the corresponding scheduled bandwidth in a corresponding bandwidth part, as shown in Table 6.2.3.2-1. The UE shall assume no PT-RS is present when the number of scheduled RBs is less than NRB0 if NRB0 > 1 or if the RNTI equals TC-RNTI.

- and the UE may be configured PT-RS time density *LPT-RS* = 2 with the higher layer parameter *timeDensityTransformPrecoding.* Otherwise, the UE shall assume *LPT-RS* = 1.

- if the higher layer parameter *sampleDensity* indicates that the sample density thresholds *NRB,i* = *NRB,i+1*, then the associated row where both these thresholds appear in Table 6.2.3.2-1 is disabled.

Table 6.2.3.2-1: PT-RS group pattern as a function of scheduled bandwidth

|  |  |  |
| --- | --- | --- |
| Scheduled bandwidth | Number of PT-RS groups | Number of samples  per PT-RS group |
| *NRB0* *NRB* < *NRB1* | 2 | 2 |
| *NRB1*  *NRB* < *NRB2* | 2 | 4 |
| *NRB2*  *NRB* < *NRB3* | 4 | 2 |
| *NRB3*  *NRB* < *NRB4* | 4 | 4 |
| *NRB4*  *NRB* | 8 | 4 |

When transform precoding is enabled and if a UE is configured with the higher layer parameter *transformPrecoderEnabled* in *PTRS-UplinkConfig,* the PT-RS scaling factor *β*' specified in Clause 6.4.1.2.2.2 of [4, TS 38.211] is determined by the scheduled modulation order as shown in table 6.2.3.2-2.

Table 6.2.3.2-2: PT-RS scaling factor (*β*') when transform precoding enabled.

|  |  |
| --- | --- |
| Scheduled modulation | PT-RS scaling factor (*β*') |
| π/2-BPSK | 1 |
| QPSK | 1 |
| 16QAM |  |
| 64QAM |  |
| 256QAM |  |

## 6.3 UE PUSCH frequency hopping procedure

### 6.3.1 Frequency hopping for PUSCH repetition Type A

For PUSCH repetition Type A (as determined according to procedures defined in Clause 6.1.2.1 for scheduled PUSCH, or Clause 6.1.2.3 for configured PUSCH), a UE is configured for frequency hopping by the higher layer parameter *frequencyHopping-ForDCIFormat0\_2* in *pusch-Config* for PUSCH transmission scheduled by DCI format 0\_2, and by *frequencyHopping* provided in *pusch-Config* for PUSCH transmission scheduled by a DCI format other than 0\_2*,* and by *frequencyHopping* provided in *configuredGrantConfig* for configured PUSCH transmission. One of two frequency hopping modes can be configured:

- Intra-slot frequency hopping, applicable to single slot and multi-slot PUSCH transmission.

- Inter-slot frequency hopping, applicable to multi-slot PUSCH transmission.

In case of resource allocation type 2, the UE transmits PUSCH without frequency hopping.

In case of resource allocation type 1, whether or not transform precoding is enabled for PUSCH transmission, the UE may perform PUSCH frequency hopping, if the frequency hopping field in a corresponding detected DCI format or in a random access response UL grant is set to 1, or if for a Type 1 PUSCH transmission with a configured grant the higher layer parameter *frequencyHoppingOffset* is provided, otherwise no PUSCH frequency hopping is performed. When frequency hopping is enabled for PUSCH, the RE mapping is defined in clause 6.3.1.6 of [4, TS 38.211].

For a PUSCH scheduled by RAR UL grant, fallbackRAR UL grant, or by DCI format 0\_0 with CRC scrambled by TC-RNTI, frequency offsets are obtained as described in clause 8.3 of [6, TS 38.213]. For a PUSCH scheduled by DCI format 0\_0/0\_1 or a PUSCH based on a Type2 configured UL grant activated by DCI format 0\_0/0\_1 and for resource allocation type 1, frequency offsets are configured by higher layer parameter *frequencyHoppingOffsetLists* in *pusch-Config*. For a PUSCH scheduled by DCI format 0\_2 or a PUSCH based on a Type2 configured UL grant activated by DCI format 0\_2 and for resource allocation type 1, frequency offsets are configured by higher layer parameter *frequencyHoppingOffsetLists-ForDCIFormat0\_2* in *pusch-Config*.

- When the size of the active BWP is less than 50 PRBs, one of two higher layer configured offsets is indicated in the UL grant.

- When the size of the active BWP is equal to or greater than 50 PRBs, one of four higher layer configured offsets is indicated in the UL grant.

For PUSCH based on a Type1 configured UL grant the frequency offset is provided by the higher layer parameter *frequencyHoppingOffset* in *rrc-ConfiguredUplinkGrant*.

For a MsgA PUSCH the frequency offset is provided by the higher layer parameter as described in [6, TS 38.213.

In case of intra-slot frequency hopping, the starting RB in each hop is given by:

,

where *i*=0 and *i*=1 are the first hop and the second hop respectively, and  is the starting RB within the UL BWP, as calculated from the resource block assignment information of resource allocation type 1 (described in Clause 6.1.2.2.2) and is the frequency offset in RBs between the two frequency hops. The number of symbols in the first hop is given by , the number of symbols in the second hop is given by , where is the length of the PUSCH transmission in OFDM symbols in one slot.

In case of inter-slot frequency hopping, the starting RB during slot  is given by:

,

where  is the current slot number within a radio frame, where a multi-slot PUSCH transmission can take place,  is the starting RB within the UL BWP, as calculated from the resource block assignment information of resource allocation type 1 (described in Clause 6.1.2.2.2) and is the frequency offset in RBs between the two frequency hops.

### 6.3.2 Frequency hopping for PUSCH repetition Type B

For PUSCH repetition Type B (as determined according to procedures defined in Clause 6.1.2.1 for scheduled PUSCH, or Clause 6.1.2.3 for configured PUSCH), a UE is configured for frequency hopping by the higher layer parameter *frequencyHopping-ForDCIFormat0\_2* in *pusch-Config* for PUSCH transmission scheduled by DCI format 0\_2, by *frequencyHopping-ForDCIFormat0\_1* provided in *pusch-Config* for PUSCH transmission scheduled by DCI format 0\_1, and by *frequencyHopping-PUSCHRepTypeB* provided in *configuredGrantConfig* for [Type 1] configured PUSCH transmission. [The frequency hopping mode for Type 2 configured PUSCH transmission follows the activating DCI format]. One of two frequency hopping modes can be configured:

- Inter-repetition frequency hopping

- Inter-slot frequency hopping

In case of resource allocation type 1, whether or not transform precoding is enabled for PUSCH transmission, the UE may perform PUSCH frequency hopping, if the frequency hopping field in a corresponding detected DCI format is set to 1, or if for a Type 1 PUSCH transmission with a configured grant the higher layer parameter *frequencyHopping-PUSCHRepTypeB* is provided, otherwise no PUSCH frequency hopping is performed. When frequency hopping is enabled for PUSCH, the RE mapping is defined in clause 6.3.1.6 of [4, TS 38.211].

For a PUSCH scheduled by DCI format 0\_1 or a PUSCH based on a Type 2 configured UL grant activated by DCI format 0\_1 and for resource allocation type 1, frequency offsets are configured by higher layer parameter *frequencyHoppingOffsetLists* in *pusch-Config*. For a PUSCH scheduled by DCI format 0\_2 or a PUSCH based on a Type 2 configured UL grant activated by DCI format 0\_2 and for resource allocation type 1, frequency offsets are configured by higher layer parameter *frequencyHoppingOffsetLists-ForDCIFormat0\_2* in *pusch-Config*.

- When the size of the active BWP is less than 50 PRBs, one of two higher layer configured offsets is indicated in the UL grant.

- When the size of the active BWP is equal to or greater than 50 PRBs, one of four higher layer configured offsets is indicated in the UL grant.

For PUSCH based on a Type1 configured UL grant the frequency offset is provided by the higher layer parameter *frequencyHoppingOffset* in *rrc-ConfiguredUplinkGrant*.

In case of inter-repetition frequency hopping, [details to be added when agreements become available].

In case of inter-slot frequency hopping, the starting RB during slot  follows that of inter-slot frequency hopping for PUSCH Repetition Type A in Clause 6.3.1.

## 6.4 UE PUSCH preparation procedure time

If the first uplink symbol in the PUSCH allocation for a transport block, including the DM-RS, as defined by the slot offset *K2* and the start and length indicator *SLIV* of the scheduling DCI and including the effect of the timing advance, is no earlier than at symbol *L2*, where *L2* is defined as the next uplink symbol with its CP starting after the end of the reception of the last symbol of the PDCCH carrying the DCI scheduling the PUSCH, then the UE shall transmit the transport block.

*- N2* is based on *µ* of Table 6.4-1 and Table 6.4-2 for UE processing capability 1 and 2 respectively, where *µ* corresponds to the one of (*µDL*, *µUL*) resulting with the largest *Tproc,2*, where the *µDL* corresponds to the subcarrier spacing of the downlink with which the PDCCH carrying the DCI scheduling the PUSCH was transmitted and *µUL* corresponds to the subcarrier spacing of the uplink channel with which the PUSCH is to be transmitted, and *κ* is defined in clause 4.1 of [4, TS 38.211].

- If the first symbol of the PUSCH allocation consists of DM-RS only, then *d2,1* = 0*,* otherwise *d2,1* = 1.

- If the UE is configured with multiple active component carriers, the first uplink symbol in the PUSCH allocation further includes the effect of timing difference between component carriers as given in [11, TS 38.133].

- If the scheduling DCI triggered a switch of BWP, *d2,2* equals to the switching time as defined in [11, TS 38.133], otherwise *d2,2*=0.

- For a UE that supports capability 2 on a given cell, the processing time according to UE processing capability 2 is applied if the high layer parameter *processingType2Enabled* in *PUSCH-ServingCellConfig* is configured for the cell and set to *enable*,

- If the PUSCH indicated by the DCI is overlapping with one or more PUCCH channels, then the transport block is multiplexed following the procedure in clause 9.2.5 of [6, TS 38.213], otherwise the transport block is transmitted on the PUSCH indicated by the DCI.

Otherwise the UE may ignore the scheduling DCI.

The value of  is used both in the case of normal and extended cyclic prefix.

Table 6.4-1: PUSCH preparation time for PUSCH timing capability 1

|  |  |
| --- | --- |
|  | PUSCH preparation time *N2* [symbols] |
| 0 | 10 |
| 1 | 12 |
| 2 | 23 |
| 3 | 36 |

Table 6.4-2: PUSCH preparation time for PUSCH timing capability 2

|  |  |
| --- | --- |
|  | PUSCH preparation time *N2* [symbols] |
| 0 | 5 |
| 1 | 5.5 |
| 2 | 11 for frequency range 1 |

# 7 UE procedures for transmitting and receiving on a carrier with intra-cell guard bands

For operation with shared spectrum channel access, when the UE is configured with any of *intraCellGuardBandUL-r16* for UL carrier and *intraCellGuardBandDL-r16* for DL carrier, the UE is provided with intra-cell guard bands on a carrier, each defined by start and end CRB, and , respectively. The intra-cell guard bands separate RB-sets, each defined by start and end CRB, and , respectively. UE determines , , and the remaining start and end CRBs as and . When the UE is not configured with *intraCellGuardBandUL-r16,* the UE determines intra-cell guard band and corresponding RB-set according to the [default intra-cell GB pattern from 38.101 corresponding to and carrier size ]. When the UE is not configured with *intraCellGuardBandDL-r16,* the UE determines intra-cell guard band and corresponding RB-set according to the [default intra-cell GB pattern from 38.101 corresponding to and carrier size ].

For a carrier with intra-carrier guard bands, the UE does not expect to receive a BWP configuration by *BWP-Downlink* or *BWP-Uplink* partially overlapping with a RB-set. RB-sets within BWP form a set of cardinality .

[The configuration of *intraCellGuardBandDL-r16* and *intraCellGuardBandUL-r16* can indicate to the UE that no intra-cell guard-bands are configured.]

# 8 Physical sidelink shared channel related procedures

A UE can be configured by higher layers with one or more sidelink resource pools. A sidelink resource pool can be for transmission of PSSCH, as described in Clause 8.1, or for reception of PSSCH, as described in Clause 8.3 and can be associated with either sidelink resource allocation mode 1 or sidelink resource allocation mode 2.

In the frequency domain, a sidelink resource pool consists of *numSubchannel* contiguous sub-channels. A sub-channel consists of *subchannelsize* contiguous PRBs, where *numSubchannel* and *subchannelsize* are higher layer parameters.

## 8.1 UE procedure for transmitting the physical sidelink shared channel

Each PSSCH transmission is associated with an PSCCH transmission.

That PSCCH transmission carries the 1st stage of the SCI associated with the PSSCH transmission; the 2nd stage of the associated SCI is carried within the resource of the PSSCH.

If the UE transmits SCI format 0-1 on PSCCH according to a PSCCH resource configuration in slot *n* and PSCCH resource *m*, then for the associated PSSCH transmission in the same slot

- one transport block is transmitted with up to two layers;

- The number of layers (ʋ) is determined according to the “Number of DMRS port” field in the SCI

- The set of consecutive symbols within the slot for transmission of the PSSCH is determined according to clause 8.1.2.1;

- The set of contiguous resource blocks for transmission of the PSSCH is determined according to clause 8.1.2.2;

Transform precoding is not supported for PSSCH transmission.

Only wideband precoding is supported for PSSCH transmission.

### 8.1.1 Transmission schemes

Only one transmission scheme is defined for the PSSCH and is used for all PSSCH transmissions.

PSSCH transmission is performed with up to two antenna ports, with antenna ports [1000-1001] as defined in clause [8.2.4] of [4, TS 38.211].

### 8.1.2 Resource allocation

In sidelink resource allocation mode 1:

- for PSSCH and PSCCH transmission, dynamic grant, configured grant type 1 and configured grant type 2 are supported.

#### 8.1.2.1 Resource allocation in time domain

The UE shall transmit the PSSCH in the same slot as the associated PSCCH.

The minimum resource allocation unit in the time domain is a slot.

The UE shall transmit the PSSCH in consecutive symbols within the slot, subject to the following restrictions:

- The UE shall not transmit PSSCH in symbols which are not configured for sidelink. A symbol is configured for sidelink, according to higher layer parameters *startSLsymbols* and *lengthSLsymbols*, where *startSLsymbols* is the symbol index of the first symbol of *lengthSLsymbols* consecutive symbols configured for sidelink.

- Within the slot, PSSCH resource allocation starts at symbol *startSLsymbols+1.*

- The UE shall not transmit PSSCH in symbols which are configured for use by PSFCH, if PSFCH is configured in this slot.

- The UE shall not transmit PSSCH in the last symbol configured for sidelink.

- The UE shall not transmit PSSCH in the symbol immediately preceding the symbols which are configured for use by PSFCH, if PSFCH is configured in this slot.

In sidelink resource allocation mode 1:

- For sidelink dynamic grant, the PSSCH transmission is scheduled by a DCI format 3\_0.

- For sidelink configured grant type 2, the configured grant is activated by a DCI format 3\_0.

- For sidelink dynamic grant and sidelink configured grant type 2:

- The "Time gap" field value *m* of the DCI format 3\_0 provides an index *m* + 1 into a slot offset table. That table is given by higher layer parameter *timeGapFirstSidelinkTransmission* and the table value at index *m* + 1 will be referred to as slot offset .

- The slot of the first sidelink transmission scheduled by the DCI is the first SL slot of the corresponding resource pool that starts not earlier than where is starting time of the downlink slot carrying the corresponding DCI, is the timing advance value and is the slot offset between the slot DCI and the first sidelink transmission scheduled by DCI, is as defined in 38.211, and t is the SL slot duration.

- For sidelink configured grant type 1:

- The slot of the first sidelink transmissions follows the higher layer configuration according to [10, TS 38.321].

#### 8.1.2.2 Resource allocation in frequency domain

The resource allocation unit in the frequency domain is the sub-channel.

The sub-channel assignment for sidelink transmission is determined using the “Frequency resource assignment” field in the associated SCI.

The lowest sub-channel for sidelink transmission is the sub-channel on which the lowest PRB of the associated PSCCH is transmitted.

If a PSSCH scheduled by a PSCCH would overlap with resources containing the PSCCH, the resources corresponding to a union of the PSCCH that scheduled the PSSCH and associated PSCCH DM-RS are not available for the PSSCH.

### 8.1.3 Modulation order, target code rate, redundancy version and transport block size determination

#### 8.1.3.1 Modulation order and target code rate determination

*IMCS* is given by the “Modulation and coding scheme” field in SCI format 0-1.

The MCS table is determined as follows: one out of Table 5.1.3.1-1, Table 5.1.3.1-2, Table 5.1.3.1-3 according to higher layer parameter *mcs-Table-SL* in resource pool configuration [ or field [TBD] in the SCI or higher layer indication].

The UE shall use *IMCS* and the MCS table determined according to the previous step to determine the modulation order (*Qm*) and Target code rate (*R*) used in the physical sidelink shared channel.

#### 8.1.3.2 Transport block size determination

The UE shall first determine the number of REs (*NRE*) within the slot.

### 8.1.4 UE procedure for determining the subset of resources to be reported to higher layers in PSSCH resource selection in sidelink resource allocation mode 2

In resource allocation mode 2, the higher layer can request the UE to determine a subset of resources from which the higher layer will select resources for PSSCH/PSCCH transmission. To trigger this procedure, in slot *n,* the higher layer provides the following parameters for this PSSCH/PSCCH transmission:

- the resource pool from which the resources are to be reported;

- L1 priority, ;

- the remaining packet delay budget;

- the number of sub-channels to be used for the PSSCH/PSCCH transmission in a slot, ;

- optionally, the resource reservation interval, , in units of ms.

The following higher layer parameters affect this procedure:

*- t2min\_SelectionWindow:* internal parameter is set to the corresponding value from higher layer parameter *t2min\_SelectionWindow* for the given value of .

*- SL-ThresRSRP\_pi\_pj*: this higher layer parameter provides an RSRP threshold for each combination , where is the value of the priority field in a received SCI format 0-1 and is the priority of the transmission of the UE selecting resources; for a given invocation of this procedure, .

*- RSforSensing* selects if the UE uses the PSSCH-RSRP or PSCCH-RSRP measurement, as defined in clause 8.4.2.1.

*- reservationPeriodAllowed*

*- t0\_SensingWindow*: internal parameter is defined as the number of slots corresponding to *t0\_SensingWindow* ms.

The resource reservation interval, , if provided, is converted from units of *ms* to units of logical slots, resulting in .

Notation:

denotes the set of slots which can belong to a sidelink resource pool and is defined in [TBD].

The following steps are used:

1) A candidate single-slot resource for transmission is defined as a set of contiguous sub-channels with sub-channel *x+j* in slot where . The UE shall assume that any set of contiguous sub-channels included in the corresponding resource pool within the time interval correspond to one candidate single-slot resource, where

- selection of is up to UE implementation under , where is TBD;

- if is shorter than the remaining packet delay budget (in slots) then is up to UE implementation subject to remaining packet budget (in slots); otherwise is set to the remaining packet delay budget (in slots).

The total number of candidate single-slot resources is denoted by .

2) The sensing window is defined by the range of slots [) where is defined above and is TBD. The UE shall monitor slots which can belong to a sidelink resource pool within the sensing window except for those in which its own transmissions occur. The UE shall perform the behaviour in the following steps based on PSCCH decoded and RSRP measured in these slots.

3) The internal parameter is set to the corresponding value from higher layer parameter *SL-ThresRSRP\_pi\_pj* for equal to the given value of and each priority value .

4) The set is initialized to the set of all the candidate single-slot resources.

5) The UE shall exclude any candidate single-slot resource from the set if it meets all the following conditions:

- the UE has not monitored slot in Step 2.

- for any periodicity value allowed by the higher layer parameter *reservationPeriodAllowed* and a hypothetical SCI format 0-1 received in slot with "Resource reservation period" field set to that periodicity value and indicating all subchannels of the resource pool in this slot, condition c in step 6 would be met.

6) The UE shall exclude any candidate single-slot resource from the set if it meets all the following conditions:

a) the UE receives an SCI format 0-1 in slot , and "Resource reservation period" field, if present, and "Priority" field in the received SCI format 0-1 indicate the values and , respectively according to Clause [TBD] in [6, TS 38.213];

b) the RSRP measurement performed, according to clause 8.4.2.1 for the received SCI format 0-1, is higher than ;

c) the SCI format received in slot or the same SCI format which, if and only if the "Resource reservation period" field is present in the received SCI format 0-1, is assumed to be received in slot(s) determines according to clause [TBD] in [6, TS 38.213] the set of resource blocks and slots which overlaps with for *q*=1, 2, …, *Q* and *j=*0, 1, …, . Here, is converted to units of logical slots, if and , where if slot n belongs to the set , otherwise slot is the first slot after slot n belonging to the set ; otherwise . is FFS.

7) If the number of candidate single-slot resources remaining in the set is smaller than , then is increased by 3 dB for each priority value and the procedure continues with step 4.

The UE shall report set to higher layers.

### 8.1.5 UE procedure for determining slots and resource blocks for PSSCH transmission associated with an SCI format 0-1

The set of slots and resource blocks for PSSCH transmission is determined by the resource used for the PSCCH transmission containing the associated SCI format 0-1, and fields "Frequency resource assignment", "Time resource assignment" of the associated SCI format 1 as described below.

[TBD]

## 8.2 UE procedure for transmitting sidelink reference signals

### 8.2.1 CSI-RS transmission procedure

A UE transmits sidelink CSI-RS within a unicast PSSCH transmission if the following conditions hold:

- CSI reporting is enabled by higher layer parameter [*CSIsiReporting*]; and

- the “CSI request” field in the corresponding SCI format 0-1 is set to 1.

The following parameters for CSI-RS transmission are configured via the higher layer parameter [TBD] for each CSI-RS configuration:

*- nrofPortsCSIRS-SL* indicates the number of ports for SL CSI-RS.

- firstSymbolInTimeDomainCSIRS-SL indicates the first OFDM symbol in a PRB used for SL CSI-RS

- frequDomainAllocationCSIRS-SL indicates the frequency domain allocation for SL CSI-RS.

### 8.2.2 PSSCH DM-RS transmission procedure

The UE selects the DM-RS time domain pattern out of the patterns configured using the higher layer parameter *TimePatternPsschDmrs* for the resource pool on which the PSSCH is to be transmitted. If more than one DM-RS time domain pattern is configured, the selected pattern is indicated by the “*DMRS pattern”* field in the SCI format 0-1 associated with the PSSCH transmission.

[ If PSSCH DMRS and PSCCH are mapped to the same OFDM symbol, then this mapping within a single sub-channel is only supported if higher layer parameter *subchannelsize* >= 20, i.e. the sub-channel size is at least 20 PRBs. ]

### 8.2.3 PT-RS transmission procedure

Transmission of PT-RS is only supported in FR2.

The UE PT-RS transmission procedure specified in section 6.2.3.1 applies for derivation of the PT-RS parameters *LPT-RS* and*, KPT-RS* and for determination of PT-RS presence, with the following changes:

- timeDensity and frequencyDensity in PTRS-UplinkConfig are replaced by timeDensity-SL and frequencyDensity-SL respectively;

- the number of antenna ports is the same as the number of DMRS antenna ports and the association between a PT-RS antenna port and a DMRS antenna port is fixed.

## 8.3 UE procedure for receiving the physical sidelink shared channel

For sidelink resource allocation mode 1, a UE upon detection of SCI format 0-1 on PSCCH can decode PSSCH according to the detected SCI format 0-2, and associated PSSCH resource configuration configured by higher layers.

For sidelink resource allocation mode 2, a UE upon detection of SCI format 0-1 on PSCCH can decode PSSCH according to the detected SCI format 0-2, and associated PSSCH resource configuration configured by higher layers.

## 8.4 UE procedure for receiving reference signals

### 8.4.1 CSI-RS reception procedure

The CSI-RS defined in Clause 8.4.1.5 of [4, TS 38.211] may be used for CSI computation.

### 8.4.2 DM-RS reception procedure for RSRP computation

8.4.2.1 RSRP for resource selection in sidelink resource allocation mode 2

In sidelink resource allocation mode 2, the UE measures RSRP for resource selection as follows:

- PSSCH-RSRP over the DM-RS resource elements for the PSCCH carrying the received SCI format 0-1 if higher layer parameter *RSforSensing* is set to “*PSSCH DM RS*”, and

- PSCCH-RSRP over the DM-RS resource elements for the PSSCH according to the received SCI format 0-1 if higher layer parameter *RSforSensing* is set to “*PSCCH DM RS*”.

### 8.4.3 PT-RS reception procedure

Reception of PT-RS is only supported in FR2.

The UE PT-RS reception procedure specified in section 5.1.6.3 applies for derivation of the PT-RS parameters *LPT-RS* and*KPT-RS* and for determination of PT-RS presence, with the following changes:

- *timeDensity* and f*requencyDensity* in *PTRS-DownlinkConfig* are replaced by *timeDensity-SL* and *frequencyDensity-SL* in [TBD] respectively, and [TBD] is (pre)configured per resource pool;

- the number of antenna ports is the same as the number of PSSCH DMRS antenna ports and the association between a PT-RS antenna port and a PSSCH DMRS antenna port is fixed.

## 8.5 UE procedure for reporting channel state information (CSI)

### 8.5.1 Channel state information framework

CSI consists of Channel Quality Indicator (CQI) and Rank Indicator (RI). The CQI and RI are always reported together.

#### 8.5.1.1 Reporting configurations

The UE shall calculate CSI parameters (if reported) assuming the following dependencies between CSI parameters (if reported)

- CQI shall be calculated conditioned on the reported RI

The CSI reporting can be aperiodic (using [10, TS 38.321]). Table 8.5.1.1-1 shows the supported combinations of CSI reporting configurations and CSI-RS configurations and how the CSI reporting is triggered for CSI-RS configuration. Aperiodic CSI-RS is configured and triggered/activated as described in Clause 8.5.1.2.

Table 8.5.1.1-1 Triggering/Activation of CSI reporting for the possible CSI-RS Configurations.

|  |  |
| --- | --- |
| **CSI-RS Configuration** | **Aperiodic CSI Reporting** |
| Aperiodic CSI-RS | Triggered by SCI. |

For CSI reporting, wideband CQI reporting is supported. A wideband CQI is reported [for each codeword] for the entire CSI reporting band.

#### 8.5.1.2 Triggering of CSI reports

An aperiodic CSI report is triggered by an SCI format 0-2 with the “CSI request” field set to 1.

### 8.5.2 Channel state information

#### 8.5.2.1 CSI reporting quantities

#### 8.5.2.1.1 Channel quality indicator (CQI)

The UE shall derive CQI as specified in section 5.2.2.1, with the following changes

- PDSCH replaced by PSSCH

- uplink slot replaced by sidelink slot

- downlink physical resource blocks replaced by sidelink physical resource blocks

- Transport Block Size determination according to Clause 8.1.3.2

- CSI reference resource according to TODO

- interference measurements are not supported

- sub-band differential CQI is not supported

#### 8.5.2.2 Reference signal (CSI-RS)

The UE can be configured with one CSI-RS pattern as indicated by the higher layer parameters TBD.

Parameters for which the UE shall assume non-zero transmission power for CSI-RS are configured according to clause 8.2.1.

#### 8.5.2.3 CSI reference resource definition

TBD

### 8.5.3 CSI reporting

CSI reporting is aperiodic and is described in [10, TS 38.321].

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Change history | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-05 | RAN1#89 | R1-1708892 | - | - | - | Draft skeleton | 0.0.0 |
| 2017-07 | AH\_1706 | R1-1712016 |  |  |  | Inclusion of agreements up to and including RAN1#AH2 | 0.0.1 |
| 2017-08 | AH\_1706 | R1-1714234 |  |  |  | Inclusion of agreements up to and including RAN1#AH2 | 0.0.2 |
| 2017-08 | RAN1#90 | R1-1714596 |  |  |  | Updated editor's version | 0.0.3 |
| 2017-08 | RAN1#90 | R1-1714626 |  |  |  | Updated editor's version | 0.0.4 |
| 2017-08 | RAN1#90 | R1-1715077 |  |  |  | Endorsed version by RAN1#90 | 0.1.0 |
| 2017-08 | RAN1#90 | R1-1715324 |  |  |  | Inclusion of agreements up to and including RAN1#90 | 0.1.1 |
| 2017-08 | RAN1#90 | R1-1715331 |  |  |  | Updated editor's version | 0.1.2 |
| 2017-09 | RAN#77 | RP-172001 |  |  |  | For information to plenary | 1.0.0 |
| 2017-09 | AH\_1709 | R1-1716930 |  |  |  | Inclusion of agreements up to and including RAN1#AH3 | 1.0.1 |
| 2017-10 | RAN1#90bis | R1-1718808 |  |  |  | Updated editor's version | 1.0.2 |
| 2017-10 | RAN1#90bis | R1-1718819 |  |  |  | Endorsed version by RAN1#90bis | 1.1.0 |
| 2017-10 | RAN1#90bis | R1-1719227 |  |  |  | Inclusion of agreements up to and including RAN1#90bis | 1.1.1 |
| 2017-11 | RAN1#90bis | R1-1720113 |  |  |  | Inclusion of agreements up to and including RAN1#90bis | 1.1.2 |
| 2017-11 | RAN1#90bis | R1-1720114 |  |  |  | Inclusion of agreements up to and including RAN1#90bis | 1.1.3 |
| 2017-11 | RAN1#90bis | R1-1721051 |  |  |  | Endorsed version | 1.2.0 |
| 2017-12 | RAN1#91 | R1-1721344 |  |  |  | Inclusion of agreements up to and including RAN1#91 | 1.3.0 |
| 2017-12 | RAN#78 | RP-172416 |  |  |  | Endorsed version for approval by plenary | 2.0.0 |
| 2017-12 | RAN#78 |  |  |  |  | Approved by plenary – Rel-15 spec under change control | 15.0.0 |
| 2018-03 | RAN#79 | RP-180200 | 0001 |  | F | CR capturing the Jan18 ad-hoc and RAN1#92 meeting agreements | 15.1.0 |
| 2018-06 | RAN#80 | RP-181172 | 0002 | 1 | F | CR to 38.214 capturing the RAN1#92bis and RAN1#93 meeting agreements | 15.2.0 |
| 2018-06 | RAN#80 | RP-181257 | 0003 | - | B | CR to 38.214 capturing the RAN1#92bis and RAN1#93 meeting agreements related to URLLC | 15.2.0 |
| 2018-06 | RAN#80 | RP-181172 | 0004 | - | F | CR to 38.214: maintenance according to agreed Rel 15 features | 15.2.0 |
| 2018-09 | RAN#81 | RP-181789 | 0005 | - | F | CR to 38.214 capturing the RAN1#94 meeting agreements | 15.3.0 |
| 2018-12 | RAN#82 | RP-182523 | 0006 | 2 | F | Combined CR of all essential corrections to 38.214 from RAN1#94bis and RAN1#95 | 15.4.0 |
| 2019-03 | RAN#83 | RP-190632 | 0007 | 3 | F | Correction to aperiodic CSI-RS triggering with different numerology between PDCCH and CSI-RS | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0009 | - | F | Correction on CSI-RS configuration in 38.214 | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0010 | - | F | Correction on uplink resource allocation type 1 | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0011 | - | F | Correction on determination of the resource allocation table for PUSCH with SP CSI | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0012 | - | F | Correction on PUSCH resource allocation | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0013 | - | F | Change Request for alignment of frequency domain resource allocation with 38.213 for a PUSCH transmission scheduled by a RAR UL grant | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0014 | - | F | CR on sequential PDSCH and PUSCH scheduling | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0015 | - | F | CR on out of HARQ order with multiple PDSCHs within one slot | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0016 | - | F | Correction to LBRM restriction | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0017 | - | F | CR on PDSCH beam indication | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0018 | - | F | Correction on TCI indication for multi-slot PDSCH | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0019 | - | F | Clarifications on CSI reporting on PUSCH | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0020 | - | F | QCL properties of Msg4 in CONNECTED Mode | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0022 | 1 | F | CR on dynamic grant overriding configured grant | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0023 | - | F | Correction on PUSCH with configured grant | 15.5.0 |
| 2019-03 | RAN#83 | RP-190450 | 0024 | - | F | Corrections to 38.214 | 15.5.0 |
| 2019-03 | RAN#83 | RP-190425 | 0025 | 1 | F | CR on QCL assumption for receiving PDSCH for RAR | 15.5.0 |
| 2019-06 | RAN#84 | RP-191552 | 0035 | - | F | Removal of "Correction to aperiodic CSI-RS triggering with different numerology between PDCCH and CSI-RS" | 15.6.0 |
| 2019-06 | RAN#84 | RP-191284 | 0026 | - | F | Corrections on non-codebook based UL transmission to TS 38.214 | 15.6.0 |
| 2019-06 | RAN#84 | RP-191284 | 0027 | - | F | CR on UE procedure for PDSCH and PUSCH | 15.6.0 |
| 2019-06 | RAN#84 | RP-191284 | 0028 | - | F | Correction on configured scheduling PUSCH repetition with dynamic SFI | 15.6.0 |
| 2019-06 | RAN#84 | RP-191284 | 0029 | - | F | CR on rate matching for PDSCH scheduled by DCI format 1\_0 | 15.6.0 |
| 2019-06 | RAN#84 | RP-191284 | 0030 | - | F | Clarification on CG transmission opportunities | 15.6.0 |
| 2019-06 | RAN#84 | RP-191284 | 0031 | 5 | F | Corrections to 38.214 including alignment of terminology across specifications | 15.6.0 |
| 2019-06 | RAN#84 | RP-191284 | 0032 | - | F | CR to 38.214 clarifying calculation of DataRate and DataRateCC | 15.6.0 |
| 2019-06 | RAN#84 | RP-191284 | 0033 | - | F | Correction on PUSCH retransmission for a serving cell configured with two uplinks | 15.6.0 |
| 2019-06 | RAN#84 | RP-191284 | 0034 | - | F | Corrections to 38.214 regarding the MAC CE activation/deactivation timing in mixed numerology scenario | 15.6.0 |
| 2019-09 | RAN#85 | RP-191943 | 0037 | - | F | Correction on UE receiving PDSCH procedure in FR2 | 15.7.0 |
| 2019-09 | RAN#85 | RP-191943 | 0038 | - | F | Correction on slot aggregation | 15.7.0 |
| 2019-09 | RAN#85 | RP-191943 | 0039 | - | F | CR on grant-based PDSCH overlapping with SPS PDSCH | 15.7.0 |
| 2019-09 | RAN#85 | RP-191943 | 0040 | - | F | Correction on the resource mapping of PDSCH in TS 38.214 | 15.7.0 |
| 2019-09 | RAN#85 | RP-191943 | 0041 | 1 | F | Corrections to 38.214 including alignment of terminology across specifications in RAN1#98 | 15.7.0 |
| 2019-09 | RAN#85 | RP-191943 | 0042 | - | F | Clarification of PUSCH with SP-CSI overlapping with PUSCH with data | 15.7.0 |
| 2019-12 | RAN#86 | RP-192627 | 0045 | - | F | Correction on resource allocation for uplink transmission with configured grant Type 1 | 15.8.0 |
| 2019-12 | RAN#86 | RP-192627 | 0046 | - | F | Clarification to the dynamically scheduled PDSCH collision with SPS-PDSCH | 15.8.0 |
| 2019-12 | RAN#86 | RP-192627 | 0047 | - | F | Correction on rate-matching for LTE-CRS-toMatchAround | 15.8.0 |
| 2019-12 | RAN#86 | RP-192627 | 0048 | - | F | Correction on timing for MAC CE applicability in 38.214 | 15.8.0 |
| 2019-12 | RAN#86 | RP-192627 | 0049 | - | F | Corrections to 38.214 including alignment of terminology across specifications in RAN1#98bis and RAN1#99 | 15.8.0 |
| 2019-12 | RAN#86 | RP-192634 | 0043 | 1 | B | Introduction of UE behaviour for SRS measurements for CLI | 16.0.0 |
| 2019-12 | RAN#86 | RP-192635 | 0050 | - | B | Introduction of two-step RACH | 16.0.0 |
| 2019-12 | RAN#86 | RP-192636 | 0051 | - | B | Introduction of NR - U | 16.0.0 |
| 2019-12 | RAN#86 | RP-192637 | 0052 | - | B | Introduction of integrated access and backhaul for NR | 16.0.0 |
| 2019-12 | RAN#86 | RP-192638 | 0053 | - | B | Introduction of NR V2X | 16.0.0 |
| 2019-12 | RAN#86 | RP-192639 | 0054 | - | B | Introduction of NR URLLC support | 16.0.0 |
| 2019-12 | RAN#86 | RP-192641 | 0055 | - | B | enhanced MIMO | 16.0.0 |
| 2019-12 | RAN#86 | RP-192642 | 0056 | - | B | Introduction of cross-slot scheduling restriction | 16.0.0 |
| 2019-12 | RAN#86 | RP-192643 | 0057 | - | B | Introduction of NR positioning support | 16.0.0 |
| 2019-12 | RAN#86 | RP-192645 | 0058 | - | B | Introduction of Cross-carrier Scheduling with Different Numerologies | 16.0.0 |
| 2019-12 | RAN#86 | RP-192646 | 0059 | - | B | Introduction of multiple LTE CRS rate matching patterns | 16.0.0 |
| 2019-12 | RAN#86 | RP-192646 | 0060 | - | B | Aperiodic CSI-RS Triggering for UE reporting beamSwitchTiming values of 224 and 336 | 16.0.0 |
| 2019-12 | RAN#86 | RP-192646 | 0061 | - | B | Behaviour for triggered with a CSI report for non-active BWP | 16.0.0 |
| 2019-12 | RAN#86 | RP-192646 | 0062 | - | B | Introduction of downgraded configurations for SRS antenna switching | 16.0.0 |
| 2019-12 | RAN#86 | RP-192646 | 0063 | - | B | Introduction of one-slot periodic TRS configuration for FR1 under a certain condition | 16.0.0 |
| 2019-12 | RAN#86 | RP-192640 | 0064 | - | B | Introduction of Industrial IoT | 16.0.0 |